IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB271 Remaining CIDs on TDLS | | | | |
| Date: July 12th, 2023 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Rubayet Shafin | Samsung Research America | 6625 Excellence Way., Plano, TX, 75023 |  | [r.shafin@samsung.com](mailto:r.shafin@samsung.com) |
| Boon Loong Ng |  |  |
| Peshal Nayak |  |  |
| Vishnu Ratnam |  |  |
| Yue Qi |  |  |
| Elliot Jen |  |  |

Abstract

This submission proposes resolutions for the following 1 comment received for TGbe LB271:

* 1 CID: 18233

SP: Do you agree to the resolutions provided in doc 11-23/1276r0 for the following CIDs for inclusion in the latest 11be draft?

18233

Revisions:

* Rev 0: Initial version.

***TGbe editor: Please note Baseline is 11be D3.2***

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. This introduction is not part of the adopted material.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Pg/Ln** | **Comment** | **Proposed Change** | **Resolution** |
| 18233 | Rubayet Shafin | 580.10 | In Clause 35.3.21.2 TDLS direct link over a single link, In Figure 35-39 line 10&15&22 (Example of TDLS discovery initiated by a STA to a non-AP MLD), Figure 35-40 line 12&19, Figure 35-41 line 37&43, the link identifier element (represented as LI in the figure) was simpliy illustrated as {LI(BSSID=AP1)}. However, in Figure 35-37 line 9&14&20, and Figure 35-38 line 39&45, the Link indentifier elements include the details containing BSSID, TDLS innitiator STA address, and TDLS responder address. This is better to be consistent with details. | Please considering complete the detailed addresses in link-identifier elements in Figure 35-39, Figure 35-40, and Figure 35-41 for better consistence and illustration. For example, replace "{LI(BSSID=AP1}" to "{LI(STA3, MLD\_S, AP1)}" in Figure 35-39 line 10&15&22. Replace "{LI(BSSID=AP1}" to "{LI(MLD\_R, MLD\_S, AP1)}" in Figure 35-40 line 10&15&22. Replace "{LI(BSSID=AP1}" to "{LI(MLD\_S, MLD\_R, AP1)}" in Figure 35-41 line 10&15&22. | **Revised.**  The LI issue in the figures was addressed in document 11-23/770r2 (see the resolution for CID 16989) and corresponding CIDs passed the SP. No further change is needed. |