IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IEEE P802.11be/D4.0 Mandatory Draft Review (MDR) Report | | | | |
| Date: 2023-11-26 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Robert Stacey | Intel |  |  | robert.stacey@intel.com |
| Emily Qi | Intel |  |  | emily.h.qi@intel.com |
| Edward Au | Huawei |  |  | edward.ks.au@gmail.com |
| Joe Levy | InterDigital |  |  | Joseph.Levy@interdigital.com |
| Rubayet Shafin | Samsung |  |  | r.shafin@samsung.com |
| Ming Gan | Huawei |  |  | ming.gan@huawei.com |
| Alfred Asterjadhi | Qualcomm Inc. |  |  | aasterja@qti.qualcomm.com |
| Atsushi Shirakawa | Sharp |  |  | shirakawa.atsushi@ieee.org |
| Carol Ansley | Cox |  |  | carol@ansley.com |
| Stephen McCann | Huawei |  |  | mccann.stephen@gmail.com |
| Claudio da Silva | Meta |  |  | claudiodasilva@meta.com |
| Graham Smith | SR Technologies |  |  | gsmith@wi-ficonsulting.org |
| Ross Jian Yu | Huawei |  |  | ross.yujian@huawei.com |
| Youhan Kim | Qualcomm Inc. |  |  | youhank@qti.qualcomm.com |
| Po-Kai Huang | Intel |  |  | po-kai.huang@intel.com |

**Abstract**

This document contains the report of the IEEE P802.11be D4.0 Mandatory Draft Review.

r0: section headings.

r1: added findings from Ming and Graham.

r2: added findings from Po-Kai.

r3: added findings from Carol.

r4: added findings from Atsushi and Stephen.

r5: added findings from Youhan.

r6: added findings from Emily.

r7: added findings from Claudio, Ross, Robert, and Alfred.

r8: added findings from Rubayet

r9: comments from review during Editors meeting on 2023-09-05 (track changes on).

r10: updates from editors meeting on 2023-09-12 (track changes on)

r11: reviewed selected reviews with TGbe: comments highlighted in blue mean that they can be accepted; comments highlighted in grey mean that they will not be implemented in the next 11be draft.

r12: reviewed selected reviews with TGbe: comments highlighted in blue mean that they can be accepted; comments highlighted in grey mean that they will not be implemented in the next 11be draft; added IEEE SA editorial team’s MEC result.

r13: added findings from Joe

r14: updates from November session editors meeting

r15: updates after the TGbe editor reviewed the review results.

# Introduction

## Purpose of this document

This document is the report from the group of volunteers that participated in the P802.11be/D4.0 mandatory draft review.

This document contains recommendations for changes to the P802.11be draft to bring it into improved compliance to IEEE-SA and WG11 style.

The recommended changes need to be reviewed by TGme and approved, or ownership of the issues taken by TGme.

## Process / references

The MDR process is described in:

* [11-11/615r6](https://mentor.ieee.org/802.11/dcn/11/11-11-0615-06-0000-wg802-11-mec-process.doc) – WG802.11 MEC Process

And references:

* [11-09/1034r20](https://mentor.ieee.org/802.11/dcn/09/11-09-1034-20-0000-802-11-editorial-style-guide.docx) – 802.11 Editorial Style Guide

A setup meeting will be held with and review topics assigned to volunteers. The review comments from the volunteers will be compiled into this document.

## Acknowledgements

The 802.11 technical editor (Robert Stacey) gratefully acknowledges the work and contribution of the members listed in the authors list. It takes a significant amount of effort to review a 1000 page draft.

# Findings

## Style

### Style Gude 2.1 – Frames

#### Style Guide 2.1.1 – Frame Format Figures

Emily Qi

[01] 136.11: change “MSI/Partial PPDU Parameters subfield when the Unsolicited MFB subfield is 1” to “MSI/Partial PPDU Parameters subfield format when the Unsolicited MFB subfield is 1”

[TGbe Editor: To implement in D5.0]

[02] 137.1: please align table 9-34 with the same table in REVme D4.0.

[TGbe Editor: To implement in a future draft to align the contents with the baseline]

[03] 147.25: “The STA Info List field contains one or more, n, STA Info fields.” Please add X- ref for the STA Info field.

[TGbe Editor: To implement in D5.0]

[04] 165.19: Bit number shall be starting with B0, not B25. Update references to bit fields, first column of Table 9-45h (NOT second column).

[TGbe Editor: To implement in D5.0]

[05] 168.58: Bit number shall be starting with B0, not B26. Check for references.

[TGbe Editor: To implement in D5.0 only in the figure. No update on other references required]

[06] 169.15: Bit number shall be starting with B0, not B26. Check for references.

[TGbe Editor: To implement in D5.0 only in the figure. No update on other references required]

[07] 171.6: table 9-45I doesn’t have a bottom border on page 171, 172, 173, and 174.

[TGbe Editor: To implement in D5.0]

[08] 178.8: Bit number shall be starting with B0, not B26. Check for references.

[TGbe Editor: To implement in D5.0 only in the figure. No update on other references required]

[09] 193.19: Figure 9-132 doesn’t have the Bit number row (the row starting with “Bits”).

[TGbe Editor: To implement in D5.0]

[10] 257.26, change the figure title to “Presence Bitmap field format of the Probe Request Multi-Link element ~~format~~”

[TGbe Editor: To implement in D5.0]

[11] 257.41: change the figure title to “Common Info field format of the Probe Request Multi- Link element ~~format~~”

[TGbe Editor: To implement in D5.0]

[12] 258.9: change the figure title to “Per-STA Profile subelement format of the Probe Request Multi-Link element ~~format~~”

[TGbe Editor: To implement in D5.0]

[13] 258.24: change the figure title to “STA Control field format of the Probe Request Multi- Link element ~~format~~”

[TGbe Editor: To implement in D5.0]

[14] 259.14: change the figure title to “Presence Bitmap subfield format of the Reconfiguration Multi-Link element ~~format~~”

[TGbe Editor: To implement in D5.0]

[15] 259.41: change the figure title to “Common Info field format of the Reconfiguration Multi- Link element ~~format~~”

[TGbe Editor: To implement in D5.0]

[16] 260.10: change the figure title to “Per-STA Profile subelement format for the Reconfiguration Multi-Link element ~~format~~”

[TGbe Editor: To implement in D5.0]

[17] 270.1: table 9-404n doesn’t have a bottom border on page 270 to 278.

[TGbe Editor: To implement in D5.0]

[Action: as suggested for all]

#### Style Guide 2.1.2 – Naming Frames

Joe Levy

1. 57.36 – “initial Control frame” refers to a type of frame not a specific frame name. Change “initial Control frame” to “initial control frame”, two locations (also 57.38).

[TGbe Editor: To implement in D5.0]

2. 76.45 “Beacon” to “Beacon frame”

[TGbe Editor: To implement in D5.0]

3. 186.36 “TWT request frame” does not apear in the base standard, what is it? – is the intent to send a “TWT Setup frame”, if so then replace “another TWT requrest frame” with “a TWT Setup frame”, also “can” should be “may”. Same change at 188.36.

[Edward to verify this change]

[TGbe Editor: Not implement. Encourage the reviewer to submit a comment in the initial SA ballot]

4. 239.13 “Beacon” to “Beacon frame”

[TGbe Editor: To implement in D5.0]

5. 303.13: “the RTS” to “an RTS frame”

[TGbe Editor: To implement in D5.0. Note that the correct page number is 330.]

6. 303.15 “the RTS” to “an RTS frame”

[TGbe Editor: To implement in D5.0. Note that the correct page number is 330.]

7. 340.12 “an RTS” to “an RTS frame”

[TGbe Editor: To implement in D5.0]

8. 334.16 “QoS Data” to “QoS Data frame”

[TGbe Editor: To implement in D5.0]

9. 335.41 “Data” to “Data frames”

[TGbe Editor: To implement in D5.0]

10. 235.46 Noun is missing – “The Broadcast TWT Recommendation is” to “The Broadcast TWT Recommendation field is”. Note this is base line text and should probably be corrected in TGme, the added 802.11be text, that follows correctly includes the noun.

[Edward to fix in REVme]

11. 336.16 “QoS Data” to QoS Data frames”

[TGbe Editor: To implement in D5.0]

12. 363.52 “Action” to “Action frame”

[TGbe Editor: To implement in D5.0]

13. 363.56 "Action” to “Action frame”

[TGbe Editor: To implement in D5.0]

14. 391.14 “Public Action” to “Public Action frame”

[TGbe Editor: To implement in D5.0]

15. 391.43 “Public Action” to “Public Action frame”

[TGbe Editor: To implement in D5.0]

16. 396.51 “Managenent Frame Subtype” to “Management frame subtype”

[Edward to fix in REVme]

17. 479.28 captitization of frame names not correct – change 36.5.2.2.3 clause title to: “Padding for a Trigger frames” – note this is a REVme change – see also [19] below – these should align.

[TGbe Editor: Not implement. Encourage the reviewer to submit a comment in the initial SA ballot]

18. 480.64 “an RTS” to “an RTS frame”

[TGbe Editor: To implement in D5.0]

19. 486.8,18 in Figure 35-2 there are two locations where “Frame” is capitalized should be “frame”

[TGbe Editor: To implement in D5.0]

20. 495.16 “Management subtype” to "Management frame subtype”

[TGbe Editor: To implement in D5.0]

21. 510.22 Frame capitization is not correct: change, also exchange is puluarized: “35.3.5.4 Basic Multi-Link element usage in the context of ML (re)setup, authentication, and FT action frame exchange between two MLDs” to “35.3.5.4 Basic Multi-Link element usage in the context of ML (Re)Setup, Authentication, and FT Action frame exchanges between two MLDs”

[TGbe Editor: To implement in D5.0]

22. 517.20 “Beacon” to “Beacon frame”

[TGbe Editor: To implement in D5.0]

23. 518.16 “Beacon” to “Beacon frame”

[TGbe Editor: To implement in D5.0]

24. 525.32 “Beacons” to “Beacon frames”

[TGbe Editor: To implement in D5.0]

25. 526.42 “Beacons” to “Beacon frames”

[TGbe Editor: The identified location is removed in D5.0 via comment resolution]

26. 558.50 “SRS Control” to “SRS Control frame”

[TGbe Editor: To implement in D5.0]

27. 566.59 this phrase should be corrected: “and the minimum MAC padding duration of the Padding field” to be either: 1) ”and the minimum MAC frame padding duration of the Padding field” or 2) "and the minimum MAC padding duration of the Padding field”

[Edward to identify appropriate change]

[TGbe Editor: To implement 1) in D5.0]

28. 568.12 this phrase should be corrected: “to ensure that the MAC padding duration of the initial Control frame” to be either: 1) “to ensure that the MAC frame padding duration of the initial Control frame” or 2) "to ensure that the MAC padding duration of the initial Control frame”

[TGbe Editor: To implement 1) in D5.0]

29. 585.57 captitization of frame names not correct – change 35.5.2.2.3 clause title to: “Padding for a Trigger frames”

[TGbe Editor: To implement in D5.0 as “Padding for a Trigger frame”]

30. 649.49 “SCS Request” to “SCS Request frame”

[TGbe Editor: To implement in D5.0]

31. 821.53 “MU-RTS” to “MU-RTS Trigger frame”

[TGbe Editor: To implement in D5.0]

32. 1027.20 – the “Control frame” is the type of frame the BSRP Trigger frame is, hence it should not be capitalized. Change “Control frame” to “control frame”.

[TGbe Editor: To implement in D5.0]

33. 1027.48 - the “Control frame” is the type of frame the MU-RTS Trigger is, hence it should not be capitalized. Change “Control frame” to “control frame”.

[TGbe Editor: To implement in D5.0]

34. 1028.20 - the “Control frame” is the type of frame the MU-RTS Trigger frame is, hence it should not be capitalized. Change “Control frame” to “control frame”.

[TGbe Editor: To implement in D5.0]

35. 1028.42 - the “Control frame” is the type of frame the BSRP Trigger frame is, hence it should not be capitalized. Change “Control frame” to “control frame”.

[TGbe Editor: To implement in D5.0]

36. 1028.42 - the “Control frame” is the type of frame the BSRP Trigger frame is, hence it should not be capitalized. Change “Control frame” to “control frame”.

[TGbe Editor: No change as this item is a duplicate of item 35]

Not frame related but noticed durring frame review:

37. 355.61 “PHY Data Rate” to “PHY data rate” – this is not a frame and should not be capitalized.

[TGbe Editor: To implement in D5.0]

38. 410.60 Capitization is wrong and an article is missing. change “STA MAC Address Identified By A2 subfield” to “STA MAC address identified by the A2 subfield” Also, note there does not seems to be an A2 subfield, only a UL HE-SIG-A2 Reserved subfield and EDMG-Header-A2 subfield.

[TGbe Editor: To implement the first change in D5.0. Regarding the second change on A2 subfield, not implement. Encourage the reviewer to submit a comment in the initial SA ballot]

39. 449.19 missing noun – “The MAC of the FTO” should be “The MAC entity of the FTO”, note this is also stated in this manner in the base line, and should be corrected in TGme. (Also “entity” should follow MAC at 449.21, 455.4, 455.6, 464.20, 464.28, 464.29, 464.47, 468.11, 468.12, 567.19, 567.27, 569.63, 570.6, 827.16, 891.7,

[Edward to fix as appropriate]

[TGbe Editor: Not implement. Encourage the reviewer to submit a comment in the initial SA ballot]

### Style Guide 2.2 – true/false

Rubayet Shafin

No issues were found.

### Style Guide 2.3 – “is set to” ###

Rubayet Shafin

In the description of the control fields, for example, the EHT MIMO Control field, the values are currently set using “is set”. Based on the current style guideline, these should be "equal to”. However, in similar contexts in the baseline, e.g. the HE MIMO Control field, “set to” is used extensively (which, to me as well, seemed appropriate).

When used for explaining a causation/rationale for setting a value in a particular way, the usage of “set to” seems appropriate. For example, “The xxx is set to 1 to indicate that…”. However, based on the current style guide, this usage of “set to” seems to be disallowed. These instances are marked as “ “set to” seems to be appropriate here.” in the below list.

[Robert: I think “is set to X to indicate” is OK since it is from the perspective of the sender; it is not a test at the receiver.]

Note:

1. In the below list, “xx.yy” refers to Page xx, Line yy
2. When there is a chance for confusion regarding the recommended changes due to multiple instance of “set to”/ “equal to” in the same sentence, additional notes have been made. For example regarding the input “237.54: Replace “set to” with “equal to”. “equal to 3” refers to the recommended change from “set to 3” to “equal to 3”, where the corresponding current spec text is the following. Other instances of “set to” in the same sentence will remain unchanged.

“The Broadcast TWT ID subfield in a Restricted TWT Parameter Set field is always set to a nonzero value, and is set to 31 when the Restricted TWT Schedule Info subfield is set to 3”

[Group consensus: Even though this is all at the sender side, use “equal to” because we have significant precedent for this.]

1. 55.31: Replace “set to” with “equal to”

2. 123.28: Replace “set to” with “equal to”

3. 123.29: Replace “set to” with “equal to”

4. 126.37: Replace “set to” with “equal to”

5. 126.38: Replace the three instances of “set to” with “equal to”

6. 126.61: “set to” seems to be appropriate here.

7. 126.62: “set to” seems to be appropriate here.

8. 127.14: “set to” seems to be appropriate here.

9. 127.15: “set to” seems to be appropriate here.

10. 130.56: Replace “set to” with “equal to”

11. 133.6: Replace “set to” with “equal to”

12. 133.7: Replace “set to” with “equal to”

13. 133.10: Replace “set to” with “equal to”

14. 133.11: Replace “set to” with “equal to”

15. 142.49: Replace “set to” with “equal to”

16. 142.50: Replace “set to” with “equal to”

17. 148.64: “set to” seems to be appropriate here.

18. 149.9: Replace “set to” with “equal to”

19. 151.1: Replace “set to” with “equal to”

20. 151.24: Replace “set to” with “equal to”

21. 151.51: “set to” seems to be appropriate here.

22. 152.13: “set to” seems to be appropriate here.

23. 152.56: “set to” seems to be appropriate here.

24. 152.61: “set to” seems to be appropriate here.

25. 152.64: “set to” seems to be appropriate here.

26. 153.4: Replace “set to” with “equal to”

27. 153.7: Replace “set to” with “equal to”

28. 153.13: Replace “set to” with “equal to”

29. 153.16: Replace “set to” with “equal to”

30. 153.23: “set to” seems to be appropriate here.

31. 153.23: Replace “set to” with “equal to”

32. 153.27: Replace “set to” with “equal to”

33. 153.30: Replace “set to” with “equal to”

34. 153.32: Replace “set to” with “equal to”

35. 154.56: Replace “set to” with “equal to”

36. 156.16: Replace “set to” with “equal to”

37. 156.17: Replace “set to” with “equal to”

38. 156.19: Replace “set to” with “equal to”

39. 159.45: “set to” seems to be appropriate here.

40. 159.48: “set to” seems to be appropriate here.

41. 161.2: Replace “set to” with “equal to”

42. 161.18: Replace “set to” with “equal to”

43. 161.52: “set to” seems to be appropriate here.

44. 161.54: Replace “set to” with “equal to”

45. 161.58: Replace “set to” with “equal to”

46. 161.59: Replace “set to” with “equal to”

47. 162.31: Replace “set to” with “equal to”

48. 163.11: “set to” seems to be appropriate here.

49. 163.23: “set to” seems to be appropriate here.

50. 163.25: “set to” seems to be appropriate here.

51. 163.28: Replace “set to” with “equal to”

52. 164.19: Replace “set to” with “equal to”

53. 165.12: Replace “set to” with “equal to”

54. 166.49: Replace “set to” with “equal to”

55. 167.1: “set to” seems to be appropriate here.

56. 167.2: “set to” seems to be appropriate here.

57. 168.16: “set to” seems to be appropriate here.

58. 168.17: “set to” seems to be appropriate here.

59. 168.34: “set to” seems to be appropriate here.

60. 168.42: “set to” seems to be appropriate here.

61. 168.44: “set to” seems to be appropriate here.

62. 168.45: Replace “set to” with “equal to”

63. 169.35: “set to” seems to be appropriate here.

64. 169.40: Replace “set to” with “equal to”

65. 175.46: Replace “set to” with “equal to”

66. 175.47: Replace “set to” with “equal to”

67. 175.48: Replace “set to” with “equal to”

68. 175.50: Replace “set to” with “equal to”

69. 175.51: Replace “set to” with “equal to”

70. 175.52: Replace “set to” with “equal to”

71. 175.53: Replace “set to” with “equal to”

72. 177.56: “set to” seems to be appropriate here.

73. 177.24: Replace “set to” with “equal to”

74. 177.34: “set to” seems to be appropriate here.

75. 177.36: “set to” seems to be appropriate here.

76. 179.9: Replace “set to” with “equal to”

77. 180.24: Replace “set to” with “equal to”

78. 181.37: “set to” seems to be appropriate here.

79. 186.27: Replace “set to” with “equal to”

80. 188.28: Replace “set to” with “equal to”

81. 194.25: Replace “set to” with “equal to”

82. 201.11: Replace “set to” with “equal to”

83. 201.20: Replace “set to” with “equal to”  “equal to 4”

84. 201.35: Replace “set to” with “equal to”

85. 201.36: Replace “set to” with “equal to”

86. 201.63: Replace “set to” with “equal to”

87. 201.64: Replace “set to” with “equal to”

88. 202.1: Replace “set to” with “equal to”

89. 204.48: Replace “set to” with “equal to”

90. 204.51: Replace “set to” with “equal to”

91. 208.48: Replace “set to” with “equal to”

92. 208.51: Replace “set to” with “equal to”

93. 208.62: Replace “set to” with “equal to”

94. 209.2: “set to” seems to be appropriate here.

95. 209.4: “set to” seems to be appropriate here.

96. 209.10: “set to” seems to be appropriate here.

97. 209.11: “set to” seems to be appropriate here.

98. 209.27: “set to” seems to be appropriate here.

99. 222.52: “set to” seems to be appropriate here.

100. 222.61: Replace “set to” with “equal to”

101. 224.16: Replace “set to” with “equal to”

102. 226.15: Replace “set to” with “equal to”

103. 230.21: Replace “set to” with “equal to”

104. 230.25: Replace “set to” with “equal to”

105. 230.38: Replace “set to” with “equal to”

106. 230.44: Replace “set to” with “equal to”

107. 230.50: Replace “set to” with “equal to”

108. 231.2: Replace “set to” with “equal to”

109. 232.51: Replace “set to” with “equal to”

110. 232.57: Replace “set to” with “equal to”

111. 233.11: Replace “set to” with “equal to”. “equal to 0”

112. 233.17: Replace “set to” with “equal to”. “equal to 1”

113. 235.6: Replace “set to” with “equal to”

114. 235.10: Replace “set to” with “equal to”

115. 236.46: Replace “set to” with “equal to”

116. 237.8: Replace “set to” with “equal to”

117. 237.54: Replace “set to” with “equal to”. “equal to 3”

118. 238.10: Replace “set to” with “equal to”

119. 238.13: Replace “set to” with “equal to”

120. 238.37: “set to” seems to be appropriate here.

121. 238.38: Replace “set to” with “equal to”

122. 238.43: Replace “set to” with “equal to”

123. 238.44: Replace “set to” with “equal to”

124. 241.11: “set to” seems to be appropriate here.

125. 241.12: “set to” seems to be appropriate here.

126. 241.28: For “Otherwise”, the usage of the “set to” seems to be correct since this is essentially a continuation of the previous sentence.

127. 245.28: For “Otherwise”, the usage of the “set to” seems to be correct since this is essentially a continuation of the previous sentence.

128. 249.33: Replace “set to” with “equal to”. “equal to 1”

129. 249.34: Replace “set to” with “equal to”. “equal to 1”

130. 258.36: Replace “set to” with “equal to”

131. 258.47: Replace “set to” with “equal to”

132. 262.31: Replace “set to” with “equal to”

133. 262.43: Replace “set to” with “equal to”

134. 262.46: Replace “set to” with “equal to”

135. 286.17: “set to” seems to be appropriate here.

136. 286.52: Replace “set to” with “equal to”

137. 287.55: Replace “set to” with “equal to”

138. 288.65: Replace “set to” with “equal to”

139. 289.27: Replace “set to” with “equal to”

140. 289.32: Replace “set to” with “equal to”

141. 291.43: Replace “set to” with “equal to”

142. 293.19: Replace “set to” with “equal to”

143. 293.23: Replace “set to” with “equal to”

144. 293.28: Replace “set to” with “equal to”

145. 293.34: Replace “set to” with “equal to”

146. 293.38: Replace “set to” with “equal to”

147. 293.43: Replace “set to” with “equal to”

148. 293.56: Replace “set to” with “equal to”

149. 293.58: Replace “set to” with “equal to”

150. 294.5: Replace “set to” with “equal to”

151. 294.8: Replace “set to” with “equal to”

152. 295.46: Replace “set to” with “equal to”

153. 307.56: Replace “set to” with “equal to”

154. 307.60: Replace “set to” with “equal to”

155. 308.15: Replace “set to” with “equal to”

156. 315.59: Replace “set to” with “equal to”

157. 339.60: Replace “set to” with “equal to”

158. 362.18: Replace “set to” with “equal to”

159. 380.31: Replace “set to” with “equal to”

160. 397.49: Replace “set to” with “equal to”

161. 398.12: Replace “set to” with “equal to”

162. 424.45: Replace “set to” with “equal to”

163. 443.22: Replace “set to” with “equal to”

164. 457.1: Replace “set to” with “equal to”

165. 457.59: Replace “set to” with “equal to”

166. 461.55: Replace “set to” with “equal to”

167. 463.28: Replace “set to” with “equal to”

168. 468.31: Replace “set to” with “equal to”

169. 471.53: Replace “set to” with “equal to”

170. 495.4: Replace “set to” with “equal to”

171. 500.2: Replace “set to” with “equal to”

172. 502.9: Replace “set to” with “equal to”

173. 512.27: Replace “set to” with “equal to”

174. 512.53: Replace “set to” with “equal to”

175. 515.58: Replace “set to” with “equal to”

176. 518.25: Replace “set to” with “equal to”

177. 523.2: Replace “set to” with “equal to”

178. 523.46: Replace “set to” with “equal to”

179. 523.53: Replace “set to” with “equal to”

180. 524.57: Replace “set to” with “equal to”

181. 527.15: Replace “set to” with “equal to”

182. 527.26: Replace “set to” with “equal to”

183. 527.40: Replace “set to” with “equal to”

184. 529.1: Replace “set to” with “equal to”

185. 530.44: Replace “set to” with “equal to”

186. 530.58: Replace “set to” with “equal to”

187. 531.18: Replace “set to” with “equal to”

188. 536.49: Replace “set to” with “equal to”

189. 542.21: Replace “set to” with “equal to”

190. 542.63: Replace “set to” with “equal to”

191. 547.3: Replace “set to” with “equal to”

192. 547.14: Replace “set to” with “equal to”

193. 551.51: Replace “set to” with “equal to”

194. 557.49: Replace “set to” with “equal to”

195. 561.6: Replace “set to” with “equal to”

196. 565.8: Replace “set to” with “equal to”

197. 565.55: Replace “set to” with “equal to”

198. 566.47: Replace “set to” with “equal to”

199. 578.45: Replace “set to” with “equal to”

200. 579.7: Replace “set to” with “equal to”

201. 579.42: Replace “set to” with “equal to”

202. 580.36: Replace “set to” with “equal to”

203. 587.14: Replace “set to” with “equal to”

204. 588.12: Replace “set to” with “equal to”

205. 588.13: Replace “set to” with “equal to”

206. 588.24: Replace “set to” with “equal to”

207. 605.42: Replace “set to” with “equal to”

208. 605.45: Replace “set to” with “equal to”

209. 605.48: Replace “set to” with “equal to”

210. 605.51: Replace “set to” with “equal to”

211. 609.59: Replace “set to” with “equal to”

212. 612.63: Replace “set to” with “equal to”

213. 613.28: Replace “set to” with “equal to”

214. 614.36: Replace “set to” with “equal to”

215. 614.40: Replace “set to” with “equal to”

216. 620.2: Replace “set to” with “equal to”

217. 620.4: Replace “set to” with “equal to”

218. 626.2: Replace “set to” with “equal to”

219. 626.3: Replace “set to” with “equal to”

220. 626.9: Replace “set to” with “equal to”

221. 627.12: Replace “set to” with “equal to”

222. 627.14: Replace “set to” with “equal to”

223. 627.20: Replace “set to” with “equal to”

224. 630.56: Replace “set to” with “equal to”

225. 657.47: Replace “set to” with “equal to”

226. 658.43: Replace “set to” with “equal to”

227. 762.27: Replace “set to” with “equal to”

228. 762.29: Replace “set to” with “equal to”. “equal to 0”

229. 762.30: Replace “set to” with “equal to”

230. 762.31: Replace “set to” with “equal to”. “equal to 1 or 2”

231. 762.33: Replace “set to” with “equal to”

232. 785.3: Replace “set to” with “equal to”

233. 785.5: Replace “set to” with “equal to”

234. 785.8: Replace “set to” with “equal to”

235. 791.18: Replace “set to” with “equal to”

236. 791.19: Replace “set to” with “equal to”

237. 791.29: Replace “set to” with “equal to”

238. 792.37: Replace “set to” with “equal to”

239. 792.38: Replace “set to” with “equal to”

240. 792.40: Replace “set to” with “equal to”

241. 896.48: Replace “set to” with “equal to”

242. 896.57: Replace “set to” with “equal to”

243. 896.62: Replace “set to” with “equal to”

244. 897.1: Replace “set to” with “equal to”

245. 897.7: Replace “set to” with “equal to”

246. 973.26: Replace “set to” with “equal to”

247. 973.39: Replace “set to” with “equal to”

248. 999.46: Replace “set to” with “equal to”

249. 999.50: Replace “set to” with “equal to”

250. 1000.2: Replace “set to” with “equal to”

251. 1009.33: Replace “set to” with “equal to”

252. 1010.2: Replace “set to” with “equal to”

253. 1016.29: Replace “set to” with “equal to”

254. 1025.40: Replace “set to” with “equal to”

[Group Consensus: Do not make these changes. Perhaps discuss further]

### Style Guide 2.4 – Information Elements/Subelements

#### Style Guide 2.4.1 – Information Elements/subelements – Naming

Ming Gan

“MLO Link Information element”, is this name aligned with that “<Purpose> does not include the word “information””?

For editorial style guide provided by Robert, the following sentence is confusing. Is that saying that <Purpose> is not exact same as “Information”, or it can’t contain “Information”. Generally speaking, element already includes the meaning of “information”. On the other hand, REVme D3. 0 still has a few instances where <Purpose> contains “information”.

Elements should be called the “<Purpose> element”, where <Purpose> does not include the word “information” (e.g., the “QoS Capability element”)

[01] Page 14, line 30: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: It is a cross reference. The text will be updated accordingly once the title of the subclause 9.4.2.317 is updated. No action here]

[02] Page 33, line 21: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: It is a cross reference. The text will be updated accordingly once the caption the figure 9-1001ax is updated. No action here]

[03] Page 192, line 37: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info element”]

[04] Page 212, line 38: Please replace “MLO Link Information” with “MLO Cross Link”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info”]

[05] Page 212, line 39: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: It is a cross reference. The text will be updated accordingly once the title of the subclause 9.4.2.317 is updated. No action here]

[06] Page 295, line 48: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info element”]

[07] Page 295, line 51: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info element”]

[08] Page 296, line 1: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info element”]

[09] Page 296, line 10: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info element”]

[10] Page 544, line 11: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info element”]

[11] Page 551 line 35: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info element”]

[12] Page 551, line 38: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info element”]

[13] Page 551, line 44: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info element”]

[14] Page 551, line 48: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info element”]

[15] Page 551, line 51: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info element”]

[16] Page 551, line 54: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info element”]

[17] Page 551, line 58: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info element”]

[18] Page 551, line 59: Please replace “MLO Link Information element” with “MLO Cross Link element”.

[TGbe Editor: To implement in D5.0 as “MLO Link Info element”]

[Robert: Agree – avoid use of “information” in element name since might be confused as part of the noun (information element). As an alternative, you can use “MLO Link Info element”, i.e. use the shortened “Info” instead of “Information”; we have precedent for this.]

[Action: change to “MLO Link Info element”]

#### Style Guide 2.4.2 – Definition Conventions

Ming Gan

No findings

#### Style Guide 2.4.3 – Element Inclusion Conventions

Ming Gan

No findings

### Style Guide 2.5 – Removal of functions and features

Not applicable

### Style Guide 2.6 – Capitalization

Alfred Asterjadhi/Edward Au

No issues were found.

### Style Guide 2.7 – Terminology: frame vs packet vs PPDU vs MPDU

Atsushi Shirakawa

[01] Page 660, line 14: Replace “frame transmission or reception” with “PPDU transmission or reception.”. Similar correction was adopted in P802.11-REVme D4.0, Page 4005, line 61, denoted as #1065.

[TGbe Editor: To implement in D5.0]

[02] Page 825, line 13: Replace “encoded packet duration” with “encoded duration”. Similar correction was adopted in P802.11-REVme D4.0, Page 4142, line 23, denoted as #1065.

[Action: fix through comment resolution]

[TGbe Editor: Not implement. Encourage the reviewer to submit a comment in the initial SA ballot]

[03] Page 879, line 47: Replace “frame” with “PPDU”. Similar correction was adopted in P802.11-REVme D4.0, Page 4182, line 22, denoted as #1065

[TGbe Editor: To implement in D5.0]

[04] Page 879, line 53: Replace “frame” with “PPDU”. Similar correction was adopted in P802.11-REVme D4.0, Page 4182, line 26, denoted as #1065

[TGbe Editor: To implement in D5.0]

[05] Page 879, line 57: Replace “frame” with “PPDU”. Similar correction was adopted in P802.11-REVme D4.0, Page 4182, line 29, denoted as #1065

[TGbe Editor: To implement in D5.0]

[06] Page 880, line 41: Replace “frame” with “PPDU”. Similar correction was adopted in P802.11-REVme D4.0, Page 4172, line 22, denoted as #1065

[TGbe Editor: To implement in D5.0]

[07] Page 880, line 62: Replace “frames” with “PPDUs”. Similar correction was adopted in P802.11-REVme D4.0, Page 4172, line 39, denoted as #1065

[TGbe Editor: To implement in D5.0]

[Robert: Agree with all suggestions except 02]

### Style Guide 2.8 – Use of verbs & problematic words

#### normative, non-normative, ensure

Carol Ansley

Normative language in NOTEs

[01] 77.30 - In implementations, the DA address filtering function ~~may~~ can be done “lower in the stack.”

[Robert: Use “might”]

[TGbe Editor: To implement in D5.0 following Robert’s suggestion]

[02] 495.63 – should be note 3, not note 4

[TGbe Editor: To implement in D5.0]

[03] 525.61 – missing space “TTLMthat”

[TGbe Editor: Agree. This comment is addressed by CID 19106]

[04] 571.56 – within NOTE 2: An NSTR mobile AP MLD that intends to swap the operating channel used for its primary and nonprimary links respectively must simultaneously perform the (extended) channel switch operation on both links. (should this be removed from the NOTE or wording changed?)

[Robert: Should change to “will” since the informative note is describing something that will happen based on the normative rules stated elsewhere.]

[TGbe Editor: To implement in D5.0 following Robert’s suggestion]

[05] 733.59 - NOTE 3—U-SIG field content ~~may~~ can vary between 80 MHz frequency subblocks

[Robert: Use “might”]

[TGbe Editor: To implement in D5.0 following Robert’s suggestion]

[06] 885.14 - NOTE—Additional test requirements and/or test methods ~~may~~ might be needed to meet regulatory requirements.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[Action: as suggested. Edward to discuss “must” change with group]

#### Style Guide 2.8.1 – which/that

Carol Ansley

[01] 56.25 - such as a non-AP STA (excluding the 20 MHz-only non-AP EHT STA) ~~which~~ that is not capable of 160 MHz operation

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[02] 56.32 - such as a non-AP STA (excluding the 20 MHz-only non-AP EHT STA) ~~which~~ that is not capable of 320 MHz operation

[Robert: agree]

[TGbe Editor: To implement in D5.0][03] 59.60 - In a 320 MHz basic service set (BSS), the 160 MHz channel not including the primary 20 MHz channel, which together with the primary 160 MHz channel, forms the 320 MHz channel of the 320 MHz extremely high throughput (EHT) BSS.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[04] 66.14 - with which BSS the GLK non-AP STA is a member ~~of~~.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[05] 76.63 - for describing the MAC sublayer ~~for~~ in which the actual implementation of each function should reside

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[06] 116.40 - When generated by an AP MLD, this primitive updates the DS’s non-AP MLD-to- AP MLD map~~,~~ ~~which~~ that controls to which AP MLD the DS delivers MAC service tuples that are destined for a given non-AP MLD.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[07] 134.22 - the RU or MRU to which the recommended EHT-MCS applies ~~to~~

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[08] 134.34 - the RU or MRU to which the recommended EHT-MCS applies ~~to~~

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[09] 135.8 - the bandwidth to which the recommended EHT-MCS applies ~~to~~

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[10] 135.14 - the bandwidth to which the recommended EHT-MCS applies ~~to~~

[Robert: agree]

[TGbe Editor: This sentence was removed via comment resolution]

[11] 156.5 - There are three variants for the User Info field:~~, which are~~ Special User Info field (see 9.3.1.22.3 (Special User Info field), HE variant User Info field (see 9.3.1.22.4 (HE variant User Info field)), and EHT variant User Info field (see 9.3.1.22.5 (EHT variant User Info field)).

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[12] 193.12 - Frames other than a Beacon frame or a Probe Response frame transmitted by an AP affiliated with an AP MLD ~~which~~ that corresponds to a transmitted BSSID in a multiple BSSID set

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[13] 225.4 - The MLO GTK subelement contains the GTK for a link, which is encrypted (see procedures in 13.8.5 (FT authentication sequence: contents of fourth message)) [unclear what is meant here]

[Robert: disagree – existing seems appropriate]

[TGbe Editor: Not implemented]

[14] 238.1 – 10 - The Aligned TWT Link Bitmap subfield indicates the link(s) ~~which~~ that has the aligned TWT SPs with the link indicated by the Link ID Bitmap Subfield in the TWT element. A value of 1 in bit position i of the Aligned TWT Link Bitmap subfield means that the link associated with the link ID i is the link ~~which~~ that has the aligned TWT SPs with the link indicated by the Link ID Bitmap Subfield. A value of 0 in bit position i of the Aligned TWT Link Bitmap subfield means that the link associated with the link ID i is the link ~~which~~ that does not have the aligned TWT SPs with the link indicated by the Link ID Bitmap Subfield. The bit in the Aligned TWT Link Bitmap subfield~~,~~ ~~which~~ that corresponds to the link indicated by the Link ID Bitmap subfield~~,~~ is set to 0.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[15] 241.44 - The EHT STA obtains a set of channel configuration parameters from the EHT Operation Information field (if present) ~~which~~ that is defined in Figure 9-1001c (EHT Operation Information field format).

[Robert: can use “, which” (with comma) since there is only one]

[TGbe Editor: To implement in D5.0 by replacing “which” with “that”.]

[16] 246.32 - The Link ID subfield of the Link ID Info field indicates the link identifier of the AP that is affiliated with the AP MLD ~~which is~~ described in the Basic Multi-Link element and satisfies one of the following

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[17] 246.39 - It is the AP that corresponds to a nontransmitted BSSID that is a member of the same multiple BSSID set as the AP that transmitted the Multiple BSSID element containing the profile for the non-transmitted BSSID ~~which~~ that includes the Basic Multi- Link element.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[18] 246.49 - occurs to the BSS parameters of the AP that is affiliated with an AP MLD ~~which~~  ~~is~~ described in the Basic Multi-Link element and satisfies one of the following:

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[19] 246.56 - It is the AP that corresponds to a nontransmitted BSSID that is a member of the same multiple BSSID set as the AP that transmitted the Multiple BSSID element containing the profile for the non-transmitted BSSID ~~which~~ that includes the Basic Multi- Link element.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[20] 287.1 - Each PPETmax NSSn RUb and PPET8 NSSn RUb subfield contains an integer as defined in Table 9-404q (Constellation index)~~,~~ ~~which~~ that is used to compute the nominal packet padding value (see Table 35-7 (PPE thresholds per PPET8 and PPETmax)).

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[21] 323.13 - indicates the link identifier of the AP ~~which~~ that is indicated for addition to or deletion from the ~~to~~ existing ML setup in the corresponding Link Reconfiguration Request frame

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[22] 369 – Figure 11-21 (appears 3 times) - Authenticated (except DMG STAs that do not perform IEEE Std 802.11 authentication, which are unauthenticated), Unassociated --- Unclear if what was meant was: (except DMG STAs that do not perform IEEE Std 802.11 authentication, or that are unauthenticated) or Authenticated (except DMG STAs that do not perform IEEE Std 802.11 authentication~~, which are unauthenticated~~), Unassociated

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[23] 376.13 - The state for any other AP, AP MLD, or PCP ~~which~~ that is State 3 or State 4

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[24] 376.27 - the state for any other AP or PCP ~~which~~ that is State 3 or State 4 prior to the association request

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[25] 381.53 - the state for any other AP or PCP ~~which~~ that is State 3 or State 4 prior to the association request

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[26] 423.10 - a Supplicant selects a pairwise cipher suite ~~which~~ that is advertised by an AP, but ~~which~~ that policy disallows for this particular STA.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[27] 438.6 – Transaction Sequence number (1 octet) ~~which~~ that shall be set to the value 2

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[28] 438.39 - Transaction Sequence number (1 octet) ~~which~~ that shall be set to the value 3

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[29] 461.35 - Transaction sequence number (1 octet)~~,~~ ~~which~~ that shall be set to the value 5 if this is a Reassociation Request frame and, otherwise, set to the value 3

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[30] 463.1 - Transaction sequence number (1 octet) ~~,~~ ~~which~~ that shall be set to the value 6 if this is a Reassociation Response frame or, otherwise, set to the value 4

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[31] 501.41 - and that includes a Basic Multi-Link element, which can carry complete or partial profile(s), based on the soliciting request,

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[32] 503.44 – unclear - The Common Info field of a Basic Multi-Link element carried in a Beacon frame or a Probe Response frame that ~~, which~~ is not a multi-link probe response~~,~~  shall not include the Medium Synchronization Delay Information subfield.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[33] 513.23 - such that all associated non-AP MLDs including the ones ~~which~~ that have all affiliated non-AP STAs in power save mode

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[34] 515.46 - NOTE 1—The ML reconfiguration operations for adding a link or deleting a link to the ML setup of a non-AP MLD is performed between the two peer MLDs ~~which~~ that are in State 4 (see Figure 11-21 (Relationship between state and services between a given pair of nonmesh STAs or nonmesh MLDs)). For a newly added link to the ML setup, the non-AP STA and the AP operating on that link inherit state from their respective MLDs and are in State 4. For a setup link ~~which~~ that gets deleted from the ML setup, the non-AP STA and the AP ~~which~~ that were previously operating on that link cease to inherit state from their respective MLDs and transition to State 1 (see Figure 11-21 (Relationship between state and services between a given pair of nonmesh STAs or nonmesh MLDs)).

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[35] 515.54 - A non-AP MLD in the associated state ~~which~~ that has dot11EHTLinkReconfigurationOperationActivated equal to true may request ML reconfiguration to its ML setup by sending a Link Reconfiguration Request frame from an affiliated non-AP STA to the corresponding AP affiliated with the associated AP MLD ~~which~~ that has the Link Reconfiguration Operation Support subfield set to 1 in the MLD Capabilities And Operations subfield of the Basic Multi-Link element that it transmits.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[36] 516.27 - The following rules apply for each Per-STA Profile subelement corresponding to a non-AP STA ~~which~~ that is contained in the Reconfiguration Multi-Link element included in the Link Reconfiguration Request frame

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[37] 517.23 - After receiving a Link Reconfiguration Request frame indicating request for adding one or more links from a non-AP STA affiliated with a non-AP MLD ~~which~~ that indicated OCVC in its RSNE

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[38] 517.44 - If the AP MLD receives a Link Reconfiguration Request frame ~~which~~ that indicates both delete link and add link for a given non-AP STA

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[39] 518.37 - After receiving a Link Reconfiguration Response frame ~~which~~ that includes a Group Key Data subfield,

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[40] 521.6 - The AP affiliated with an AP MLD that operates on a link ~~which~~ that is disabled for an associated non-AP MLD

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[41] 524.10 - A non-AP MLD might receive more than one TID-to-link Mapping elements on more than one link ~~which~~ that indicate different times for the advertised TTLM to be established

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[42] 524.62 - then the profile for that nontransmitted BSSID carries a Non-Inheritance element ~~which~~ that includes the Element ID Extension of the TID-To-Link Mapping element.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[43] 525.45 - or at the time indicated by the Expected Duration field of an existing advertised TTLM ~~which~~ that will be replaced by the default mapping

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[44] 528.35 - The BSS Transition Candidate List Entries field, which contains one or more Neighbor Report elements, may be included~~, which contains one or more Neighbor~~  ~~Report elements in order~~ to provide a BSS transition candidate list

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[45] 533.29 - The bitmap corresponding to each scoreboard context control shall have the same size, *WinSizeR*, ~~which that is set to~~ as the smaller of the bitmap length and the buffer size indicated in the ADDBA Response frame.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[46] 537.37 - corresponding to the affected AP ~~which~~ that is contained in the Basic Multi-Link element corresponding to the AP MLD

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[47] 538.24 - corresponding to the affected AP ~~which~~ that is contained in the Basic Multi-Link element corresponding to the AP MLD

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[48] 552.58 - corresponding to a nontransmitted BSSID (maximum possible number of BSSIDs – 1) ~~which~~ that is in the same multiple BSSID set as the AP.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[49] 553.21 - corresponding to a nontransmitted BSSID (maximum possible number of BSSIDs – 1) ~~which~~ that is in the same multiple BSSID set as the AP.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[50] 556.29 - consider the transmit queue for that AC as empty until any frame exists in the queue ~~which~~ that if transmitted, the transmitter determines, will not cause an unacceptable level of interference caused by transmission at the non-AP STA operating on the other link of an NSTR link pair that the AP or non-AP STA belongs to.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[51] 571.32 - the optional features supported by an AP affiliated with an AP MLD ~~which~~ that is not an NSTR mobile AP MLD

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[52] 578.46 – A single TWT agreement is requested for the STA affiliated with the same MLD ~~which~~ that is operating on the indicated link

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[53] 587.51 - An AP shall not send a PPDU that is neither an HE PPDU nor an EHT PPDU ~~which~~ that carries a TRS Control subfield.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[54] 589.32 - The RU\_ALLOCATION parameter is set to the value indicated by the RU Allocation subfield of the TRS Control subfield and a PS160 subfield, which is determined based on the RU allocation in the EHT MU PPDU carrying the TRS control subfield according to Table 35-2 (PS160 subfield for RU allocation in EHT TRS).

[Robert: agree – comma before which]

[TGbe Editor: To implement in D5.0]

[55] 606.29 - The EHT NDP Announcement frame shall be followed after a SIFS by an EHT sounding NDP. The EHT sounding NDP ~~, which~~ shall be followed after a SIFS by a PPDU containing one or more EHT Compressed Beamforming/CQI frames

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[56] 606.38 - The EHT NDP Announcement frame shall be followed after a SIFS by an EHT sounding NDP. The EHT sounding NDP~~, which~~ shall be followed after a SIFS by the BFRP Trigger frame.

[TGbe Editor: To implement in D5.0]

[57] 618.11 - whichever exists and ~~which~~ that is used to determine PHY-CCA.indication

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[58] 624.2 - defines constraints on certain fields ~~which~~ that in turn are constraints on the associated PHY MIB variables.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[59] 656.4 - MU-MIMO reception on an RU or MRU in an EHT TB PPDU ~~which~~ that consists of multiple RU(s) or MRU(s) in the entire PPDU bandwidth

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[60] 657.11 - MU-MIMO reception on an RU or MRU in an EHT MU PPDU ~~which~~ that consists of multiple RUs and/ or MRUs

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[61] 665.28 - MU-MIMO transmission on an RU or MRU in an EHT TB PPDU ~~which~~ that consists of multiple RUs and/or MRUs in the entire PPDU bandwidth

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[62] 677.30 - contains an OPERATING\_CHANNEL parameter~~, which~~ that identifies the operating or primary channel

[Robert: looks ok, no change]

[TGbe Editor: Not implemented]

[63] 677.35 - contains a CHANNEL\_WIDTH parameter~~, which~~ that identifies the operating channel width

[Robert: looks ok, no change]

[TGbe Editor: Not implemented]

[64] 677.41 - contains a CENTER\_FREQUENCY\_SEGMENT\_0 parameter~~, which~~ that identifies the center frequency of the channel

[Robert: looks ok, no change]

[TGbe Editor: Not implemented]

[65] 677.47 - contains a DISABLED\_SUBCHANNEL\_BITMAP parameter~~, which~~ that carries the value of the Disabled Subchannel Bitmap subfield in an EHT Operation element

[Robert: looks ok, no change]

[TGbe Editor: Not implemented]

[66] 719.27 - an MU-MIMO transmission on an RU or MRU in an EHT PPDU ~~which~~ that consists of more than one RU or MRU within the PPDU bandwidth

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[67] 720.59 - UL MU-MIMO transmissions in an EHT TB PPDU ~~which~~ that consist~~s~~ of more than one RU or MRU

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[68] 721.6 - in an EHT PPDU ~~which~~ that consists of more than one RU or MRU within the PPDU bandwidth.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[69] 779.17 - An RU Allocation subfield shall not indicate an RU or MRU ~~which~~ that occupies all nonpunctured 20 MHz channels within the PPDU bandwidth.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[70] 820.12 - as punctured subchannels ~~which~~ that are subject to the additional restrictions as defined in 36.3.20.1.2

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[71] 995.2 - On channel 3, there are three APs ~~which~~ that belong to the same multiple BSSID set

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[72] 997.24 - transmits an Association Request frame ~~which~~ that includes a Basic Multi-Link element

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[73] 998.40 - The frame also carries a Basic Multi-Link element ~~which~~ that is carrying two Per- STA Profile subelements corresponding to STA 1 and STA 2.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[74] 1008.28 - Next the AP MLD starts to advertise a TTLM B ~~which~~ that maps all TIDs to a set of link(s) that is a subset of the enabled link set in the TTLM A.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[75] 1008.62 - Next the AP MLD starts to advertise a TTLM B ~~which~~ that maps all TIDs to a set of link(s) that is a superset of the enabled link set in the TTLM A.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

#### Style Guide 2.8.2 – articles

Joe Levy

No comments received from the reviewer.

#### Style Guide 2.8.3 – missing nouns

Stephen McCann

[01] At P397L63 in clause 11.49, there is a missing “value”. The text should read:

“…ignore the remaining TBTT Information Length field value minus 16 octets…”. Alternatively “TBTT Information Length” could be changed to “TBTT Information length”. It also appears that the baseline text at P397.58 has the same issue.

[Robert: agree]

[TGbe Editor: To implement in D5.0 as “field value” at both locations]

[02] At P592L4, the equation of min(2(23 + Maximum A-MPDU Length Exponent Extension)- 1….), is missing an extra noun. It should use either “Maximum A-MPDU Length Exponent Extension value” or “Maximum A-MPDU Length Exponent Extension subfield”.

There is the same issue at P592L18 and P592L30.

[Robert: fix through comment resolution]

[TGbe Editor: Not implement. Encourage the reviewer to submit a comment in the initial SA ballot]

[03] At P593L32, the text “20 MHz-Only Limited Capabilities Support equal to 1” is missing the word “subfield”. Change it to “20 MHz-Only Limited Capabilities Support subfield equal to 1”

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[04] At P209L9, “Link ID equal” is missing the word “subfield”. Change it to “Link ID subfield equal”. There are the same issues at P209L18 and P209L19 several times and P209L26.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[05] At P291L16, “link ID equal” is missing the word “subfield” and the initial “l” should be capitalised. Change it to “Link ID subfield equal”. There are the same issues at P291L25, P291L30, P291L35, P291L37 and P527L29.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[06] At P350L15, “BSSBasicRateSet that is” is missing the word “parameter”. Change it to “BSSBasicRateSet parameter that is”.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[07] At P376L42, “Timeout Interval Type” is missing the word “field”. Change it to “Timeout Interval Type field”. There are similar issues at P376L45, P382L9 and P382L13.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[08] At P531L36, “Status Code equal” is missing the word “field”. Change it to “Status Code field equal”.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

Extra findings

[09] Note: Regarding the clause title “35.3.16.5.2 End time alignment of response PPDUs using SRS Control field”, this should be “SRS Control subfield”.

[TGbe Editor: To implement in D5.0]

[10] Note: At P422L27, “LinkId field” should be “LinkID field”.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

#### Style Guide 2.8.4 – unnecessary nouns

Stephen McCann

[01] At P359L19, “an interval of PIFS” is unnecessary. Change “an interval of PIFS” to “a PIFS”. There is the same issue at P359L22.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[02] At P545L33, “Examples of listen interval operation in MLO are shown in AF.8.3…”, the word operation is effectively repeated. Change this sentence to “Examples of listen intervals in MLO are shown in AF.8.3…”.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[03] At P71L54, “…operate at any given time in either MLO…”, the acronym MLO is treated as a state, whereas it is a function. Change the text to “operate at any given time as either multi-link…”.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[04] At P71L59, “The reference architecture when operating in MLO…”, the acronym MLO is treated as a state, whereas it is a function. Change the text to “The MLO reference architecture…”.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[05] At P73L38, “When MLO is being used,…”, the acronym MLO is treated as a state, whereas it is a function. Change the text to “In MLO,…”.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[06] At P73L49, “…(Not operating in MLO)…”, the word operate is effectively repeated. Change the text to “(Not in MLO)”.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[07] At P76L37, “Non-MLO peer operations,…”, the word operate is effectively repeated. Change the text to “Non multi-link peer operations,…”.

[Robert: fix through comment resolution]

[TGbe Editor: Not implement. Encourage the reviewer to submit a comment in the initial SA ballot]

[08] At P77L14, “…non-MLO links.”, the word link is effectively repeated. Change the text to “…links.”.

[Robert: fix through comment resolution]

[TGbe Editor: Not implement. Encourage the reviewer to submit a comment in the initial SA ballot]

[09] On P393, there are several occurrences of the text “non-AP STA(for non-MLO) or non-AP MLD (for MLO)”. Clause 1.4 (P49) states that an MLD is used for multi-link operation and a STA is not, so the addition of the terms on this page, in paranthesis, are not required. Change each occurrence of “non-AP STA(for non-MLO) or non-AP MLD (for MLO)” to “non-AP STA or non-AP MLD”.

[Robert: agree]

[TGbe Editor: TGbe does not agree with this commenter. Not implemented. Encourage the reviewer to submit a comment in the initial SA ballot]

[10] At P456L24, “MLO GTK is the MLO GTK subelement…” is repeating the term MLO GTK. Change the text to “MLO GTK is the subelement…”. There is a similar issue on P456L27 and P456L29.

[Robert: agree]

[TGbe Editor: TGbe does not agree with this commenter. Not implemented]

[11] At P59L10, “Operations that do not involve multi-link operation…”, the word operation is repeated. Change the text to “Operations that do not involve multi-links…”.

[Robert: agree]

[TGbe: delete “operation”]

[TGbe Editor: To implement in D5.0]

#### Style Guide 2.8.5 – unicast and multicast

Atsushi Shirakawa

[01] Page 31, line 8: Replace “unicast data frames” with “individually addressed Data frames” because Figure 5-2a is diagram for MAC layer.

[TGbe Editor: Not implement because it is a cross reference]

[02] Page 73, line 17: Replace “unicast data frames” with “individually addressed Data frames” because Figure 5-2a is diagram for MAC layer.

[TGbe Editor: Not implement because it is a cross reference]

[03] Page 73, line 21: Replace “unicast data frames” with “individually addressed Data frames” because Figure 5-2a is diagram for MAC layer.

[TGbe Editor: Not implement because it is a cross reference]

[04] Page 73, line 28: Replace “unicast data frames” with “individually addressed Data frames” because Figure 5-2a is diagram for MAC layer.

[TGbe Editor: Not implement because it is a cross reference]

[05] Page 73, line 34: Replace “unicast data frames” with “individually addressed Data frames” because Figure 5-2a is diagram for MAC layer.

[TGbe Editor: Not implement because it is a cross reference]

[06] Page 73, line 38: Replace “unicast MPDUs” with “individually addressed MPDUs”.

[TGbe Editor: To implement in D5.0]

[07] Page 73, line 41: Replace “unicast MPDUs” with “individually addressed MPDUs”.

[TGbe Editor: To implement in D5.0]

[08] Page 73, line 44: Replace “unicast data frames” with “individually addressed Data frames” because Figure 5-2a is diagram for MAC layer.

[TGbe Editor: Not implement because it is a cross reference]

[09] Page 74, line 60: Replace “unicast data frames” with “individually addressed Data frames” because Figure 5-2a is diagram for MAC layer.

[Robert: agree – one change to figure title]

[TGbe Editor: To implement in D5.0]

[10] Page 76, line 14: Replace “unicast frames” with “individually addressed frames” because this sentence describe MAC layer function.

[TGbe Editor: To implement in D5.0]

[11] Page 76, line 18: Replace “unicast frames” with “individually addressed frames” because this sentence describe MAC layer function.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[12] Page 77, line 24: Replace “unicast data frames” with “individually addressed Data frames” because Figure 5-2a is diagram for MAC layer.

[TGbe Editor: Not implement because it is a cross reference]

[13] Page 77, line 47: Replace “unicast data frames” with “individually addressed Data frames” because Figure 5-2a is diagram for MAC layer.

[TGbe Editor: Not implement because it is a cross reference]

### Style Guide 2.9 – Numbers

Alfred Asterjadhi

[01] Please replace “zeros” with “0s” throughout the draft.

[Action: Edward to review case by case]

[Edward: In D4.1, replace “zeros” with “0s” at 834.51]

[TGbe Editor: To implement in D5.0]

[02] Please replace “20MHz” with “20 MHz”, 80MHz with 80 MHz, 160MHz with 160 MHz, 320MHz with 320 MHz

[Action: Add spaces as appropriate]

[Edward: In D4.1, add the missing space at 312.40, 312.42, 647.58, 697.14, 721.28.

[TGbe Editor: To implement in D5.0]

### Style Guide 2.10 – Maths operators and relations

Claudio da Silva

A range of values is represented in two different ways in the TXVECTOR/RXVECTOR table: “Integer in the range: 0–15” and “Set to a value in the range 0 to 63”. Not sure if this is a problem. Based on 2.10, I believe “x to y” is preferred.

[Action: change n-dash to “to”, otherwise no change]

[TGbe Editor: To implement in D5.0]

Also, please note that both ranges include integers only. This is defined only in the first sentence. Not sure if this definition is necessary.

Multiplication is represented by a space or by an x in most of the draft. However, a dot is used in some equations, such as (36-116), (36-120), and (36-122). I’m not sure if this breaks any rules, but it is inconsistent with the first part of the draft.

[Action: No change]

[TGbe Editor: Not implement]

### Style Guide 2.11 – Hyphenation

Alfred Asterjadhi

[01] Please replace “non-dynamic” with “nondynamic” throughout the draft.

[Robert: agree]

[TGbe Editor: To implement in D5.0]

[02] Please replace “non-multiple BSSID” with “single BSSID” throughout the draft.

[Robert: fix through comment resolution]

[TGbe Editor: Not implement. Encourage the reviewer to submit a comment in the initial SA ballot]

[03] Please replace “non-high-throughput” with “non-high throughput” throughout the draft.

[Robert: agree, use n-dash]

[TGbe Editor: To implement in D5.0]

[04] Please replace “non-reserved” with “nonreserved” throughout the draft.

[Robert: keep hyphenated word]

[TGbe Editor: Not implement]

[05] Please replace “De-aggregation” with “Deaggregation” throughout the draft.

[Robert: keep hyphenated word]

[TGbe Editor: Not implement]

[06] Please replace “pre-correction “ with “precorrection” throughout the draft.

[Robert: keep hyphenated word]

[TGbe Editor: Not implement]

[TGbe: ask the WG editors to make sure the grandfather list of the style guide is up-to- date]

[07] Please replace “STA to STA” with “STA-to-STA” throughout the draft.

[Action: Edward to review]

[TGbe Editor: To implement in D5.0]

### Style Guide 2.12 – References to SAP primitives

Graham Smith

This new way of describing the primitives, and indicating when you might want to provide full details, is described in 11me D 3.0 at

“6.5 MLME SAP primitives

6.5.1 Introduction

MLME SAP primitives are detailed in this clause when they do not directly correspond to frame exchanges described in subsequent clauses, where the primitive parameters differ significantly from the fields in the respective frames, or when the primitives may not be clear from the descriptions in those clauses.”

Hence, again, I suggest deleting from P80.27 to P112.40

[Action: review suggested changes with task group]

[TGbe Editor: To implement in D5.0 by removing subclauses 6.5.24a, 6.5.24b, and 6.5.24c. Note that this change is made via a comment resolution]

### Style Guide 2.13 – References to the contents of a field/subfield

Emily Qi

No issues were found.

### Style Guide 2.14 – MIB attributes

Yongho Seok

No comments received from the reviewer.

### Style Guide 2.15 – Hanging Paragraphs

Claudio da Silva

I did not find a hanging paragraph. However, 35.3.16.2 (Multi-link device capability and operation signaling) only has one sub-clause: 35.3.16.2.1 (General). I’m not sure if this breaks any rules, but it looks awkward to me.

[Action: remove subclause heading]

[TGbe Editor: To implement in D5.0. Note that this change is made via a comment resolution]

### Style Guide 2.16 – Abbreviations

Ross Yu

Discussion

Editorial guide for abbreviations:

Abbreviations may be defined for terms that are used frequently throughout the document. When an abbreviation has been defined, use it. (If you don’t the publication editor will probably replace most occurences in the text of the full term with the abbreviation).

But don’t create abbreviations for:

* Terms used only a handful of times
* Names of fields, structures, elements or frames

Do not include an abbreviation of the name of a field in the name of the field itself. e.g., a field labelled “Number of Taps (N\_taps)” is wrong.

Don’t create an abbreviation that includes the whole of a noun phrase – e.g., a XYZE being defined as an Xray Yankee Zulu element. This causes confusion because names are generally adjectives followed by a noun.

[01] Page 55, line 41, remove “[non-HT]”.

[TGbe Editor: To implement in D5.0 by removing “(non-HT)”]

[02] Page 55, line 56, add “(RU)” after “resource unit”, remove “[RU]”.

[TGbe Editor: Not implement as per the latest style applicable to Clause 3]

[03] Page 55, line 59, add “(SP)” after “service period”, remove “[SP]”.

[TGbe Editor: Not implement as per the latest style applicable to Clause 3]

[04] Page 58, line 20, add “(MLD)” after “multi-link device”, remove “[MLD]”

[TGbe Editor: Not implement as per the latest style applicable to Clause 3].

[05] Page 58, line 30, add “(MLO)” after “multi-link operation”, remove “[MLO]”.

[TGbe Editor: Not implement as per the latest style applicable to Clause 3]

[06] Page 58, line 53, add “(MRU)” after “multiple resource unit”, remove “[MRU]”.

[TGbe Editor: Not implement as per the latest style applicable to Clause 3]

[07] Page 59, line 10, remove “[non-MLO]”

[TGbe Editor: Not implement as per the latest style applicable to Clause 3]

[08] Page 306, line 8, add “(BTM)” after “BSS Transition Management”

[TGbe Editor: Not implement as per the latest style applicable to capitalization]

[Action: as suggestion]

Discussion:

BSS Transition Management exists in Draft P802.11REVme D4.0 for 290 times

BTM exists in Draft P802.11REVme D4.0 for 35 times for MLME and BTM Status Code

The abbreviation of BTM is defined in Draft P802.11be D4.0, but not in P802.11REVme D4.0.

BSS Transition Management Request frame, BSS Transition Management Query frame, and BSS Transition Management Response frame are used in Draft P802.11REVme D4.0 without using BTM.

In Draft P802.11be D4.0, BSS Transition Management exists for 72 times, BTM exists for 11 times. The reviewer intends to follow REVme style that expands BTM to BSS Transitions Management for the frames.

No changes for “35.3.23 (BSS transition management for MLDs)” in P223, L3 and several other places.

No changes for “BTM request and remain” in P308, L7.

No changes for “non-AP STAs that support BTM and” in P513, L36.

No changes for “shall interpret the BTM to” in P514, L37.

[09] Page 514, line 26, change “BTM Request frame(s)” to “BSS Transition Management Request frame(s)”

[TGbe Editor: To implement in D5.0]

[10] Page 514, line 43, change “BTM Request frame” to “BSS Transition Management Request frame”

[TGbe Editor: To implement in D5.0]

[11] Page 514, line 44, change “BTM Request frame” to “BSS Transition Management Request frame”

[TGbe Editor: To implement in D5.0]

[12] Page 529, line 29, change “BTM Request frame” to “BSS Transition Management Request frame”

[TGbe Editor: To implement in D5.0]

[13] Page 351, change “EHT link adaptation procedure” to “ELA procedure”

[TGbe Editor: To implement in D5.0]

[Action: as suggested]

Discussion

restricted TWT exists for 79 times, R-TWT exists for 197 times

No changes for:

Restricted TWT Traffic Info field

Restricted TWT Parameter Set field

Restricted TWT DL TID Bitmap

Restricted TWT UL TID Bitmap

Restricted TWT Support subfield

35.8 Restricted TWT (R-TWT)

[14] Page 366, line 22, change “Restricted TWT parameter set” to “R-TWT parameter set”

[TGbe Editor: To implement in D5.0]

[15] Page 611, line 37 change “Restricted TWT operation” to “R-TWT operation”

[TGbe Editor: To implement in D5.0]

[Action: as suggested]

Discussion

TID-to-link mapping exists for 224 times, TTLM exists for 312 times

No changes for:

9.6.35.2 (TID-To-Link Mapping Request frame format),

9.6.35.3 (TID-To-Link Mapping Response frame format)

9.6.35.4 (TID-To-Link Mapping Teardown frame format)

9.4.2.314 (TID-To-Link Mapping element)

TID-To-Link Mapping Negotiation Support

TID-To-Link Mapping Control field

TID-To-Link Mapping element

TID-To-Link Mapping field

35.3.7.2.4 (Advertised TTLM in Beacon and Probe Response frames) .

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Service Name** | **MLME-XXX** |  |  |  |
|  |  |  |  |  |
| TTLM |  |  |  |  |

**6.5.24b TTLM**

**35.3.7.2 TTLM**

**35.3.7.2.3 Negotiation of TTLM**

**B.4.40.2 EHT MAC features**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Protocol capability** |  |  |  |
| \*EHTM10.4.1 | TTLM |  |  |  |

[16] Page 73, line 22, change “TID-to-link mapping process (see 35.3.7.2 (TTLM))” to “TID-to- link mapping (TTLM) process (see 35.3.7.2 (TTLM)”

[TGbe Editor: To implement in D5.0]

[17] Page 74, line 36 (in figure 5-2a), change “TID-to-Link mapping” to “TTLM”

[TGbe Editor: To implement in D5.0]

[18] Page 74, line 59 (in figure 5-2a), change “TID-to-Link mapping” to “TTLM”

[TGbe Editor: To implement in D5.0]

[19] Page 75, line 31 (in figure 5-2b), change “TID-to-Link mapping” to “TTLM”

[TGbe Editor: To implement in D5.0]

[20] Page 75, line 51 (in figure 5-2b), change “TID-to-Link mapping” to “TTLM”

[TGbe Editor: To implement in D5.0]

[21] Page 76, line 20, change “(TID-to-link mapping (see 35.3.7.2 (TTLM)))” to “(TTLM (see 35.3.7.2 (TTLM)))”

[TGbe Editor: Not implement, as it is a cross reference]

[22] Page 87, line 13 (Primitive parameters), change “TID-To-Link Mapping” to “TTLM”

[TGbe Editor: To implement in D5.0]

[23] Page 88, line 143 (Primitive parameters), change “TID-To-Link Mapping” to “TTLM”

[TGbe Editor: To implement in D5.0]

[24] Page 90, line 25 (Primitive parameters), change “TID-To-Link Mapping” to “TTLM”

[TGbe Editor: To implement in D5.0]

[25] Page 91, line 28 (Primitive parameters), change “TID-To-Link Mapping” to “TTLM”

[TGbe Editor: To implement in D5.0]

[26] Page 92, line 48 (Primitive parameters), change “TID-To-Link Mapping” to “TTLM”

[TGbe Editor: To implement in D5.0]

[27] Page 94, line 15 (Primitive parameters), change “TID-To-Link Mapping” to “TTLM”

[TGbe Editor: To implement in D5.0]

[28] Page 95, line 22 (Primitive parameters), change “TID-To-Link Mapping” to “TTLM”

[TGbe Editor: To implement in D5.0]

[29] Page 96, line 43 (Primitive parameters), change “TID-To-Link Mapping” to “TTLM”

[TGbe Editor: To implement in D5.0]

[30] Page 103, line 50 (Primitive parameters), change “TID-To-Link Mapping” to “TTLM”

[TGbe Editor: Not implement, as it is removed via comment resolution]

[31] Page 104, line 30 (Primitive parameters), change “TID-To-Link Mapping” to “TTLM”

[TGbe Editor: Not implement, as it is removed via comment resolution]

[32] Page 105, line 9 (Primitive parameters), change “TID-To-Link Mapping” to “TTLM”

[TGbe Editor: Not implement, as it is removed via comment resolution]

[33] Page 105, line 55 (Primitive parameters), change “TID-To-Link Mapping” to “TTLM”

[TGbe Editor: Not implement, as it is removed via comment resolution]

[34] Page 528, line 12, change “currently advertised TID-to-link mapping” to “currently advertised TTLM”

[TGbe Editor: To implement in D5.0]

[Action: as suggested]

Disucssion

triggered TXOP sharing exists for 72 times, TXS exists for 83 times

No changes for:

**35.2.1.2 (Triggered TXOP sharing procedure)**

Page 157, line 32 (within trigger frame): GI And HE-LTF Type/Triggered TXOP Sharing Mode

Page 158, line 10 (within trigger frame): GI And HE-LTF Type/Triggered TXOP Sharing Mode

Page 160, line 31: Triggered TXOP Sharing Mode Subfield

**Table 9-53a (Triggered TXOP Sharing Mode subfield encoding).**

Page: 265

Triggered TXOP Sharing Mode 1 Support

Triggered TXOP Sharing Mode 2 Support

TXOP Return Support In Triggered TXOP Sharing Mode 2

Page 123: MU-RTS TXS Trigger frame

[35] Page 62, line 65, add “(TXS)” after “triggered TXOP sharing”

[TGbe Editor: To implement in D5.0]

[36] Page 180, line 11, change “triggered TXOP sharing procedure” to “TXS procedure”

[TGbe Editor: To implement in D5.0]

[37] Page 180, line 13, change “triggered TXOP sharing procedure” to “TXS procedure”

[TGbe Editor: To implement in D5.0]

[38] Page 180, line 16, change “triggered TXOP sharing procedure” to “TXS procedure”

[TGbe Editor: To implement in D5.0]

[39] Page 483, line 60, change “triggered TXOP sharing procedure” to “TXS procedure”

[TGbe Editor: To implement in D5.0]

[Action: as suggested]

Discussion

In Draft P802.11be D4.0, ML exists for 281 times, multi-link exists for 1376 times

multi-link probe exists for 182 times

ML probe exists for 19 times

multi-link device exists for 64 times

multi-link operation exists for 98 times

No changes for:

Basic Multi-Link element

35.3 (Multi-link operation).

[40] Page 58, line 31: remove “[MLO]”, add “(MLO)” after “multi-link operation”

[TGbe Editor: Not implement as per the latest style applicable to Clause 3]

[41] Page 58, line 31: add (ML) after the 2nd “multi-link” and before “setup”

[TGbe Editor: To implement in D5.0]

[Action: as suggested]

No changes for:

multi-link probe request in Page 58, line 36

multi-lnk probe response in Page 58, line 42

Probe Request Multi-Link element in Page 58, line 37

35.3.4.2 (Use of multi-link probe request and response).

[42] Page 59, line 10, remove “[non-MLO]”

[TGbe Editor: Not implement as per the latest style applicable to Clause 3]

[43] Page 59, line 10, change “multi-link operation” to “MLO”.

[TGbe Editor: To implement in D5.0 by replacing multi-link operation with multi-links per another reviewer comment]

[Action: as suggested]

No changes for:

(see 35.3.5.3 (Multi-link tear down procedure))

4.9.6 Reference model for multi-link operation (MLO)

(see 35.3.8 (Block ack procedures in Multi-link operation))

9.4.2.312.6 (EPCS Priority Access Multi-Link element)

9.4.2.312.5 (TDLS Multi-Link element)

35.3.17 (Enhanced multi-link single radio operation), and 35.3.18 (Enhanced multi-link multi-radio operation)

Multi-Link Traffic Indication

9.4.2.315 (Multi-Link Traffic Indication element)

[44] Page 80, line 55, change “MULTI-LINK PROBE” to “ML PROBE”

[TGbe Editor: Not implement, for sake of consistency with “multi-link probe request/response”]

[45] Page 80, line 54, change “Multi-link probe” to “ML probe”

[TGbe Editor: Not implement, for sake of consistency with “multi-link probe request/response”]

[46] Page 82, line 59, change “Multi-link parameters” to “ML parameters”

[TGbe Editor: To implement in D5.0]

[47] Page 83, line 31, change “Multi-link parameters” to “ML parameters”

[TGbe Editor: To implement in D5.0]

[48] Page 84, line 31, change “Multi-link parameters” to “ML parameters”

[TGbe Editor: To implement in D5.0]

[49] Page 85, line 4, change “Multi-link parameters” to “ML parameters”

[TGbe Editor: To implement in D5.0]

[50] Page 85, line 43, change “Multi-link parameters” to “ML parameters”

[TGbe Editor: To implement in D5.0]

[51] Page 87, line 38, change “Multi-link parameters” to “ML parameters”

[TGbe Editor: To implement in D5.0]

[52] Page 89, line 36, change “Multi-link parameters” to “ML parameters”

[TGbe Editor: To implement in D5.0]

[53] Page 90, line 51, change “Multi-link parameters” to “ML parameters”

[TGbe Editor: To implement in D5.0]

[54] Page 91, line 46, change “Multi-link parameters” to “ML parameters”

[TGbe Editor: To implement in D5.0]

[55] Page 93, line 8, change “Multi-link parameters” to “ML parameters”

[TGbe Editor: To implement in D5.0]

[56] Page 94, line 47, change “Multi-link parameters” to “ML parameters”

[TGbe Editor: To implement in D5.0]

[57] Page 95, line 53, change “Multi-link parameters” to “ML parameters”

[TGbe Editor: To implement in D5.0]

[58] Page 96, line 62, change “Multi-link parameters” to “ML parameters”

[TGbe Editor: To implement in D5.0]

[59] Page 98, line 7, change “Multi-link parameters” to “ML parameters”

[TGbe Editor: To implement in D5.0]

[Action: as suggested (clause 6 might delete all this)]

No changes for:

see 35.3.2 (Multi-link device addressing)

in 35.3.20 (Multi-link operation in a multiple BSSID set or co-hosted BSSID set) and a single Reconfiguration Multi-Link element is optionally present (see 35.3.6.3 (Removing affiliated APs));

(see 35.3.11 (Multi-link procedures for (extended) channel switching and channel quieting)):

35.3.3 (Advertisement of multi-link information in Multi-Link element) when it includes a Basic Multi-Link subelement in the Neighbor Report element.

Multi-Link Control field

The TDLS Multi-Link element

Multi-Link Operation Update Request

Multi-Link Operation Update Response

Reconfiguration Multi-Link element

35.3.15 (Multi-link operation group addressed frames)

35.3.14 (Multi-link device individually addressed Management frame delivery))

(see 35.3.12 (Multi-link power management)).

an exchange of Multi-Link Probe Request and Multi-Link Probe Response frames

35.3.21 (TDLS procedure in multi-link operation).

35.3.2 Multi-link device addressing

35.3.16 Multi-link channel access

35.3.19.3 NSTR mobile AP MLD multi-link procedures for channel switching, extended channel switching, and channel quieting

35.3.20 Multi-link operation in a multiple BSSID set or co-hosted BSSID set

[60] Page 483, line 22, change the 1st “multi-link operation” to “MLO”.

[TGbe Editor: To implement in D5.0]

[61] Page 492, line 58, change “multi-link operations” to “MLOs”.

[TGbe Editor: To implement in D5.0]

[62] Page 573, line 24, change “Multi-link procedures” to “ML procedures”

[TGbe Editor: To implement in D5.0]

[63] Page 993,line 31, change “multi-link operation” to “MLO”.

[TGbe Editor: To implement in D5.0]

[64] Page 1007, line 37, change the 1st “multi-link setup” to “ML setup”

[TGbe Editor: To implement in D5.0]

[65] Page 1007, line 58, change “multi-link setup” to “ML setup”

[TGbe Editor: To implement in D5.0]

[66] Page 1008, line 3, change “multi-link setup” to “ML setup”

[TGbe Editor: To implement in D5.0]

[67] Page 1008, line 8, change “multi-link setup” to “ML setup”

[TGbe Editor: To implement in D5.0]

[68] Page 1008, line 13, change “multi-link setup” to “ML setup”

[TGbe Editor: To implement in D5.0]

[69] Page 1012, line 36, change “multi-link operation” to “MLO”.

[TGbe Editor: To implement in D5.0]

[70] Page 1018, line 63, change “multi-link operation” to “MLO”.

[TGbe Editor: To implement in D5.0]

[71] Page 1023, line 42, change “multi-link channel access” to “ML channel access”

[TGbe Editor: To implement in D5.0]

[Action: as suggested]

No changes for:

35.3.5 (ML (re)setup).

35.3.5.1 (ML (re)setup procedure)

35.3.5.2 ML security

35.3.5.4 Basic Multi-Link element usage in the context of ML (re)setup, authentication, and FT action frame exchange between two MLDs

35.3.4.6 Frame exchange sequences during MLO discovery and ML setup

35.3.6 (ML reconfiguration)

35.3.6.4 (ML reconfiguration to the ML setup)

35.3.6.5 AP MLD recommendation for ML reconfiguration

35.3.16.9 ML retransmit procedures

AF.2.3 Contents of Management frames during ML reconfiguration AP remove operation

AF.4 Example of ML setup

AF.8 ML power-save operation

Figure 35-5—Possible frame exchange sequences during MLO discovery and ML setup when the AP operating on the channel does not correspond to a nontransmitted BSSID

Figure AF-4—Contents of a Beacon frame or a non-multi-link probe response during ML reconfiguration AP removal procedure (non-multiple BSSID scenario)

Figure AF-5—Contents of a Beacon frame or a non-multi-link probe response during ML reconfiguration AP removal procedure for an AP affiliated with the AP MLD of the transmit-ted BSSID

Figure AF-6—Contents of a Beacon frame or a non-multi-link probe response during ML reconfiguration AP removal procedure for an AP affiliated with the AP MLD of a nontrans-mitted BSSID

Figure AF-7—Contents of a multi-link probe response during ML reconfiguration AP removal procedure for an AP affiliated with the AP MLD of the transmitted BSSID

Figure AF-8—Contents of a multi-link probe response during ML reconfiguration AP removal procedure for an AP affiliated with the AP MLD of a nontransmitted BSSID

Figure AF-11—Contents of an Authentication frame transmitted by a non-AP STA affiliated with a non-AP MLD during ML setup

Figure AF-12—Contents of a (Re)Association Request frame transmitted by a non-AP STA affiliated with a non-AP MLD during ML setup

Figure AF-15—Contents of an Authentication frame transmitted by an affiliated AP that is nota member of a multiple BSSID set during ML setup

Figure AF-20—Contents of an Authentication frame transmitted by an AP affiliated with an AP MLD that is a member of multiple BSSID set during ML setup

Figure AF-21—Contents of a (Re)Association Response frame transmitted by nontransmittedBSSID corresponding to index 5 during ML setup

ML reconfiguration operations

ML setup

### Style Guide 2.17 – Format for code/pseudocode

Ross Yu

No issues were found.

### Style guide 3 – Style applicable to specific Clauses

#### Definitions (Clause 3)

Youhan Kim

(Please enable Change Tracking for better viewing of the changes.)

[01] P56L2: Change

“~~non-access-point~~non-access point”

to

“non-access point” (no strikeout, no underline).

(Reason: The same change has already been made at REVme D4.0 P239L62.)

[Action: already in REVme; reverse chage in 11be]

[TGbe Editor: To implement in D5.0]

[02] P56L11:

**20 MHz-only non-access point (non-AP) extremely high throughput station (EHT STA):** [20 MHz-only non-AP EHT STA] …

(Reason: Acronym missed the phrase “-only”.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[03] P56L60:

**affiliated AP:** An affiliated station (STA) that is an access point (AP) and …

(Reasons: An AP is a STA – see REVme D4.0 P180L18. Also, neither REVme D4.0 nor TGbe D4.0 contains a definition for an “AP STA” in Clause 3.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[04] P56L64:

**affiliated non-access point (non-AP) station (STA):** [affiliated non-AP STA] An affiliated STA that is a non-AP STA …

(Reason: Need to spell out acronyms within the definition terms.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[05] P57L1:

**affiliated station (STA):** [affiliated STA] A STA, which can be an access point (AP) or non-access point (non-AP) STA (non-AP STA), …

(Reason: Need to expand acronyms within the definition terms. AP is a STA. Use the full acronym ‘non-AP STA’.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[06] P57L6:

**disabled link:** A setup link of a non-access point (non-AP) multi-link device (non-AP MLD) to which no traffic identifier (TID) is mapped …

(Reason: Expand acronyms when used first time in the definition.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[07] P57L11:

**emergency preparedness communications service (EPCS) priority access:** [EPCS priority access] A dynamically invoked functionality that allows access point (AP) multi-link devices (AP MLDs) to authorize and facilitate non-access point (non-AP) MLDs (non-AP MLDs) to communicate EPCS traffic with a higher priority.

(Reason: Use full acronyms so that it is searchable. E.g., as originally written, a search for “AP MLD” will not return this location.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[08] P57L16:

**emergency preparedness communications service (EPCS) traffic:** [EPCS traffic] All traffic generated by a non-access point (non-AP) multi-link device (non-AP MLD) or traffic destined for a non-AP MLD when the EPCS priority access is authorized and enabled for that non-AP MLD.

(Reason: Use full acronyms.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[09] P57L20:

**enabled link:** A setup link of a non-access point (non-AP) multi-link device (non-AP MLD) to which at least one traffic identifier (TID) is mapped …

(Reason: Expand acronyms when used first time in the definition.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[10] P57L25:

**enhanced multi-link multi-radio (EMLMR) operation:** [EMLMR operation] A mode of operation that allows a non-access point (non-AP) multi-link device (non-AP MLD) with multiple receive chains to listen on a set of enabled links when the corresponding stations (STAs) affiliated with the non-AP MLD are in awake state for an initial frame sent by an access point (AP) affiliated with an AP multi-link device (AP MLD) in a physical layer (PHY) protocol data unit (PPDU) whose Nss satisfy the receiving STA’s receiving capabilities, followed by frame exchanges that satisfy the MCS, Nss capabilities in EMLMR mode on the link on which the initial frame was received.

(Reason: Use full acronyms. Expand acronyms when used first time in the definition.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[11] P57L33:

**enhanced multi-link single radio (EMLSR) operation:** [EMLSR operation] A mode of operation that allows a non-access point (non-AP) multi-link device (non-AP MLD) with multiple receive chains to listen on a set of enabled links when the corresponding stations (STAs) affiliated with the non-AP MLD are in the awake state for an initial Control frame sent by an access point (AP) affiliated with an AP multi-link device (AP MLD) in a non-high-throughput (non-HT) (duplicate) physical layer (PHY) protocol data unit (non-HT duplicate PPDU) with one spatial stream, followed by frame exchanges on the link on which the initial Control frame was received.

(Reason: Use full acronyms. Expand acronyms when used first time in the definition.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[12] P57L46:

**extremely high throughput (EHT) beamformee:** [EHT beamformee] An EHT station (STA) that receives an EHT physical layer (PHY) protocol data unit (EHT PPDU) that was transmitted using a beamforming steering matrix.

(Reason: Use full acronym.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[13] P57L54:

**extremely high throughput (EHT) modulation and coding scheme (MCS):** [EHT-MCS] A specification of the EHT physical layer (PHY) parameters that consists of modulation order (BPSK, QPSK, 16- QAM, 64-QAM, 256-QAM, 1024-QAM, 4096-QAM) and forward error correction (FEC) coding rate (1/2, 2/3, 3/4, 5/6) and that is used in an EHT PHY protocol data unit (EHT PPDU).

(Reason: Put the full acronym of the definition term in [] after the “:”. Use full acronym.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[14] P58L2:

**extremely high throughput (EHT) single user (SU) transmission:** [EHT SU transmission] A transmission to a single user using the non-orthogonal frequency division multiple access (non-OFDMA) EHT multi-user (MU) physical layer (PHY) protocol data unit (non-OFDMA EHT MU PPDU) format that is not an EHT sounding null data PPDU (EHT sounding NDP). See 36.3.19 (EHT SU transmission).

(Reason: Use full acronym.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[15] P58L12:

**mobile access point (AP):** [mobile AP] An AP that is capable of keeping its Basic Service Set(s) (BSS(es)) operational while its geolocation is changed.

(Reason: Expand acronyms only once.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[16] P58L16:

**mobile access point (AP) multi-link device (MLD):** [mobile AP MLD] An AP multi-link device (AP MLD) where all affiliated APs are colocated and are mobile APs.

(Reason: Expand acronyms only once. Use full acronym.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[17] P58L23:

**multi-link device:** [MLD] A logical entity that is capable of supporting more than one affiliated station (STA) and can operate using one or more affiliated STAs, and that presents one medium access control (MAC) data service and a single MAC service access point (MAC SAP) to the logical link control (LLC) sublayer.

(Reason: Use full acronym.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[18] P58L27:

**multi-link device (MLD) max idle period:** [MLD max idle period] A time period during which the access point (AP) MLD (AP MLD) does not disassociate a non-AP MLD due to nonreceipt of frames from any of the stations (STAs) affiliated with that non-AP MLD.

(Reason: Use full acronym.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[19] P58L36:

**multi-link probe request:** A Probe Request frame that is transmitted by a station (STA) affiliated with a non-access point (non-AP) multi-link device (non-AP MLD) carrying a Probe Request Multi-Link element to solicit information of one or more access points (APs) affiliated with an AP multi-link device (AP MLD) as defined in 35.3.4.2 (Use of multi-link probe request and response).

(Reason: Use full acronym.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[20] P58L43:

**multi-link probe response:** A Probe Response frame transmitted by an access point (AP) affiliated with an AP multi-link device (AP MLD) carrying a Basic Multi-Link element in response to a multi-link probe request to provide complete profile or requested information of one or more APs affiliated with an AP MLD as defined in 35.3.4.2 (Use of multi-link probe request and response).

(Reason: Use full acronym.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[21] P58L52:

**multiple resource unit (RU):** [MRU] A group of subcarriers that consist of multiple RUs of 26-tone RU, 52-tone RU, 106-tone RU, 242-tone RU, 484-tone RU, 996-tone RU, and 2×996-tone RU.

(Reason: Use the acronym “RU”.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[22] P59L2:

**nonsimultaneous transmit and receive (NSTR) mobile access point (AP) multi-link device (MLD):**

[NSTR mobile AP MLD] A mobile access point (AP) multi-link device (mobile AP MLD) with one nonsimultaneous transmit and receive (NSTR) link pair.

(Reason: Use full acronym.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[23] P59L10:

**non-multi-link operation:** [non-MLO] Operations that do not involve multi-link operation between two multi-link devices (MLDs) as described in 35.3 (Multi-link operation).

(Reason: Put the full acronym after the “:”. Expand acronym during first usage.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[24] P59L27:

**non-trigger-based (non-TB) physical layer (PHY) protocol data unit (PPDU):** [non-TB PPDU] A PPDU that is not transmitted using high efficiency (HE) TB PPDU (HE TB PPDU) or extremely high throughput (EHT) TB PPDU (EHT TB PPDU) format.

(Reason: Use full acronym.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[25] P59L65:

**trigger based (TB) physical layer (PHY) protocol data unit (PPDU):** [TB PPDU] A PPDU transmitted with high efficiency (HE) TB PPDU (HE TB PPDU) format or extremely high throughput (EHT) TB PPDU (EHT TB PPDU) format.

(Reason: Use full acronym.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

[26] P60L1:

**setup link:** Between the access point (AP) multi-link device (AP MLD) and the associated non-access point (non-AP) MLD (non-AP MLD), a link that is requested by the non-AP MLD in the (Re)Association Request frame and is accepted by the AP MLD in the (Re)Association Response frame (see 35.3.5 (ML (re)setup)).

(Reason: Use full acronym.)

[Action: as suggested]

[TGbe Editor: To implement in D5.0]

#### General Description (Clause 4)

Po-Kai Huang

Clause 4 provides a general description of the wireless system. It should be written in declarative, not normative, language.

[01] Page 71, line 57: Please replace two instances of “may” with “might”.

[TGbe Editor: To implement in D5.0]

#### Frame formats (Clause 9) – shall or may?

Ming Gan

[01] Page 204, line 64: Please replace “shall” with “does”.

[TGbe Editor: To implement in D5.0]

[02] Page 236, line 48: Please replace “may” with “might”.

[TGbe Editor: To implement in D5.0]

[03] Page 294, line 45: Please replace “may” with “might”.

[TGbe Editor: To implement in D5.0]

[04] Page 308, line 7: Please replace “may” with “might”.

[TGbe Editor: To implement in D5.0]

#### SAP interfaces (Clause 6)

Graham Smith

I have looked at Clause 6 of 11be Draft 4.0. They have added 5 MLME SA interfaces to Table 6-1 and these look OK. However, they have also added the same 5 in all their glory into section 6.5. The new idea introduced in 11me, is that the 31 pages describing these individual primitives are not required. There is enough in the Table, together with the references, to instruct the user on what to do.

I would propose that the 31 pages from 80.27 to 112.40 are deleted.

[Action: review suggestion from Graham of deleting the 31 pages with task group]

If, however, the authors feel that the full details are needed because it is particularly complicated or the contents of the primitives are not obvious from the text, then they can opt to include them in their full glory. However, in this case, in Table 6-1, the references in the Table should be to 6.5.24a/b/c/d/e/f. The Comment column can stay.

BUT

The idea of the Table 6-1 is that in the vast majority of cases the primitives are obvious once the Type is specified and hence we do not need the full descriptions which wasted hundreds of pages.

[TGbe Editor: To implement in D5.0 by removing subclauses 6.5.24a, 6.5.24b, and 6.5.24c. Note that this change is made via a comment resolution]

#### New top level clauses

Emily Qi

[01] 554.28: 35.3.16.2 has only one subclause 35.3.16.2.1 General. Should the subclause 35.3.16.2.1 number be removed?

[TGbe Editor: To implement in D5.0. Note that this change is made via a comment resolution]

#### Annex A – Bibliography

Not applicable

#### Annex B – PICS

Po-Kai Huang

[01] Page 924, line 33: Please replace “EHT Action frames” with “EHT Action frame”.

[TGbe Editor: To implement in D5.0]

[02] Page 925, line 31: Please replace “EHT Action frames” with “EHT Action frame”.

[TGbe Editor: To implement in D5.0]

[03] Page 926, line 21: Please replace “FR76” for EHT NDP Announcement frame with “FR77”. Note otherwise, there are duplicate FR76.

[TGbe Editor: To implement in D5.0]

Several instances about bold texts in B.4.40.1 EHT PHY features and B.4.40.2 EHT MAC features. Note that in revme D3.1 all texts in the corresponding clause are not bold. Also, fix several editorial. Details below.

[04] Page 926, line 37: add one row above EHT P1 with only “Are the following PHY protocol features supported?” in the column of Protocol capability

[TGbe Editor: To implement in D5.0]

[05] Page 926, line 37: Please replace “**EHTP1**” with “EHTP1” and “**PHY operating modes**” with “PHY operating modes”

[TGbe Editor: To implement in D5.0]

[06] Page 926, line 60: Please replace “**EHTP2**” with “EHTP2” and “**EHT PPDU formats**” with “EHT PPDU format”

[TGbe Editor: To implement in D5.0]

[07] Page 928, line 4: Please replace “**EHTP3**” with “EHTP3” and “**BSS Bandwidth**” with “BSS Bandwidth”

[TGbe Editor: To implement in D5.0]

|  |  |
| --- | --- |
|  |  |

[08] Page 928, line 55: Please replace “**EHTP4**” with “EHTP4” and “**EHT LTF formats**” with “EHT-LTF formats”

[TGbe Editor: To implement in D5.0]

[09] Page 930, line 16: Please replace “**EHTP5**” with “EHTP5” and “**RU support**” with “RU support”

[TGbe Editor: To implement in D5.0]

[10] Page 931, line 42: Please replace “**EHTP6**” with “EHTP6” and “**Coding**” with “Coding”

[TGbe Editor: To implement in D5.0]

[11] Page 931, line 54: Please replace “**EHTP7**” with “EHTP7” and “**EHT MCS support**” with “EHT-MCS support”

[TGbe Editor: To implement in D5.0]

[12] Page 934, line 14: Please replace “**EHTP8**” with “EHTP8” and “**Preamble**” with “Preamble”

[TGbe Editor: To implement in D5.0]

[13] Page 934, line 41: Please replace “**EHTP9**” with “EHTP9” and “**Sounding**” with “Sounding”

[TGbe Editor: To implement in D5.0]

[14] Page 935, line 50: Please replace “**EHTP10**” with “EHTP10” and “**Spatial reuse**” with “Spatial reuse”

[TGbe Editor: To implement in D5.0]

[15] Page 935, line 55: Please replace “**EHTP11**” with “EHTP11” and “**Power boost factor**” with “Power boost factor”

[TGbe Editor: To implement in D5.0]

[16] Page 936, line 7: Please replace “**Are the following MAC protocol features supported?**” with “Are the following MAC protocol features supported?”

[TGbe Editor: To implement in D5.0]

[17] Page 936, line 10: Please replace “**EHTM1**” with “EHTM1” and “**EHT capabilities signaling**” with “EHT capabilities signaling”

[TGbe Editor: To implement in D5.0]

[18] Page 936, line 31: Please replace “**EHTM2**” with “EHTM2” and “**Signaling of EHT operation**” with “Signaling of EHT operation”

[TGbe Editor: To implement in D5.0]

[19] Page 936, line 34: Please replace “**EHTM3**” with “EHTM3” and “**HE variant HT Control field**” with “HE variant HT Control field”

[TGbe Editor: To implement in D5.0]

[20] Page 936, line 43: Please replace “**EHTM4**” with “EHTM4” and “**Restricted TWT**” with “Restricted TWT”

[TGbe Editor: To implement in D5.0]

[21] Page 936, line 45: Please replace “**EHTM5**” with “EHTM5” and “**EPCS priority access**” with “EPCS priority access”

[TGbe Editor: To implement in D5.0]

[22] Page 936, line 47: Please replace “**EHTM6**” with “EHTM6” and “**Triggered TXOP sharing procedure**” with “Triggered TXOP sharing procedure”

[TGbe Editor: To implement in D5.0]

[23] Page 936, line 48: Please replace “**EHTM7**” with “EHTM7” and “**EHT BSS operation**” with “EHT BSS operation”

[TGbe Editor: To implement in D5.0]

[24] Page 936, line 57: Please replace “**EHTM8**” with “EHTM8” and “**Transmit beamforming**” with “Transmit beamforming”

[TGbe Editor: To implement in D5.0]

[25] Page 936, line 57: Reference of EHTM8.1 to EHTM8.6 is 36.1.1, which is a PHY clause even though we talk about MAC function. The right reference seems to be 9.4.2.313 EHT Capabilities element. This is how HE provide the reference for Transmit beamforing. See revme D3.1

[TGbe Editor: To implement in D5.0]

[26] Page 937, line 30: Please replace “**EHTM9**” with “EHTM9” and “**MU Beamforming capable**” with “MU Beamforming capable”

[TGbe Editor: To implement in D5.0]

[27] Page 937, line 44: Please replace “**EHTM10**” with “EHTM10” and “**EHT MLD features**” with “EHT MLD features”

[TGbe Editor: To implement in D5.0]

[28] Page 939, line 17: Please replace “**EHTM11**” with “EHTM11” and “**EHT sounding protocol**” with “EHT sounding protocol”

[TGbe Editor: To implement in D5.0]

[29] Page 926, line 32: Please add description to all the references in References column of B.4.3 IUT configuration, B.4.4.2 MAC frames, B.4.40.1 EHT PHY features and B.4.40.2 EHT MAC features. For example, “Clause 17” should be “Clause 17 (Orthogonal frequency division multiplexing (OFDM) PHY specification)”. Note that in revme D3.1, all references have descriptions.

[TGbe Editor: Not implement. Will implement prior to the publication of the standards.]

#### Annex G – Frame exchange sequences

Not applicable

## ANA

Check for correct use of numbers against database.

Check names against database (update database if names have changed).

Robert Stacey

|  |  |  |  |
| --- | --- | --- | --- |
| **Resource** | **Ref** | **Value** | **Status** |
| StatusCodes | Table 9-78 | 130-135, 139-141 | OK |
| ReasonCodes | Table 9-49 | None | OK |
| Element ID Extension 1 | Table 9-128 | 106-110, 113, 133-135 | OK |
| Categories | Table 9-79 | 36, 37 | OK |
| FastBSSTransitionSubElementIDs | Table 9-219 | 8-10 | OK |
| ExtendedCapabilities | Table 9-190 | 103 | Draft shows <ANA> for 103 |
| CipherSuitSelectors | Table 9-186 | None | OK |
| AKMSuiteSelectors | Table 9-188 | None | OK |
| RSNCapabilities | Figure 9-345 | None | OK |
| ExtendedRSNCapabilitieis | Table 9-365 | None |  |
| Neighbor Report Subelement IDs | Table 9-210 | 199-201 | OK |
| Public Action field values | Table 9-450 | None | OK |
| ANQP-element InfoID | Table 9-412 | None | OK |
| FILS Discovery frame Control field | Figure 9-1127 | None | OK |
| Dot11smt | MIB | 46-47 | OK |
| Dot11StationConfigEntry | MIB | 205, 222-223, 228-232 | Draft shows <ANA> for 230-232 |
| Dot11phy | MIB | 35-36 | OK |
| Dot11Groups | MIB | 120-122 | OK |
| OperatingClassGlobal | Annex E | 137 | Used without allocation (no conflict) |

Additional Actions:

Replace <ANA> with assigned number for dot11StationConfigEntry and ExtendedCapabilities.

[TGbe Editor: Not implement. These assigned numbers were updated in D4.1.]

Send ANA request for OperatingClassGlobal value 137.

[TGbe Editor: To implement in D5.0]

## MIB

Yongho Seok

The compiled MIB is embedded as the following.

[Embed MIB after compilation]

### Detailed proposed changes

No comments received from the reviewer.

* MIB Detail

# Collateral findings

None

# IEEE-SA MEC

|  |
| --- |
| From: Michelle Turner  Sent: Monday, November 13, 2023 3:49 AM  To: Stacey, Robert  Cc: Christy Bahn  Subject: MEC for IEEE P802.11be  Hello Robert,  My apologies for the delay, this one completely slipped through. Please see my official comment with regard to the MEC.  "This draft meets editorial requirements."  --  Michelle Turner  Senior Manager, Content Production and Management  IEEE Standards Association |