IEEE P802.11
Wireless LANs

|  |
| --- |
| LB275 CR for CID 19686 |
| Date: 2023-09-12 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Jeongki Kim | Ofinno |  |  | jkim@ofinno.com |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for the following CID for TGbe LB275:

• 19686

**Revisions:**

* Rev 0: Initial version of the document.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clasue** | **Page/Line** | **Comment** | **Proposed Change** | **Resolution** |
| 19686 | 35.3.7.2.1 | 520.40 | The term "MPDU with TIDs" (mentioned in P520L40) may correspond also to "QoS Null frames".Thus, there is a conflict between the requirement in P520L40 to send the MPDUs only on the links that are mapped to the TIDs of these MPDUs and the requirement in P520L44 which allows the QoS Null frames to be transmitted on any enabled link | Replace the term "MPDUs with TIDs mapped to that link" with "Data frames with TIDs mapped to that link". | RevisedAgree in principle with the comment.To avoid the conflict, “MPDUs with TIDs” should be changed to “QoS data frame with TIDs”. TGbe editor to make the changes shown in 11-23/1617r0 under all headings that include CID 19686 |

**Proposed texts:**

***TGbe editor: Change the following paragraphs in 35.3.7.2.1 General as follows: (#19686):***

**35.3.7.2.1 General**

**…**

If a link is enabled for a non-AP MLD, then:

—it may be used for individually addressed frame exchange, subject to the power state of the non-AP STA operating on that link and only (#19686) QoS Data frames with TIDs mapped to that link may be transmitted on that link between the corresponding non-AP STA and AP affiliated with the non-AP MLD and the AP MLD, respectively, in the direction (DL/UL) corresponding to the TTLM.

—Individually addressed Management frames, QoS Null frames, and Control frames may be sent on any enabled links between the corresponding non-AP MLD and AP MLD both in DL and UL, except that a BlockAckReq frame requesting TID(s) that are not mapped to a link shall not be transmitted on the link by the corresponding non-AP STA affiliated with the non-AP MLD and by the corresponding AP affiliated with the AP MLD.