IEEE P802.11
Wireless LANs

|  |
| --- |
| SA Ballot CR for Miscellaneous CIDs |
| Date: 2024-02-26 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Ming Gan | HuaweiHuawei |  |  | ming.gan@huawei.com |
| Jason Yuchen Guo |  |  |  |
| Yunbo Li | Huawei |  |  |  |
| Guogang Huang | Huawei |  |  |  |
| Zhi Mao | Huawei |  |  |  |
| Lan Peng | Huawei |  |  |  |
| Zhenguo Du | Huawei |  |  |  |
| Steven Qi Wang | Huawei |  |  |  |
| Yue Zhao | Huawei |  |  |  |
| Ying Li | Huawei |  |  |  |
| Maolin Zhang | Huawei |  |  |  |

Abstract

This submission proposes resolutions of comments received from TGbe SA Ballot based on TGbe D5.0.

22103 22209 22214 22322 (4 CIDs)

Revisions:

Rev 0: Initial version of the document.

1. **Introduction**

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. The introduction and the explanation of the proposed changes are not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11be editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 22103 | 11.2.3.14 | 372.45 | On behalf of Laurent Cariou. "shall also be considered as a critical update" is unclear. Please change it to "shall also be reported by the transmitted BSSID as a critical update". Also please clarify that both the critical update flag and non transmitted BSSID critical update flag is set to 1 in this case. | as in comment | Revised-Agree with the comment partially. Rephrase "shall also be considered as a critical update" to "shall also be reported by the transmitted BSSID as a critical update". For the second part, the critical update flag setting rules in clause 9 and clause 35.3.10 are clear, there is no need to clarify them here. Apply the changes marked as #22103 in this document. |
| 22209 | 35.3.12.6 | 553.26 | when the link is disabled, then the STA may cease maintaining a power state and power management mode as soon as practical. So "enable" is redudant when the STA is power save mode. Moreover, in p520 line 24 and p550 line 31, they all don't mention "enable" while saying all affiliated non-AP STAs in power save mode. [m] | Remove "and operating on enabled links" | Accepted- |
| 22214 | 35.3.15.1 | 560.43 | On page 561 line 44, it doesn't mention "enabled links", please make them consistent with each other. Moreover, enabled links may change from time to time, fix size should be easy for parsing. [m] | Remove "that operate on enabled link(s)" | Accepted- |
| 22322 | 35.3.4.4 | 511.29 | [Al Petrick] sub-bullet text " may include.... " needs to be aligned with statement "in a Beacon frame ......." need clarification. Doesn't read correctly. | as commented | Rejected-The page number should be 509.29. The commenter failed to identify the technical issue. It is correct that the AP may include a Reconfiguration Multi-Link element in a Beacon frame. |

**Discussion:** None.

***TGbe Editor: please add the following paragraph***

**11.2.3.14 TIM Broadcast**

Insert the following paragraph after NOTE 4:

When the AP belongs to a multiple BSSID set and the critical update occurs for any of the reasons specified in m) and m1) and when the relevant TWT parameter set is a R-TWT parameter set, then this critical update shall also be (#22103)reported by the transmitted BSSID as a critical update for all the reported nontransmitted BSSID(s).