IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CIDs 7218 & 7219 | | | | |
| Date: 2024-04-09 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Dave Halasz | Morse Micro |  |  | dave.halasz@morsemicro.com |

Abstract

This document contains proposed text changes to address IEEE P802.11-REVme SB2 CIDs 7218, 7219, etc.

Revision History:

R0: Initial version.

Proposed Resolution:

* CID 7218 & 7219: Revised. Incorporate the changes shown as “Proposed change” in this document.

|  |  |  |  |
| --- | --- | --- | --- |
| CID | Clause | Comment | Proposed Change |
| 7218 | L | "Group Addressed Traffic Indicator field" -- no such field | Delete "Group Addressed " (16x) |

***Proposed resolution for CID 7218:***

In Annex L, change 8 instances of “Group Addressed Traffic Indicator field” to “Traffic Indicator field” and update figures L-8, L-9, L-10, L-11, L-12, L-13, L-14 & L-15 as follows.



Figure L-8—Partial Virtual Bitmap example #7 for S1G STAs, Block Bitmap mode



Figure L-9—Partial Virtual Bitmap example #8 for S1G STAs, Single AID mode



Figure L-10—Partial Virtual Bitmap example #9 for S1G STAs, OLB mode



Figure L-11—Partial Virtual Bitmap example #7 for S1G STAs, ADE mode(#6043)



Figure L-12—Partial Virtual Bitmap example #10 for S1G STAs, Inverse Bitmap + Block Bitmap mode



Figure L-13—Partial Virtual Bitmap example #11 for S1G STAs, Inverse Bitmap + Single AID mode



Figure L-14—Partial Virtual Bitmap example #12 for S1G STAs, Inverse Bitmap + OLB mode(#6045)



Figure L-15—Partial Virtual Bitmap example #10 for S1G STAs, Inverse Bitmap + ADE mode(#6046)

|  |  |  |  |
| --- | --- | --- | --- |
| CID | Clause | Comment | Proposed Change |
| 7219 | L | I also note that in some of the Annex L figures the Traffic Indicator field is described as Transmitted BSSID group addressed traffic indication/AID 0 and Nontransmitted BSSID group addressed traffic indication though some of the figures aren't searchable (grrr ) | Use consistent wording and make figures searchable |

***Note: NonTxBSS ID is from clause 9.4.2.5.1.***

***Proposed resolution for CID 7219, in Annex L, update figures L-4, L-5, L-6 & L-7 as follows:***



Figure L-4—Partial Virtual Bitmap example #4, Method A and Method B



Figure L-5—Partial Virtual Bitmap example #5, Method A or Method B



Figure L-6—Partial Virtual Bitmap example #6, Method A



Figure L-7—Partial Virtual Bitmap example #6, Method B

**References:**

