IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Correction to TGbe Fig 7-2 | | | | |
| Date: 2024-06-28 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Mark Hamilton | Ruckus/CommScope | 350 W Java Dr.  Sunnyvale, CA 94089 | +1-303-818-8472 | mark.hamilton2152@gmail.com |
|  |  |  |  |  |

Abstract

This contribution proposed a resolution to CID 23074 on P802.11be D6.0.


**Background:**

This document proposes a resolution to the following comment on P802.11be D6.0:


|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Subclause** | **Page** | **Line** | **Comment** | **Proposed Change** |
| 23074 | Michael Montemurro | 7.1 | 113 | 12 | [AK] A5:F22In Figure 7-2 (Example DS access fir an AP MLD with two affiliated APs), the upper MAC sublayer of the AP MLD is erroneously designated as "Non-MLD upper MAC sublayer".  Please correct the designation as suggested | The upper MAC sublayer of the AP MLD shall be designated as "MLD upper MAC sublayer" |

**Context:**

Figure 7-2 in 802.11be D6.0:



The corrected figure would be:



**Proposed Resolution:**

**Accepted.**