IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CR for CIDs on MLO | | | | |
| Date: June 19, 2024 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Giovanni Chisci | Qualcomm Technologies Inc. |  |  | gchisci@qti.qualcomm.com |

Abstract

This submission proposes resolutions for following CID received for TGbe recirculation SA ballot:

* 23030, 23087

**Revisions:**

* Rev 0: Initial version of the document.
* Rev 1: Minor edits to the CR for CID 23087.
* Rev 2: Minor edits to the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e., they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Clause** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 23030 | Joseph Levy | 35.3.3.3 | 521 | This sentence is unclear, difficult to parse, and therefore technically incorrect. Also, it does not matter why the element is being added, all that is necessary is to know where the additional element would be placed. | Change: "If an element is included in the STA profile field due to other conditions being satisfied in addition to the ones listed in the tables of 9.3.3 ((PV0) Management frames) as per the indicated rules above, then the element appears after all the applicable elements listed in the tables of 9.3.3 ((PV0) Management frames) for the reported STA. "  To:  "If an additional element, other than the ones listed in the tables of 9.3.3 ((PV0) Management frames), is included in the STA profile field the element shall follow all the applicable elements listed in the tables of 9.3.3 ((PV0) Management frames) for the reported STA." | **Revised**  Agree in principle. Amended with minor editorials, e.g., added a “comma”.  TGbe editor: please implement changes as shown in 11-24/1036r0 tagged 23030. |
| 23087 | Abhishek Patil | 35.3.3.3 | 520 | NOTE 1 in this subclause is incorrect. Even the Reconfig Multi-Link element can carry complete profile. | Replace "Only a Basic Multi-Link element can include a complete profile of a reported STA. Therefore, the" with "The" | **Accepted** |

*TGbe editor: the reference text is 11be Draft 6.0.*

35.3.3.3 Advertisement of complete or partial per-link information

*TGbe editor: please find below the changes related to CID 23087*

NOTE 1—The above definition of a complete profile applies only to a Basic Multi-Link element.

*TGbe editor: please find below the changes related to CID 23030*

* If an additional element is included in the STA profile field, other than the ones listed in the tables of 9.3.3 ((PV0) Management frames), then the element shall follow all the applicable elements listed in the tables of 9.3.3 ((PV0) Management frames) for the reported STA. When more than one such additional elements are included, they are ordered based on their Element ID and Element ID Extension (if present).