IEEE P802.11
Wireless LANs

|  |
| --- |
| Initial SA Ballot Comment Resolutions for Exchange CIDs |
| Date: 2024.07.16 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Zhuqing Tang | Huawei Technologies | F3, Huawei Base, Shenzhen, Guangdong, China, 518129 |  | tangzhuqing@huawei.com |
| Rui Du |  |  |  |
| Narengerile |  |  |  |
| Mengshi Hu |  |  |  |
| Yiyan Zhang |  |  |  |

Abstract

This submission contains the proposed comment resolutions for the CIDs  6007 6008 6169 submitted to Initial SA Ballot. The reference text is 11bf D4.0.

R0: initial document

R1: remove the resolution of CID 6018

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page****Line** | **Comment** | **Proposed Change** | **Resolution** |
| 6007 | 9.3.1.22.15.3 | 38.03 | I believe there is a normative requirement implied by this sentence which is not correctly stated. It seems this is specifying the format of a field WHEN the condition is met. | When the AID12/USID12 subfield is equal to 2008 the format of the User Info field in the SR2SI Sounding Trigger frame shall be as shown in Figure 9-103e (User Info field format for SR2SI/SR2SR Sounding Trigger frame if the AID12/USID12 subfield is equal to 2008). | RevisedAgree with the commenter in principle.TGbf Editor make changes specified in 1297r1. ([https://mentor.ieee.org/802.11/dcn/24/11-24-1297-01-00bf- Initial-SA-Ballot-Comment-Resolutions-for- Exchange-CIDs.docx](https://mentor.ieee.org/802.11/dcn/24/11-24-1297-01-00bf-%20Initial-SA-Ballot-Comment-Resolutions-for-%20Exchange-CIDs.docx)) |

**Discussion:**

The location that the commenter indicates:



There exists a normative requirement in the current spec, it has been put in a rearward position.

***Instructions to the editor: please make the following changes to the paragraph from P38L3 to P38L7 in the subclause 9.3.1.22 Trigger frame format in D4.0 as shown below:***

The format of the User Info field in the SR2SI Sounding Trigger frame if the AID12/USID12 subfield is equal to 2008 is defined in Figure 9-103e (User Info field format for SR2SI/SR2SR Sounding Trigger frame if the AID12/USID12 subfield is equal to 2008).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page****Line** | **Comment** | **Proposed Change** | **Resolution** |
| 6008 | 9.3.1.22.15.3 | 37.20 | I think that there is a normative requirement in this sentence somewhere which is not correctly stated. Perhaps this is meant to say that WHEN the AID12/USID12 subfield is not equal to 2008 the User Info Field in the SR2SI Sounding Trigger frame shall be formatted as defined in Figure 9-103d..??? | change to: When the AID12/USID12 subfield is not equal to 2008 the User Info Field in the SR2SI Sounding Trigger frame shall be formatted as defined in Figure 9-103d (the AID12/USID12 subfield is not equal to 2008 the User Info Field in the SR2SI Sounding Trigger frame shall be formatted as defined in Figure 9-103d). |  RevisedAgree with the commenter in principle.TGbf Editor make changes specified in 1297r1. ([https://mentor.ieee.org/802.11/dcn/24/11-24-1297-01-00bf- Initial-SA-Ballot-Comment-Resolutions-for- Exchange-CIDs.docx](https://mentor.ieee.org/802.11/dcn/24/11-24-1297-01-00bf-%20Initial-SA-Ballot-Comment-Resolutions-for-%20Exchange-CIDs.docx)) |

The location that the commenter indicates:



***Instructions to the editor: please make the following changes to the paragraph from P37L20 to P37L23 in the subclause 9.3.1.22 Trigger frame format in D4.0 as shown below:***

The format of the User Info field in the SR2SI Sounding Trigger frame if the AID12/USID12 subfield is not equal to 2008 is defined in Figure 9-103d (User Info field format for SR2SI Sounding Trigger frame if the AID12/USID12 subfield is not equal to 2008).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page****Line** | **Comment** | **Proposed Change** | **Resolution** |
| 6169 | 11.55.1.5.2.5 | 156.44 | In "When transmitting an SR2SI Sounding Trigger frame" - "SR2SI" should be "SR2SR" in this subclause. | As in the comment | Accepted |

**Discussion:**

Taken from 11bf



## SP

Do you support the proposed resolutions to the CIDs 6007 6008 6169 and incorporate the text changes into the latest TGbf draft?

Y/N/A