IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 11bi D0.4 CR for CID 1146 | | | | |
| Date: 2024-10-28 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Po-Kai Huang | Intel |  |  | po-kai.huang@intel.com |

Abstract

This submission proposes resolutions for the following CIDs:

1146

Revisions:

* Rev 0: Initial version of the document.
* Rev 1: Revision based on the discussion during the teleconference
* Rev 2: Revision based on the discussion during the teleconference

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbi D0.6 Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbi D0.6 Draft. (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents). TGbi Editor: Editing instructions preceded by “TGbi Editor” are instructions to the TGbi editor to modify existing material in the TGbi draft. As a result of adopting the changes, the TGbi editor will execute the instructions rather than copy them to the TGbi Draft.***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Clause** | **P.L** | **Comment** | **Proposed Change** | **Resolution** |
| 1146 | Po-Kai Huang | 12.2.10 | 0.00 | Several statements in 12.2.10 needs to be tweaked to allow MAC address change during reassociation. Suggested change as proposed in 11-23-1664r1 | As in comment | Revised –  Agree in principle with the commenter. We follow the principle of 11ax and 11be to add introduction in 12.14 to describe exception with 12.2.10.  TGbi editor to make the changes shown in 11-24/1727r2 under all headings that include CID 1146 |

**Discussion:**

None

**Proposal: (#1146)**

**TGbi Editor: *Instruction: Add 12.14.1 Introduction as shown below***

**12.14 Client Privacy Enhancement**

**12.14.1 Introduction**

When dot11MACPrivacyActivated is true, an EDP STA or an EDP MLD has a MAC that comprises the functions defined in 12.2.11 (Requirements for support of MAC privacy enhancements) except when the functions in Clause 12.14 (Client Privacy Enhancement) supersede the functions in 12.2.11 (Requirements for support of MAC privacy enhancements).