IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| AP termination frame to unassociated non-AP STA in NTB | | | | |
| Date: 2024-11-12 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Ali Raissinia | Qualcomm Inc. |  |  | [alirezar@qti.qualcomm.com](mailto:alirezar@qti.qualcomm.com) |
|  |  |  |  |  |

Abstract

Missing normative text for AP (as a sensing responder) to transmit an explicit termination frame to an unassociated non-AP STA (as a sensing initiator).

TGBF editor, add the text below under clause 11.55.1.6 (Sensing measurement session termination) in P165L5.

During the non-TB sensing measurement exchange, an AP as a sensing responder shall only transmit a Sensing Measurement Termination frame to an unassociated non-AP STA as a sensing initiator either in an A-MPDU aggregated with the Sensing Measurement Report frame if required, or as an S-MPDU frame SIFS after SR2SI NDP.

**References: References: P802.11bfD5.0, P802.11REVmeD7.0 and P802.11bkD3.0.**