IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Tentative Table of Contents for TGbn D0.1 | | | | |
| Date: 2024-12-02 | | | | |
| Author: | | | | |
| Name | Affiliation | Address | Phone | Email |
| Ross Jian Yu | Huawei Technologies |  |  | ross.yujian@huawei.com |

##### This submission presents a tentative table of contents for TGbn D0.1.

R0: initial version

R1: added 38.3.15.5 Segment deparser, 38.3.15.6 Frequency domain duplication, 38.3.19 Transmit requirements for an UHR ELR PPDU

1 Contents

2

3 [Contents 7](#_bookmark0)

4

5

6 Figures 13

7

8 Tables 15

9

10

11 Editorial Notes 17

12

13 3. Definitions, acronyms, and abbreviations 19

14

15 3.1 Definitions 19

16

17 3.4 Abbreviations and acronyms 19

18

19 4. General description 21

20

21 4.3 Components of the IEEE Std 802.11 architecture 21

22

1. 4.3.15bUltra high reliability (UHR) STA 21

24

25 6. Layer management 23

26

27 6.3 MLME SAP interface 23

28

1. 6.3.7 Associate 23
2. 6.3.7.3 MLME-ASSOCIATE.confirm 23
3. 6.3.7.3.2Semantics of the service primitive 23
4. 6.3.7.5 MLME-ASSOCIATE.response 23
5. 6.3.7.5.2Semantics of the service primitive 23

34

1. 6.3.8 Reassociate 23
2. 6.3.8.3 MLME-REASSOCIATE.confirm 23
3. 6.3.8.3.2Semantics of the service primitive 23
4. 6.3.8.5 MLME-REASSOCIATE.response 23
5. 6.3.8.5.2Semantics of the service primitive 23

40

1. 6.5 PLME SAP interface 23

42

43 9. Frame formats 25

44

45 9.2 MAC frame formats 25

46

1. 9.3 Format of individual frame types 25
2. 9.3.1 Control frames 25
3. 9.3.1.19 NDP Announcement frame format 25
4. 9.3.1.22 Trigger frame format 25

51 9.3.1.22.1General 25

52

1. 9.3.1.22.2Common Info field 25
2. 9.3.1.22.3Special User Info field 25
3. 9.3.1.22.5aUHR variant User Info field 25
4. 9.3.1.22.10BSRP Trigger frame format 25
5. 9.3.3 (PV0) Management frames 25

58

1. 9.3.3.2 Beacon frame format 25
2. 9.3.3.5 Association Request frame format 25
3. 9.3.3.6 Association Response frame format 26
4. 9.3.3.7 Reassociation Request frame format 26
5. 9.3.3.8 Reassociation Response frame format 26

64

65 9.3.3.9 Probe Request frame format 26

1. 9.3.3.10 Probe Response frame format 26
2. 9.3.3.aaaUHR Action frame details 26
3. 9.3.3.aabProtected UHR Action frame details 26
4. 9.4 Management and Extension frame body components 26

5

1. 9.4.1 Fields that are not elements 26
2. 9.4.1.aaa UHR MIMO Control field 26
3. 9.4.1.aab UHR Compressed Beamforming Report field 26
4. 9.4.1.aac UHR MU Exclusive Beamforming Report field 26
5. 9.4.2 Elements 26

11

1. 9.4.2.aaa UHR Operation Element 26
2. 9.4.2.aab UHR Capabilities 27
3. 9.4.2.aab.1UHR PHY Capabilities Information field 27
4. 9.4.2.aab.2UHR MAC Capabilities Information field 27
5. 9.6 Action frame format details 27

17

1. 9.7 Aggregate MPDU (A-MPDU) 27
2. 9.7.3 A-MPDU contents 27

20

21 10. MAC sublayer functional description 29

22

23

1. 10.2 MAC architecture 29
2. 10.2.7 MAC data service 29
3. 10.25Block acknowledgment (block ack) 29

27 10.25.2 29

28

29

30 11. MLME 31

31

32 11.1 Synchronization 31

33 11.1.3 Maintaining synchronization 31

34 11.1.4 31

35

36

37 12. Security 33

38

39 37. Ultra high reliability (UHR) MAC specification 35

40

41

1. 37.1 Introduction 35
2. 37.2 Enhanced channel access 35
3. 37.3 UHR BSS operation 35
4. 37.4 Buffer status report 35
5. 37.5 Nominal packet padding values selection rules 35

47

1. 37.6 UHR sounding operation 35

49 37.6.1 General 35

50 37.6.2 35

1. 37.6.2.1 35
2. 37.7 Multi-AP coordination framework 35

53

54 37.8 Coordinated beamforming 35

55 37.9 Coordinated spatial reuse 35

1. 37.10Coordinated time division multiple access 36
2. 37.11Coordinated R-TWT 36
3. 37.12Roaming 36

65

1. 37.13Power save 36
2. 37.14Non-primary channel access 36
3. 37.15In-device coexistence 36
4. 37.16TWT SP management 36

5

6

7 38. Ultra high reliability (UHR) PHY specification 37

8

1. 38.1 Introduction 37
2. 38.1.1 Introduction to the UHR PHY 37

11

12 38.1.2 Scope 37

13 38.1.3 UHR PHY functions 37

14 38.1.3.1 General 37

15 38.1.3.2 PHY management entity (PLME) 37

16 38.1.3.3 Service specification method 37

17

1. 38.1.4 PPDU formats 37
2. 38.2 UHR PHY service interface 38
3. 38.2.1 Introduction 38
4. 38.2.2 TXVECTOR and RXVECTOR parameters 38
5. 38.2.3 TRIGVECTOR parameters 38

23

1. 38.2.4 PHY CONFIG\_VECTOR 38
2. 38.2.5 Effect of CH\_BANDWIDTH parameter on PPDU format 38
3. 38.2.6 Support for non-HT, HT, VHT, and HE formats 38

27 38.2.6.1 General 38

28 38.2.6.2 Support for non-HT format 38

29

1. 38.2.6.3 Support for HT format 38
2. 38.2.6.4 Support for VHT format 38
3. 38.2.6.5 Support for HE format 38
4. 38.2.6.6 Support for EHT format 38
5. 38.3 UHR PHY 39

35

1. 38.3.1 Introduction 39
2. 38.3.2 Subcarrier and resource allocation 39

38 38.3.2.1 39

1. 38.3.3 Transmission of DRU 39
2. 38.3.4 Interference mitigation 39

41

1. 38.3.5 LDPC encoding 39
2. 38.3.6 UHR PPDU formats 39
3. 38.3.7 Transmitter block diagram 39
4. 38.3.8 Enhanced long range PPDU 39
5. 38.3.9 Overview of the PPDU encoding process 39

47

48 38.3.9.1 General 39

1. 38.3.9.2 Construction of L-STF 39
2. 38.3.9.3 Construction of L-LTF 39
3. 38.3.9.4 Construction of L-SIG 39
4. 38.3.9.5 Construction of RL-SIG 40

53

1. 38.3.9.6 Construction of U-SIG 40
2. 38.3.9.7 Construction of UHR ELR-MARK 40
3. 38.3.9.8 Construction of UHR-SIG 40
4. 38.3.9.9 Construction of UHR-STF 40
5. 38.3.9.10 Construction of UHR-LTF 40

59

1. 38.3.9.11 Construction of ELR-SIG 40
2. 38.3.9.12 Construction of Data field in a UHR PPDU 40
3. 38.3.9.12.1non-ELR PPDU 40
4. 38.3.9.12.2ELR PPDU 40
5. 38.3.10UHR modulation and coding schemes (UHR-MCSs) and Unequal modulation (UEQM)

65

|  |  |  |
| --- | --- | --- |
| 1 | 40 |  |
| 2  3  4  5 |  | * + 1. UHR-SIG modulation and coding schemes (UHR-SIG-MCSs) 40     2. Timing-related parameters 40     3. Mathematical description of signals 40 |
| 6 |  | 38.3.13.1 Notation 41 |
| 7 |  | 38.3.13.2 Subcarrier indices in use 41 |
| 8  9  10  11 |  | 38.3.13.3 Channel frequencies 41  38.3.13.4 Transmitted signal 41  38.3.14UHR preamble 41 |
| 12 |  | 38.3.14.1 Introduction 41 |
| 13 |  | 38.3.14.2 Cyclic shift 41 |
| 14  15  16  17 |  | * + - * 1. Cyclic shift for pre-UHR modulated fields 41         2. Cyclic shift for UHR modulated fields 41   38.3.14.3 L-STF 41 |
| 18 |  | 38.3.14.4 L-LTF 41 |
| 19 |  | 38.3.14.5 L-SIG 41 |
| 20  21  22  23 |  | * + - 1. RL-SIG 41       2. U-SIG 42          1. General 42 |
| 24 |  | 38.3.14.7.2Content 42 |
| 25 |  | 38.3.14.7.3Encoding and modulation 42 |
| 26  27  28  29 |  | * + - 1. Enhanced Long Range (ELR) MARK field 42          1. ELR-MARK Matrix 42          2. Encoding and Modulation 42 |
| 30 |  | 38.3.14.9 UHR-SIG 42 |
| 31 |  | 38.3.14.9.1General 42 |
| 32  33  34  35 |  | * + - * 1. UHR-SIG content channels 42         2. Common field for OFDMA transmission 43         3. Common field for non-OFDMA transmission 43 |
| 36 |  | 38.3.14.9.5Common field for Co-BF transmission 43 |
| 37 |  | 38.3.14.9.6User Specific field 43 |
| 38  39  40  41 |  | 38.3.14.9.7Encoding and modulation 43   * + - 1. UHR-STF 43          1. UHR-STF for DRUs 43 |
| 42 |  | 38.3.14.10.2Global CSD for DRU transmission 43 |
| 43 |  | 38.3.14.10.3Global CSD index assignment for DRU STF transmission 43 |
| 44  45  46  47 |  | * + - 1. UHR-LTF 43          1. UHR-LTF for DRUs 43       2. ELR-SIG 44 |
| 48 |  | 38.3.14.12.1General 44 |
| 49 |  | 38.3.14.12.2Content 44 |
| 50  51  52  53 |  | 38.3.14.12.3Encoding and modulation 44   * + 1. Data field 44        1. Coding 44 |
| 54 |  | 38.3.15.1.1General 44 |
| 55 |  | 38.3.15.1.2BCC coding 44 |
| 56  57  58  59 |  | * + - * 1. LDPC coding 44         2. UHR PPDU padding process 44         3. Encoding process for an UHR MU PPDU 44 |
| 60 |  | 38.3.15.1.6Encoding process for an UHR TB PPDU 44 |
| 61 |  | 38.3.15.1.7Encoding process for an UHR ELR PPDU 44 |
| 62  63  64  65 |  | * + - 1. Segment parser 44       2. BCC interleavers 45       3. LDPC tone mapper 45 |

1 38.3.15.5 Segment deparser 45

2 38.3.15.6 Frequency domain duplication 45

3 38.3.15.7 Pilot subcarriers 45

4 38.3.15.8 OFDM modulation 45

5

1. 38.3.16Packet extension 45
2. 38.3.17Non-HT duplicate transmission 45
3. 38.3.18Transmit requirements for PPDUs sent in response to a triggering frame 45
4. 38.3.19Transmit requirements for an UHR ELR PPDU 45
5. 38.3.20Beamforming 45

11

12 38.3.20.1 General 45

13 38.3.20.2 UHR beamforming feedback matrix V 45

14 38.3.20.3 UHR CQI feedback 46

15 38.3.21Sounding NDP for UHR 46

16 38.3.22Transmit specification 46

17

18 38.3.22.1 Transmit spectral mask 46

19 38.3.22.1.1General 46

20 38.3.22.2 Spectral flatness 46

21 38.3.22.3 Transmit center frequency and symbol clock frequency tolerance 46

22 38.3.22.4 Modulation accuracy 46

23

1. 38.3.22.4.1Introduction to modulation accuracy tests 46
2. 38.3.22.4.2Transmit center frequency leakage 46
3. 38.3.22.4.3Transmitter modulation accuracy (EVM) test 46
4. 38.3.23Receiver specification 46

28 38.3.23.1 General 46

29

1. 38.3.23.2 Receiver minimum input sensitivity 46
2. 38.3.23.3 Adjacent channel rejection 47
3. 38.3.23.4 Nonadjacent channel rejection 47
4. 38.3.23.5 Receiver maximum input level 47
5. 38.3.24UHR transmit procedure 47

35

1. 38.3.25UHR receive procedure 47
2. 38.3.26Channel numbering 47
3. 38.3.27Regulatory requirements 47
4. 38.4 UHR PLME 47
5. 38.4.1 PLME\_SAP sublayer management primitives 47

41

42 38.4.2 PHY MIB 47

1. 38.4.3 TXTIME and PSDU\_LENGTH calculation 47
2. 38.4.4 UHR PHY 48
3. 38.5 Parameters for UHR-MCSs 48

46

47

48 Annex B 49

49

1. B.4 PICS proforma—IEEE Std 802.11-<year> 49
2. B.4.3 IUT configuration 49
3. B.4.37a Ultra High Reliability (UHR) features 49

53

1. B.4.37a.1UHR MAC features 49
2. B.4.37a.2UHR PHY features 49

56

57 Annex C 51

58

59

60 C.3 MIB Detail 51

61

62 Annex E 53

63

64 E.1 Country information and operating classes 53

65

1 Annex AA 55

2

3 AA.1 Introduction 55