IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 11bi D1.0 12.16.4 comments | | | | |
| Date: 2025-03-25 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Po-Kai Huang | Intel |  |  | po-kai.huang@intel.com |

Abstract

This submission resolves the following CIDs:

174

Revisions:

* Rev 0: Initial version of the document.
* Rev 1: Revision based on the discussion offline and during the meeting
* Rev 2: Revision based on 174
* Rev 3: Revision based on the discussion during the teleconference call

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbi D1.0 Draft. This introduction is not part of the adopted material.

Editing instructions formatted like this are intended to be copied into the TGbi D1.0 Draft. (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents). TGbi Editor: Editing instructions preceded by “TGbi Editor” are instructions to the TGbi editor to modify existing material in the TGbi draft. As a result of adopting the changes, the TGbi editor will execute the instructions rather than copy them to the TGbi Draft.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **P.L** | **Comment** | **Proposed Change** | **Resolution** |
| 174 | 12.16.4 | 121.12 | Will be useful to define inheritance rules based on the first per-STA profile to reduce overhead. | As in comment | Revised –  Agree in principle with the commenter.  TGbi editor to make the changes shown in the latest version of 11-25/0532 under all headings that include CID 174 |

***Discussion:***

***Proposal:***

**TGbi Editor: *Instruction: Modify 12.16.4 as follows***

* Capabilities and operation parameters request and response procedure(#159)
* MLO

For MLO, all STAs affiliated with an MLD shall set the EDP Capabilities And Operation Parameters Request/Response Support field in the RSNXE to the same value.(#765)

A non-AP STA affiliated with a non-AP MLD that sets the EDP Capabilities And Operation Parameters Request/Response Support field in the RSNXE to 1 may send an EDP Capabilities And Operation Parameters Request frame with a Basic Multi-Link element to request capabilities and operation parameters of APs affiliated with an associated AP MLD if APs affiliated with the associated AP MLD set the EDP Capabilities And Operation Parameters Request/Response Support field in the RSNXE to 1.

If APs affiliated with an AP MLD set the EDP Capabilities And Operation Parameters Request/Response Support field in the RSNXE to 1 and the AP MLD receives through a setup link from an associated non-AP MLD an individually addressed(#262) EDP Capabilities And Operation Parameters Request frame with a Basic Multi-Link element, then the AP MLD shall respond with an individually addressed(#262) EDP Capabilities And Operation Parameters Response frame through an affiliated AP over a setup link to the non-AP MLD.

If APs affiliated with an AP MLD set the EDP Capabilities And Operation Parameters Request/Response Support field in the RSNXE to 1, the AP MLD may send an unsolicited individually addressed(#262) EDP Capabilities And Operation Parameters Response frame to an associated non-AP MLD through a setup link, where non-AP STAs affiliated with the non-AP MLD set the EDP Capabilities And Operation Parameters Request/Response Support field in the RSNXE to 1. If BPE APs affiliated with a BPE AP MLD set the EDP Capabilities And Operation Parameters Request/Response Support field in the RSNXE to 1, a BPE AP affiliated with the BPE AP MLD may send an unsolicited broadcast addressed EDP Capabilities And Operation Parameters Response frame if there exists at least one BPE non-AP STA affiliated with an associated BPE non-AP MLD corresponding to the setup link that sets the EDP Capabilities And Operation Parameters Request/Response Support field in the RSNXE to 1.(#262)

The unsolicited(#264) EDP Capabilities And Operation Parameters Response frame shall include a Basic Multi-Link element, and the Basic Multi-Link element shall include a Per-STA Profile subelement with the Complete Profile subfield set to 1 for each AP affiliated with the AP MLD (see 9.4.2.321.2.4 (Link Info field of the Basic Multi-Link element)). The individually addressed EDP Capabilities And Operation Parameters Response frame sent in response to an EDP Capabilities And Operation Parameters Request frame shall include a Basic Multi-Link element, and the Basic Multi-Link element shall include a Per-STA Profile subelement with the Complete Profile subfield set to 1 for each requested AP affiliated with the associated AP MLD (see 9.4.2.321.2.4 (Link Info field of the Basic Multi-Link element)). If the Basic Multi-Link element in the EDP Capabilities And Operation Parameters Request frame does not include any per-STA profiles, then all APs affiliated with the associated AP MLD shall be the requested APs. If the Basic Multi-Link element in the EDP Capabilities And Operation Parameters Request frame includes one or more per-STA profiles, then only APs affiliated with the associated AP MLD and whose link ID is equal to the value in the Link ID field in a per-STA profile in the Basic Multi-Link element in the EDP Capabilities And Operation Parameters Request frame shall be the requested APs.(#264) The STA profile field in the Per-STA Profile subelement for each AP affiliated with the AP MLD shall include(#174) the following in order and does not follow 35.3.3.3 (Advertisement of complete or partial per-link information):

* The Capability Information field as defined in 9.4.1.4 (Capability Information field).

All elements that are not inherited(#174) and would be included in a Probe Response frame except the Multi-Link element and the Multiple BSSID element, and the elements shall be in the order defined for a Probe Response frame.(#672, #673, #674) Except for the Vendor Specific element, if an element, identified by an Element ID and Element ID Extension (if applicable), is carried in the first per STA profile subelement in the Basic Multi-Link element of the EDP Capabilities And Operation Parameters Response frame and there is no element having the same Element ID and Element ID Extension (if applicable) in a complete profile of a following per STA profile subelement in the same Basic Multi-Link element, then the element is inherited and is considered to be part of the following per STA profile subelement and the value of the element to use in the following per STA profile subelement is the same as that of the corresponding element carried in the first per STA profile subelement unless the following per STA profile subelement carries the Non-Inheritance element (see 9.4.2.239 (Non-Inheritance element)) and the element is listed in the Non-Inheritance element.(#174)

The Vendor Specific element shall not be inherited in any per STA profile subelement in the Basic Multi-Link element of the EDP Capabilities And Operation Parameters Response frame.