IEEE P802.11
Wireless LANs

|  |
| --- |
| TGbp Spec Text Topics and Volunteers |
| Date: 2025-04-07 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Yinan Qi | OPPO |  |  | v-qiyinan@oppo.com |
| Bo Sun | Sanechips |  |  | Sun.bo1@sanechips.com.cn |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This document contains a table with the spec text topics and volunteers for TGbp draft.

Revisions:

* Rev 0: Initial version of the document.
* Rev 1: Revised version based on the comments from task group members.
* Rev 2: Revised version based on the comments from task group members and updated SFD.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **SFD Topic** | **Sub-clause** | **POC** | **TTT** | **Status** | **Notes** |
| **General** |
| Components of architecture | 4.3.35 |  |  |  | Motion 22, 29, 34 |
| Communication mode | 1.3 |  |  |  | Motion 7, 14, 15, 73 |
|  | 6 |  |  |  | Layer management (void) |
| **PHY** |
| Clock accuracy | 40.3.6 |  |  |  | Motion 20, 72 |
| DL PPDU format | 40.3.2.1 |  |  |  | Motion 8 |
| DL non-AMP portion preamble | 40.3.8.1, 40.3.8.2.1 |  |  |  | Motion 28 |
| DL waveform generation | 40.3.3.1 |  |  |  | Motion 30, 39, 70, 71 |
| DL synchronisation field | 40.3.8.1, 40.3.8.2.2 |  |  |  | Motion 18, 33, 69, 76 |
| DL modulation and coding | 40.3.5, 40.3.9, 40.5 |  |  |  | Motion 9, 10, 16, 37, 40, 41, 77 |
| UL PPDU format | 40.3.2.2 |  |  |  | Motion 11, 42 |
| UL synchronisation field | 40.3.8.2 |  |  |  |  |
| UL modulation and coding | 40.3.5, 40.3.9, 40.5 |  |  |  | Motion 19, 21, 31, 38, 43, 78 |
| UL carrier center frequency | 40.3.10 |  |  |  | Motion 27 |
|  | 40.1 |  |  |  | AMP PHY introduction |
| **MAC** |
| AMP TSF | 39.2 |  |  |  | Motion 13, 82 |
| Time-slot based UL access mechanism | 39.3 |  |  |  | Motion 24, 45, 50, 51, 56 |
| AMP triggering procedure | 9.10.2, 39.4 |  |  |  | Motion 46, 47, 48 |
| Duty-cycle operation | 39.5 |  |  |  | Motion 32, 75 |
| Secure communication-general | 12.2 |  |  |  | Motion 26, 44, 68 |
| Secure communication-key generation | 11.3, 12.2, 12.7 |  |  |  | Motion 61, 62, 64, 65 |
| Secure communication-secured data communication | 12.2, 12.7 |  |  |  | Motion 66, 67 |
| Support of UHF RFID logic interface | 39.6 |  |  |  | Motion 52 |
| PM for AMP enabled non-AP STA | 11.2, 39.8 |  |  |  | Motion 58, 59, 60, 63 |
| Frame format-general | 9.10 |  |  |  | Motion 23 |
| Frame format-Ack frame format | 9.10.1 |  |  |  | Motion 49 |
| Frame format-AMP trigger frame format | 9.10.2, 39.4 |  |  |  | Motion 46, 48, 56 |
| Frame format-AMP wake-up frame format | 9.10.3 |  |  |  | Motion 57 |
| WPT Energizer control | 39.7.2 |  |  |  | Motion 35, 53, 55, 74, 81 |
| WPT AMP non-AP STA reporting | 39.7.1 |  |  |  | Motion 36 |
| WPT signal co-existence | 39.7.3 |  |  |  | Motion 54, 80 |
|  | 39.1 |  |  |  | AMP MAC introduction |
|  | 10 |  |  |  | MAC sublayer functional description (void) |