**IEEE P802.11
Wireless LANs**

|  |
| --- |
| CC50 CR for miscellaneous CIDs |
| **Date**: July. 8, 2025.  |
| **Author(s):** |
| **Name** | **Affiliation** | **Address** | **Phone** | **email** |
| Yan Li | ZTE |  |  | li.yan16@zte.com.cn |
| Jay Yang |  |  | yang.zhijie@zte.com.cn |
| Zisheng Wang |  |  | wang.zisheng@zte.com.cn |

 **Abstract**

This submission proposes resolutions for following CIDs received for TGbn CC50:

3319, 3320, 3321, 2938, 3156 (5 CIDs)

**Revisions:**

Rev 0: Initial version of the document

Rev 1: add CR for CID 2938 and 3156

Rev 2: change the resolution for CID 2938 base on suggestion from Brian

***TGbn editor: The baseline for this document is P802.11bn D0.3 and P802.11-2024***

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbn Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbn Draft (i.e., they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbn Editor: Editing instructions preceded by “TGbn Editor” are instructions to the TGbn editor to modify existing material in the TGbn draft. As a result of adopting the changes, the TGbn editor will execute the instructions rather than copy them to the TGbn Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Pg/Ln** | **Comment** | **Proposed Change** | **Resolution** |
| 3319 | 3.2 | 22.01 | In the definition of Co-TDMA, the word "procedure" is not appropriate. | Replace "procedure" with "Multi-AP coordination scheme." | Accepted. |
| 3320 | 3.2 | 22.19 | In the definition of Polled AP, the word "operation" is not appropriate. | Replace the word "operation" with "scheme." | Accepted. |
| 3321 | 6.4 | 26.17 | Typo in Table 6-1 in citing the number of the Subclause | Replace "337.8" with "37.8". | Revised.The typo has been resolved in 11bn D0.3. No further change is needed. |
| 2938 | C.3 | 362.4 | "dot11UHROptionImplemented" -- shouldn't that be ...Activated? | As it says in the comment | Revised.The UHR capability is unchanged during the lifetime of instance of the STA. According to the guidance in 11-18/52r2 and 11-15/355r13, such static capability should use “xxximplemented” instead of “xxxactivated”TGbn editor, please make the changes tagged by CID #2938 in 25/1115r2. |
| 3156 | 3.2 | 22.06 | The TXOP is a time domain concept, so it is redundent to say a time potion of obtained TXOP. | "a time portion of" --> "a portion of" | Accepted. |

**Introduction：**

Editorial changes to definition of Co-TDMA and Polled AP.

Please notice the definition of Co-TDMA is cited from 25/638r7, which has passed motion(#444), while the definition of polled AP is based on 11bn D0.3

**Proposed Texts**

**3. Definitions, acronyms, and abbreviations**

**3.2 Definitions specific to IEEE 802.11**

*TGbn editor: please change the text below as follows:*

**coordinated time division multiple access (TDMA)**: [Co-TDMA] A multi-AP coordination (#3319)scheme that enables an AP that has obtained a TXOP to share a (#3156) portion of the obtained TXOP with a set of coordinated APs.

**polled access point (AP)**: [polled AP] An AP polled by a sharing AP in the ICF that is transmitted as part of a multi-AP (#3320)coordination scheme.

**Annex C**

**C.3 MIB Detail**

*TGbn editor: please change the text below as follows:*

dot11UHROptionImplemented OBJECT-TYPE

SYNTAX TruthValue

MAX-ACCESS read-only

STATUS current

DESCRIPTION

"This is a capability variable.

Its value is determined by device capabilities.

This attribute indicates whether the (#2938)instance of implementation is UHR-capable."

::= { dot11StationConfigEntry ANA }