IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| TGbi Comments – LB288-Misc. | | | | |
| Date: 2025-07-08 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Carol Ansley | Cox Communications |  |  | carol@ansley.com |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

**Abstract**

This document covers comments: 369, 735, 736, 876, 902.

Similarly,

The Measurement ID subelement is optionally included in a Beacon request to request that the responding STA to include a Measurement ID element in the Probe Request frames it transmits.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 876 | Carol ANSLEY |  | “The current AID element text does not allow for AID changes during association. This text is in the baseline, but needs to be updated for EDP.” | Update the AID element text in section 9 to accommodate the EDP AID changes. | Revised.  Editor, please update the text shown in document 25/116r0 marked with tag #876. |
| 735 | Mark RISON | 139.43 | "Station Configuration attributes" bad case and not specific enough | Change to "EDP station configuration attributes" | Accept. |
| 736 | Mark RISON | 139.53 | This DESCRIPTION seems both too detailed and too generic | Align with other StationConfigEntrys | Revised.  Editor, please update the DESCRIPTION as shown in document 25/116r0 marked with tag #736. |
| 902 | Robert Stacey | 1.35 | The terminology -- specifically the term "data" -- as used in this amendment is misleading. The first sentence in 4.5.4.10a highlights this: "Third parties observing the wireless medium may seek to track device locations and device activity." It's not about data. | I recommend we change the title to "Enhanced Service with Privacy Protection". This will require a PAR change -- a slow process, but not very time consuming (TG approval, WG approval, 802 approval, NesCom approval). Specific to the draft itself. Replace the term "Enhanced Data Protection" and its acronym "EDP" with "Enhanced Privacy Protection (EPP)" | Propose accept but would like discussion. |
| 369 | Mark RISON | 1.35 | "Enhanced Service with Data Privacy Protection" is a poor name since it's more than just data privacy, it's user privacy | Delete "Data " | Propose accept but would like discussion. |

***Change the text as follows:***

9.4.1.8 AID field

In infrastructure BSS operation, the AID field contains a value assigned by an AP or PCP ~~during association~~. The field represents the 16-bit IS of a STA.[#876]

9.4.2.162 AID Element

The AID element contains the AID assigned by the AP ~~during association~~. The format of the AID element is shown in Figure 9-717 (AID element format).[#876]

***Change the dot11EDPStationConfigEntry Description as follows:***

An entry in the dot11EDPStationConfigTable. The entries address configuration options for EDP operation~~. It is possible for there to be multiple IEEE 802.11 interfaces on one agent, each with its unique MAC address. The relationship between an IEEE 802.11 interface and an interface in the context of the Internet-standard MIB is one-to-one. As such, the value of an ifIndex object instance can be directly used to identify corresponding instances of the objects defined herein. ifIndex - Each IEEE 802.11 interface is represented by an ifEntry.~~ [#736]