IEEE P802.11
Wireless LANs

|  |
| --- |
| Proposed resolution for REVmf LB289 comments - Part 3 |
| Date: 2025-10-06 |
| Author: |
| Name | Affiliation | Address | Phone | Email |
| Edward Au | Huawei | Ottawa, ON, Canada |  | edward.ks.au@gmail.com  |

##### This submission present proposed resolutions to the following CIDs: 387, 388, 507.

##### The proposed changes are based on REVmf D1.0.

##### Revision history:

##### R0 – initial version

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Comment | Proposed Change |
| 387 |  |  |  | "optionally present if" doesn't always have some kind of "otherwise not present" afterwards. One example is "The parameter is optionally present if dot11DMGOptionImplemented is true." but sadly there are 500 other hits for "optionally present if" | As it says in the comment |

***Discussion:***

There are 526 instances of “optionally present if” and all are in Clause 6, Clause 9, and Clause 10. While the commenter is correct that some kind of “otherwise not present” should be added, the followings are exceptions that need to restructure the sentence without simply adding “otherwise, not present”:

P834.28:

Change from “The BSS Average Access Delay element is present if dot11RMBSSAverageAccessDelayActivated is true and the AP Average Access Delay field is not equal to 255 (measurement not available); otherwise, the BSS Average Access Delay element is optionally present if dot11RMBSSAverageAccessDelayActivated is true.”

to “The BSS Average Access Delay element is present if dot11RMBSSAverageAccessDelayActivated is true and the AP Average Access Delay field is not equal to 255 (measurement not available) and is optionally present if dot11RMBSSAverageAccessDelayActivated is true. Otherwise, not present”.

P834.33:

Change from “The Antenna element is present if dot11RMAntennaInformationActivated is true and the Antenna ID field is not equal to 0 (unknown antenna); otherwise, the Antenna element is optionally present if dot11RMAntennaInformationActivated is true.”

to “The Antenna element is present if dot11RMAntennaInformationActivated is true and the Antenna ID field is not equal to 0 (unknown antenna) and is optionally present if dot11RMAntennaInformationActivated is true. Otherwise, not present.”

P834.46:

Change from “The BSS AC Access Delay element is present if dot11RMBSSAverageAccessDelayActivated is true and at least one field of the element is not equal to 255 (measurement not available); otherwise, the BSS AC Access Delay element is optionally present if dot11RMBSSAverageAccessDelayActivated is true.”

to “The BSS AC Access Delay element is present if dot11RMBSSAverageAccessDelayActivated is true and at least one field of the element is not equal to 255 (measurement not available) and is optionally present if dot11RMBSSAverageAccessDelayActivated is true. Otherwise, not present”

P835.16:

Change from “The Supported Operating Classes element is present if dot11ExtendedChannelSwitchActivated or dot11OperatingClassesRequired is true. The Supported Operating Classes element is optionally present if dot11TVHTOptionImplemented is true.”

to “The Supported Operating Classes element is present if dot11ExtendedChannelSwitchActivated or dot11OperatingClassesRequired is true and is optionally present if dot11TVHTOptionImplemented is true. Otherwise, not present.”

***Proposed resolution:***

Revised

Review each of the 526 instances of “optionally present if”. For those instances that do not have some kind of “otherwise not present” following except P834.28, P834.33, P834.46, and P835.16, append the following: “Otherwise, not present”.

P834.28:

Change from “The BSS Average Access Delay element is present if dot11RMBSSAverageAccessDelayActivated is true and the AP Average Access Delay field is not equal to 255 (measurement not available); otherwise, the BSS Average Access Delay element is optionally present if dot11RMBSSAverageAccessDelayActivated is true.”

to “The BSS Average Access Delay element is present if dot11RMBSSAverageAccessDelayActivated is true and the AP Average Access Delay field is not equal to 255 (measurement not available) and is optionally present if dot11RMBSSAverageAccessDelayActivated is true. Otherwise, not present”.

P834.33:

Change from “The Antenna element is present if dot11RMAntennaInformationActivated is true and the Antenna ID field is not equal to 0 (unknown antenna); otherwise, the Antenna element is optionally present if dot11RMAntennaInformationActivated is true.”

to “The Antenna element is present if dot11RMAntennaInformationActivated is true and the Antenna ID field is not equal to 0 (unknown antenna) and is optionally present if dot11RMAntennaInformationActivated is true. Otherwise, not present.”

P834.46:

Change from “The BSS AC Access Delay element is present if dot11RMBSSAverageAccessDelayActivated is true and at least one field of the element is not equal to 255 (measurement not available); otherwise, the BSS AC Access Delay element is optionally present if dot11RMBSSAverageAccessDelayActivated is true.”

to “The BSS AC Access Delay element is present if dot11RMBSSAverageAccessDelayActivated is true and at least one field of the element is not equal to 255 (measurement not available) and is optionally present if dot11RMBSSAverageAccessDelayActivated is true. Otherwise, not present”

P835.16:

Change from “The Supported Operating Classes element is present if dot11ExtendedChannelSwitchActivated or dot11OperatingClassesRequired is true. The Supported Operating Classes element is optionally present if dot11TVHTOptionImplemented is true.”

to “The Supported Operating Classes element is present if dot11ExtendedChannelSwitchActivated or dot11OperatingClassesRequired is true and is optionally present if dot11TVHTOptionImplemented is true. Otherwise, not present.”

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Comment | Proposed Change |
| 388 |  |  |  | C.3 sometimes uses "station" rather than consistently using "STA" | As it says in the comment |

***Proposed resolution:***

Revised

Check the “DESCRIPTION” of each of the MIB variables and replace the word “station” with “STA”.

Note to the Editors: There are over 700 instances of “station”.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Comment | Proposed Change |
| 507 |  |  |  | Use glyphs rather than Floor(), e.g. in the BIPN = equations and the NOTE 1; ditto Ceil() | Fix in Equation (9-5), (12-1), (12-2), (26-4), the NOTE 1 on page 1297 (2x), Table 9-14, the equation at the bottom of page 2410, the middle of page 2421, the top of page 2425, (10-19) and 6 lines down, the bottom of page 2434, the same NOTE 1 on page 1297 (2x), 4411.6, 5368.27 |

***Discussion:***

Agree with the commenter in principle, except that the two Floor() and two Ceil() in page 1297 should be page 3297.

***Proposed resolution:***

Revised.

Replace Floor()/Ceil() with glyphs in Equation (9-5), (12-1), (12-2), (26-4), the NOTE 1 on page 3297 (2x), Table 9-14, the equation at the bottom of page 2410, the middle of page 2421, the top of page 2425, (10-19) and 6 lines down, the bottom of page 2434, the same NOTE 1 on page 3297 (2x), 4411.6, 5368.27.