**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title |  | |
| Date Submitted | [11 February, 2010] | |
| Source | [Jaeseung Son, Taehan Bae, Sridhar Rajagopal, E.T. Won] [Samsung Electronics] [Suwon, Korea] | Voice:[82-31-279-7293] Fax: [ ] E-mail:[taehan.bae@samsung.com] |
| Re: | [] | |
| Abstract | [Subclauses 7.4.15] | |
| Purpose | [Description of what the authors wants P802.15 to do with the information in the document.] | |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |

**7.4.15 Channel hopping command**

|  |  |  |
| --- | --- | --- |
| Octets:7 | 1 | 7 |
| MHR fields | Command frame identifier(see table 73) | Channel hopping fields |

When the VLC communication system uses the same time slot between the adjacent light sources or cells with multiple channel communication, the channel hopping should be used. In order to avoid interference and increase system capacity, pre assigned hopping pattern should be adopted.

**7.4.15.1 Multiple channel hopping fields**

Refer section 7.8.2 Channel hopping for interference avoidance