**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title |  |
| Date Submitted | 17 August 2011 |
| Source |  Hayward, CA | Voice: 1 510 400 2936 Fax: E-mail: jsimon@dustnetworks.com |
| Re: | Editorial instructions in support of proposed resolutions to sponsor ballot comments (J. Simon) |
| Abstract | Editor instructions for fixing ACK/NACK encoding |
| Purpose | Provide instructions to the editor to correct problems identified with the TSCH ACK/NACK time correction description in the sponsor ballot draft D6 review. |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

The ACK/NACK Time Correction header IE is described as a 16-bit signed integer, which requires all 16-bits be used, but the MSB is described as being reused to indicate a NACK. The original intent was to bound the correction to +/- 2 ms, so we only need 11 bits of the field for actual representation. Language needs to be added to indicate how to handle the encoding properly.

0 to 2047 µs = 0x000 - 0x7FF

-1 to -2048 µs = 0xFFFF - 0xF800

So we can mask the value with 0xFFF and only look at the lower 3 nibbles. We OR the result with 0x8000 to indicate a NACK.

***Editor’s instructions – Modify third paragraph of 5.2.4.3.6 and figure 43a as follows:***

The Time Sync Info field shall specify time synchronization information and ACK/NACK status. This field is constructed by taking a signed 16-bit 2’s compliment time correction in the range of -2048 to 2047 µs, and logically AND’ing it with 0xfff, and OR’ing again with 0x8000 to indicate a NACK. This field shall be set as indicated in Table 4i.

Table 4i— Values of the Time Sync Info field for ACK with timing Information

|  |  |
| --- | --- |
| Range | Description |
| ~~0x0000–0x7fff~~ | ~~Time correction, in μs, signed 16 bit integer (2’s complement).~~ |
| ~~0x8000~~ | ~~MSB set to indicate NACK~~ |
| 0x000 – 0x7ff | ACK with positive time correction in µs. |
| 0x800 – 0xfff | ACK with negative time correction is µs.  |
| 0x8000 – 0x87ff | NACK with positive time correction in µs. |
| 0x8800 – 0x8fff | NACK with negative time correction is µs.  |