4e comment resolution for CID 520 in doc. 576-04

Change 'the next higher layer of the coordinator shall send the association response command to the device directly' (Page 21 Line 12) to 'the MAC sublayer of the coordinator shall send the association response command to the device directly (figure 67a)', and change figure 67a to the figure in the other document, because the current figure 67a seems to be in the wrong place. And figure 67a is as follow:

Association request

MLME-ASSOCIATE.request

Device next higher layer

Device

MLME

Coordinator

MLME

MLME-ASSOCIATE.indication

MLME-ASSOCIATE.confirm

Acknowledgement

MLME-ASSOCIATE.response

Association response

Coordinator next higher layer

Acknowledgement