**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **MAC simulation scenarios**  |
| Date Submitted | January 15, 2013 |
| Source | Sunggeun Jin (ETRI) | E-Mail: [sgjin@etri.re.kr] |
| Re: | MAC simulation scenarios |
| Abstract | This is a proposal for the MAC simulation scenarios in TGD |
| Purpose |  |
| Notice | This document does not represent the agreed views of the IEEE 802.15 Working Group or IEEE 802.15.8 Task Group. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |
| Patent Policy | The contributor is familiar with the IEEE-SA Patent Policy and Procedures:<http://standards.ieee.org/guides/bylaws/sect6-7.html#6> and<http://standards.ieee.org/guides/opman/sect6.html#6.3>.Further information is located at <http://standards.ieee.org/board/pat/pat-material.html> and<http://standards.ieee.org/board/pat>. |

## System-level simulation (MAC)

MAC simulation scenarios may provide network topologies and metrics in order to compare MAC performances.

### Scenarios & parameters for just PDs

<Simulation condition >

|  |  |
| --- | --- |
| PD deployment | All PDs are randomly scattered with uniform distribution in a ‘D’ by ‘D’ region. D indicates a distance in units of meter. |
| Data rate | Basic data rate may be applied |
| Number of PDs | > 0 |
| Channel model | Channel model may or may not be applied  |

<Performance Metric>

* Average discovery time depending on the number of PDs

### Scenarios & parameters for PD links

<Simulation condition>

|  |  |
| --- | --- |
| PD deployment | All PDs are randomly scattered with uniform distribution in a ‘D’ by ‘D’ region. D indicates a distance in units of meter. |
| Data rate | All data rates, which PHY may support, may be applied |
| Number of PDs | > 0 |
| Channel model | Channel model may or may not be applied  |

<Performance Metric>

* Throughput depending on the number of PDs (bps)
* Transmission delay (sec.)
* Fairness index (TBD)