**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | C**omments on 15-14-0338-05** |
| Date Submitted | June 11, 2014 |
| Source | Soo-Young Chang (SYCA),Jaehwan Kim (ETRI), Sangjae Lee (ETRI), and Sangsung Choi (ETRI) | Voice: [+1-530-574-2741]E-mail: [sychang@ecs.csus.edu] |
| Re: | [Subclause 7.1 of 802.15 TG10 TGD and [TGD Scenario Parameters #319r0](https://mentor.ieee.org/802.15/dcn/14/15-14-0319-00-0010-tgd-scenario-parameters.docx)] |
| Abstract | [Comments on 15-14-0338-05, Scenario Parameters for CfFP] |
| Purpose | [Define the parameters to consider in the scenario for final proposals] |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

**Introduction**

This document has been prepared to suggest some comments on 15-14-0338-05 regarding the operational scenarios which will be included in the TG10 TGD so that the TG10 scenarios **meet all requirements and fit better to real situations, by which proposals can be fairly compared.**

**Comments on 15-14-0338-05**

**The comments are as shown in purple in the following:**

|  |  |
| --- | --- |
|  | **Scenarios** |
| **Parameter** | **Mostly Upstream:****Smart metering, infrastructure monitoring, Irrigation Optimization** | **Mostly Downstream:****Street lighting, smart lighting** | **Balanced upstream and downstream:****CEMS, BEMS, HEMS 3** | **P2P:****Variety of applications** |
| Packet size | 100 bytes | 31 bytes, 255 bytes, 2047 bytes |
| Data rate | 100kbps, 250kbps  | 20kbps, 250kbps, 2Mbps[6] |
| Packet birth rate | 1 packet every 30 min | 1 packet / sec[[1]](#footnote-1)1 packet/min, 1 packet/30min |
| Duty cycle | 100%, 1% |
| Mobile devices (Y/N) - speed | N | Y – 1.4m/s (human walking speed)\* |
| Number of entry points  | 1 | 1, 3\* |
| Number of exit points  | 1 | 1, 3\* |
| PAN Coord to Device | Unicast[[2]](#footnote-2) (Y/N) | Y | N |
| Multicast (Y/N) |
| Broadcast (Y/N) |
| Device to PAN Coord[[3]](#footnote-3) |
| Device to device | Unicast (Y/N) | N | Y |
| Multicast (Y/N) |
| Broadcast (Y/N) |
| Multiple devices to device (Y/N)  |
| Number of PAN coordinators  | 1 | 1, 3\* |
| Linear Topology (Y/N) | N | Y | N | N |
| Energy consumption | TX | 28 mA  | 30 mA  |
| RX | 11.2 mA  | 37 mA  |
| Idle | 1.5 uA [1] | 500 uA  |
| Sleep | 0.1 uA [1] | 0.2 uA  |
| Link failure rates |

|  |  |
| --- | --- |
|  |  |
| a) | b) |

 |

**Definitions**:

Data rate: data rate at the physical layer

Packet birth rate: rate at which packets are being generated at the application layer of the device

Duty cycle: ratio of wake-up time to total operational time including sleeping time of a device

Device: node other than the PAN coordinator

M: Number of nodes in the PAN

M = 121 (11x11), 1089 (33x33), 10000 (100x100)

For linear topology, only 1 row of m nodes is considered, with m = 100

Unicast: transmission from 1 source to 1 destination

Multicast: transmission from 1 source to m destinations (m < M -1)

 m=11 for M=121, m=33 for M =1089, and m=100 for M =10000

Broadcast: transmission from 1 source to M -1 destinations

Multiple devices to device: transmission from n devices to one device

 m=11 for M =121, m=33 for M =1089, and m=100 for M =10000

**References**

1. <http://www.semtech.com/images/datasheet/sx1272.pdf>
2. MC13202, Low power transceiver for the IEEE 802.15.4 Standard, http://cache.freescale.com/files/rf\_if/doc/data\_sheet/MC13202.pdf?pspll=1&Parent\_nodeId=1141674020187711908069&Parent\_pageType=product
3. Tokyo statistical yearbook, Population and Households, <http://www.toukei.metro.tokyo.jp/tnenkan/2012/tn12qa021000.xls>
4. 15-14-0239-02 Proposed operational scenarios of L2R networks for TG10 TGD
5. C. Townsend, S. Arms (2005). Wireless Sensor Networks: Principles and Applications. In J.S. Wilson (Ed), Sensor Technology Handbook (pp. 575-589). Oxford, UK: Elsevier.
6. Nordic Semiconductor, nRF24L01+, https://www.sparkfun.com/datasheets/Components/SMD/nRF24L01Pluss\_Preliminary\_Product\_Specification\_v1\_0.pdf

**Additional comments on this table**

**Comment 1**

**From 6.18 of TGD (**Multiple Entry and Exit points)

*For the proposal:*

* *Devices shall implement a method to select the most appropriate entry/exit point for their communications with entities outside the network*
* *If a device becomes unable to communicate with an entity outside the network at the required quality of service using its preferred entry/exit point, it shall be possible for the device to find an alternative entry/exit point (if one exists) and begin to use that*
* *It shall be possible for devices to use different entry/exit points to communicate with different external entities*

**Use of multiple entry/exit points seems to be mandatory.**

**Comment 2**

## From 6.1 of TGD (Deployment architecture)

It should be possible to merge an independent subnet into a larger network when connectivity between them becomes available, providing both are using similar operating parameters. The merge operation should ideally take place without outside intervention. It should be possible for a network to operate as a number of independent subnets in the event of failure of parts of the network.

**Use of multiple networks seems to be mandatory even though “should” be used for this subclause.**

**Comment 3**

## Link failure rates should be specified.

1. This data rate is to be simulated only with data rates of 250 kbps and 2 Mbps [↑](#footnote-ref-1)
2. In a PAN coord to device unicast communication, the PAN coord shall send a packet to every devices (M-1) alternately

3 CEMS: continuous emission monitoring systems, BEMS: building energy management system, HEMS: home energy management systems [↑](#footnote-ref-2)
3. In a device to PAN coordinator communication, all the devices (M-1) shall send a packet to the PAN coordinator with the packet birth rate specified in the table

\* Values followed by “\*” are optional since they correspond to “MAY” statements of the TGD [↑](#footnote-ref-3)