**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title | Text for Relative Positioning | |
| Date Submitted | January 2015 | |
| Source | Igor Dotlić (NICT)  Huan-Bang Li (NICT)  Marco Hernandez (NICT)  Ryu Miura (NICT)  Billy Verso (DecaWave),  Michael McLaughlin (DecaWave) | dotlic @ nict.go.jp  lee @ nict.go.jp  marco @ nict.go.jp  ryu @ nict.go.jp  billy.verso @ decawave.com  michael.mclaughlin @ decawave.com |
| Re: | draft text of UWB PHY for 802.15.8 | |
| Abstract | This is the work in progress text of the Relative Positioning for IEEE 802.15.8 group for PAC. | |
| Purpose | This document provides the details of the PHY proposal to IEEE 802.15.8 | |
| Notice | This document does not represent the agreed views of the IEEE 802.15 Working Group or IEEE 802.15.8 Task Group. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |
| Patent Policy | The contributor is familiar with the IEEE-SA Patent Policy and Procedures:  <http://standards.ieee.org/guides/bylaws/sect6-7.html#6> and  <http://standards.ieee.org/guides/opman/sect6.html#6.3>.  Further information is located at <http://standards.ieee.org/board/pat/pat-material.html> and  <http://standards.ieee.org/board/pat>. | |

1. Relative positioning

## Symmetrical double-sided two-way ranging

This sub-clause describes principles of relative positioning between two devices in PAC networks. Regarding positioning the standard specifies only the time units used for ranging timestamps in clause 10.4.1 and SAP for relative positioning that is defined in previous sub-clause). Since the positioning calculation is done by higher layers, and the standard specifies only PHY and MAC, this clause only gives recommendation for the positioning methodology.

P12

P12

P22

P22

P21

*Tround*1

*Tprop*

*Treply*1

*t*

*Tprop*

*Tprop*

*t*

*Tround*2

*Treply*2

Device 1

Device 2

*Tprop*

P21

P11

P11

Figure : Principle of symmetrical double-sided two-way ranging.

The positioning method recommended is called symmetrical double-sided two-way ranging.

As Figure 1 shows, symmetrical double-sided two-way ranging is achieved by measuring two round trip times: round trip time from device 1 to device 2 denoted and round trip time from device 2 to device 1 denoted . denotes propagation time that is being estimated, while and represent reply times of device 1 and 2 respectively. The time of sending a certain frame is defined as time of beginning of SFD. In order to measure device 1 sends frame P11. After receiving P11 and time period device 2 sends frame P21 which device 1 receives. After that the same procedure is repeated with device 1 and device 2 switching places. Hence, the second part of the procedure is initiated by device 2 which sends frame P22. After receiving P22 and time device 1 sends frame P12.

At the end, estimate should be calculated as follows

|  |  |  |
| --- | --- | --- |
|  |  | **(1)** |

If relative errors of timing at device 1 and 2 are denoted and it follows that

|  |  |  |
| --- | --- | --- |
|  |  | **(2)** |
|  |  | **(3)** |
|  |  | **(4)** |
|  |  | **(5)** |

Thus error of estimation is:

|  |  |  |
| --- | --- | --- |
|  |  | **(6)** |

Hence, relative error of the range estimation is also in the same order of magnitude as and , which for crystal oscillators are usually in tenths of ppm.