**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title | **ToC of P802.15.8 PAC Draft Std.** | |
| Date Submitted | Sept. 2015 | |
| Source | [] [] [address] | Voice: [ ] Fax: [ ] E-mail: [ ] |
| Re: |  | |
| Abstract | ToC of P802.15.8 PAC Draft Std. | |
| Purpose |  | |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |

Red font: we don’t have any text yet.

Highlighted in yellow: we have some simple text there, like 1~3 lines.

Highlighted in green: we have reasonable text there, not to that level of detail yet but the best that we’ve done so far.

Highlighted in blue: we have approved the text to be adopted by the latest revision of spec. draft “P802.15.8\_PAC”.

Contents

**1. Overview 1**

**1.1 General 1**

**1.2 Scope 1**

**1.3 Purpose 2**

**2. Normative references 2**

**3. Definitions 2**

**3.1 Definitions 2**

**3.2 Acronyms and abbreviations 4**

**4. General description 6**

**4.1 General 6**

**4.2 Components of IEEE 802.15.8 PAC 6**

**4.3 Network Topologies 6**

**4.4 Architecture 7**

**4.4.1 Physical layer (PHY) 8**

**4.4.2 MAC sublayer 8**

**4.5 Functional Overview 8** (Yes, wait till Clause 5&6 are done, TBD.)

**4.5.1 Superframe structure 9**

**4.5.2 Communication types 9 (**general description)

4.5.3 Frame structure

4.5.4 Security

4.6 Concept of primitives

**5. MAC protocol 10**

**5.1 MAC functional description 10**

**5.1.1 Channel access 10 (We need general description of CFP and CAP, etc.)**

**5.1.2 Starting and maintaining PACs 11 (Move 5.3 here)**

**5.1.3 Peering and de-peering 11 (Figures are missing, ask Qing for the figure, if not available, use the old one to update. Ref: 554r1)**

**5.2 MPDU formats 13**

**5.2.1 General MPDU format 13**

**5.2.2 Transmission, reception, and acknowledgment 14**

**5.3 Channel scanning 20**

**5.3.1 General description 20**

**5.3.2 ED Channel scan 20**

**5.3.3 Active and passive channel scan 20**

**5.X1 General MAC frame (to be added)**

5.2.1.1 Frame Control field

5.2.1.1.1 Frame Type field

5.2.1.1.2 Security Enabled field

5.2.1.1.4 Acknowledgment Request (AR) field

5.2.1.1.8 Source Addressing Mode field

5.2.1.2 Sequence Number field

5.2.1.4 Destination Address field

5.2.1.6 Source Address field

5.2.1.6 Link ID field (optional)

5.2.1.1.7 Frame Version field

5.X1 IE field (ref. IEEE 802.15.4e or 4g, etc.)

5.2.1.7 Auxiliary Security Header field

5.2.1.8 Frame Payload field

5.2.1.9 FCS field

**5.X2 Format of individual frame types**

**5.2.2.2 Data frame format**

5.2.2.2.1 Data frame MHR fields

5.2.2.2.2 Data Payload field

**5.2.2.3 Acknowledgment frame format**

**5.2.2.4 MAC command frame format**

5.2.2.4.1 MAC command frame MHR fields

5.2.2.4.2 Command Frame Identifier field

5.2.2.4.3 Command Payload field

**5.4 Synchronization procedure 23**

**5.4.1 Initial synchronization procedure 23**

**5.4.2 Maintaining synchronization procedure 28**

**5.4.3 Re-synchronization procedure 30**

**5.5 Discovery 30**

**5.5.1 Discovery types 30**

**5.5.2 Discovery information 30**

**5.5.3 Discovery procedure 30**

**5.5.4 Discovery messages 34**

**5.6 Peering 34**

**5.6.1 One-to-one peering procedure 34**

**5.6.2 One-to-one Re-peering procedure 36**

**5.6.3 One-to-one De-peering procedure 37**

**5.6.4 One-to-Many peering/de-peering/re-peering procedure (to be added) (HB & Marco)**

**5.7 Communication period 39**

**5.7.1 CAP (Contention Access Period) 39 (BJ)**

**5.7.2 CFP (Contention Free Period) 40 (Marco)**

**5.8 MAC command frames 42**

**5.8.1 One-to-one peering request command 42**

**5.8.2 One-to-one peering response command 43**

**5.8.3 One-to-one Re-peering request command 44**

**5.8.4 One-to-one re-peering response command 45**

**5.8.5 One-to-one de-peering request 45**

**5.8.6 One-to-one De-peering response command 46**

**5.8.7 ReS request command 46**

**5.8.x one-to-many peering/de-peering/re-peering commands (to be added) (HB & Marco)**

**5.8.8 Discovery commands (to be added) (Marco)**

**5.8.9 Commads for CAP (to be added) (BJ)**

**5.8.10 Commads for CFP (to be added) (Marco)**

**6. MAC services 48 (Marco)**

**6.1 Overview 48**

**6.2 MAC management service 48**

**6.2.1 Common requirements for MLME primitives 48**

**6.3 MAC data services 52**

**6.3.1 MCPS-DATA.request 52**

**6.3.2 MCPS-DATA.confirm 52**

**6.3.3 MCPS-DATA.indication 53**

**6.4 PIB 54**

**7. General PHY requirements 55**

**7.1 Operating frequency range 55**

**7.2 Minimum LIFS and SIFS periods 56**

**7.3 Transmitter On/Off power 56**

**7.4 Transmitter transient period 56**

**7.5 Frequency error 57**

**7.6 Error vector magnitude (EVM) 57**

**7.7 Output RF spectrum emissions 58**

**7.7.1 Transmission bandwidth 58**

**7.7.2 Out-of-band emissions (OOB) 58**

**7.8 RF power measurement 59**

**7.9 Transmit spectral mask 59**

**7.10 Transmit power 60**

**7.11 Receiver sensitivity 60**

**7.12 Start and end of a PPDU 60**

**7.13 RX-to-TX turnaround time 60**

**7.14 TX-to-RX turnaround time 60**

**7.15 Receiver energy detection (ED) 60**

**7.15.1 ED threshold 60**

**7.15.2 ED measurement time 61**

**7.16 Channel quality indicator (CQI) 61**

**7.17 Clear channel assessment (CCA) 61**

**8. PHY services 61**

**8.1 Overview 61**

**8.2 PHY description 62**

**8.3 PHY procedures 63**

**8.4 PHY measurements 63**

**9. PHY 63**

**9.1 Low Mobility PHY specification 64**

**9.1.1 Operating frequency range 64**

**9.1.2 Channel assignments 64**

**9.1.3 Duplex schemes 64**

**9.1.4 Multiplexing schemes 64**

**9.1.5 PPDU format for low mobility PHY 64**

**9.1.6 Modulation and coding 73**

**9.1.7 RF requirements 74**

**9.1.8 Multiple antennas 75**

**9.1.9 Clear channel assessment (CCA) 75**

**9.2 High Mobility PHY specification 75**

**9.2.1 PHY frame structure 75**

**9.2.2 TDD frame 76**

**9.2.3 Guard interval 77**

**9.2.4 Preamble 77**

**9.2.5 Control channel 78**

**9.2.6 PHY header 78**

**9.2.7 Data rate 79**

**9.2.8 PSDU length 79**

**9.2.9 Burst mode 79**

**9.2.10 Scrambler seeds 79**

**9.2.11 Frame type 79**

**9.2.12 PSDU type 79**

**9.2.13 Header check sequence 80**

**9.2.14 Discovery 80**

**9.2.15 Random access PHY generation 81**

**9.2.16 Random access procedure 82**

**9.2.17 PSDU construction 83**

**9.2.18 QC-LDPC encoder parameters 85**

**9.2.19 Interleaver 85**

**9.2.20 Scrambler 86**

**9.2.21 Modulation mapper 86**

**9.2.22 Pad bits 86**

**9.2.23 Modulations 87**

**9.2.24 Layer mapping 87**

**9.2.25 Layer mapping for one antenna 88**

**9.2.26 Open loop spatial multiplexing 88**

**9.2.27 Transmit diversity 88**

**9.2.28 Precoding 89**

**9.2.29 Single antenna mapping 89**

**9.2.30 Open loop spatial multiplexing 89**

**9.2.31 Transmit diversity 91**

**9.2.32 Multicarrier modulation 92**

**9.2.33 Cyclic prefix 92**

**9.2.34 Resource block 92**

**9.2.35 Filtered OFDM symbols for sub-1 GHz band 94**

**9.2.36 Carrier aggregation 95**

**9.2.37 Data rates 95**

**9.2.38 Reference signals 96**

**9.2.39 Optional GFSK modulation 97**

**9.2.40 Operating frequency bands 98**

**10. UWB Physical (PHY) layer specification 99**

**10.1 General 99**

**10.1.1 PPDU format 99**

**10.1.2 PPDU encoding process 100**

**10.1.3 PHY header (PHR) 103**

**10.1.4 Data field 107**

**10.1.5 Forward error correction (FEC) 107**

**10.1.6 UWB PHY band allocation 110**

**10.2 BPM-BPSK modulation mode 110**

**10.2.1 General 110**

**10.2.2 SHR preamble 111**

**10.2.3 PHR and PSDU - Symbol structure and modulation 117**

**10.2.4 BPM-BPSK modulation mode RF requirements 122**

**10.3 OOK modulation mode 124**

**10.3.1 General description 124**

**10.3.2 Format of SHR 124**

**10.3.3 Spreading and data rates 126**

**10.3.4 Symbol structure 127**

**10.3.5 Compliant pulses 127**

**10.4 Timestamps and time units 127**

**10.4.1 Time units 128**

**10.4.2 Antenna delays 128**

**11. Transmit power control 128**

**11.1 Power control information detection 128**

**11.2 Power control during CFP 130**

**11.2.1 PAC device behavior 130**

**11.3 Power control during CAP 133**

**12. Multi-hop operation 135 (Multi-hop is mentioned in TG8 PFD Doc: 15-14-0085-01-0008, TG8 decided to provide an interface to upper layer for multi-hop operation.**) **(Together)**

**13. Relative positioning and localization 135**

**13.1 Overview 135**

**13.2 Service access points for message time stamps 136**

**13.2.1 Frame transmission timestamping 136**

**13.2.2 Frame reception timestamping 136**

**13.2.3 Control of ranging and the transfer of timestamps 136**

**13.3 Ranging and localization methods 139**

**13.3.1 Preface 139**

**13.3.2 Single-sided two-way ranging 139**

**13.3.3 Double-sided two-way ranging 140**

**13.3.4 Double-sided two-way ranging with three messages 141**

**13.3.5 Time difference of arrival (TDOA) 141**

**13.3.6 Localization 141**

**13.3.7 Angle of arrival (AOA) 142**

**13.3.8 Received signal strength indication (RSSI) 142**

**13.4 Ranging procedures 142**

**13.4.1 General ranging procedures 142**

**13.4.2 Ranging procedure for SS-TWR with deferred reply time result 142**

**13.4.3 Ranging procedure for SS-TWR with embedded reply time result 143**

**13.4.4 Ranging procedure for DS-TWR with deferred timestamp information 144**

**13.4.5 Ranging procedure for DS-TWR with embedded timestamp information 145**

**14. Power management 146 (HB)**

**15. Security 146 (BJ)**

**15.1 PHY Security**

**Annex A 147**

**Annex B 149**

**Annex C (informative) 152**

**Annex D (informative) 155**

**D.1 The mathematics of two-way ranging 155**

**D.1.1 Single-sided two-way ranging error due to clock offset 155**

**D.1.2 Deviation of double-sided two-way ranging formula 156**

**D.1.3 Asymmetric double-side two-way ranging error due to clock offset 159**

The following items are from the **TG8 PFD Doc: 15-14-0085-01-0008**

1. QoS **(Together)**