**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title | Received Signal Weakness (RSW) metric specification for TG10 (L2R) | |
| Date Submitted | [26 November, 2015] | |
| Source | [Charlie Perkins] [Futurewei] | Voice: [+1-408-330-4586] Fax: [+1-408-330-5088] E-mail: [charliep@computer.org] |
| Re: | [Received Signal Weakness metric] | |
| Abstract | Proposed alternate metric to replace SQS | |
| Purpose | [TG10 (L2R) draft specification improvement.] | |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |

* ***Replace the title of 5.2.2.1 with “Received Signal Weakness (RSW)”***
* ***Replace 5.2.2.1 with the following text:***

RSW is a metric which measures the cost of a path due to reductions in signal strength and has the following properties:

1. As signal strength degrades, the value of the metric increases.  In other words, the metric measures signal weakness instead of signal strength.
2. The value of the metric increases rapidly with weakness of the signal, so that links with better signal strength are greatly preferred. The RSW value increases exponentially with loss of signal strength.
3. Links with very strong signals should have very low metric values, close to zero.
4. Signal strength measurements are notoriously unstable and inaccurate, so great precision is not needed.

Make the following definitions:

*Pmax* the maximum feasible value for received signal strength, measured in mW

*Pmin* the minimum feasible value for received signal strength, measured in mW

*Pmeas* the measured value for received signal strength, measured in mW

*P* normalized received power ratio in the range (0, 1)

*Max\_RSW* the maximum possible value for the RSW metric

*Min\_RSW* the minimum possible value for the RSW metric

*0*, ** calculated values for the received signal weakness metric

Let *P* = (*Pmax* - *Pmeas*) / (*Pmax* - *Pmin*). *P* is a positive number in the range (0, 1).  The following formula satisfies properties (1) – (3) above:

* 0* (*P*) = *P*8.

* 0* also lies in the range (0, 1). In order for the RSW metric ** to be in the range (*Min\_RSW*, *Max\_RSW*), we multiply * 0* by the scaling factor (*Max\_RSW-Min\_RSW*), convert to integer, and add *Min\_RSW*:

** (*P*) = ⌊(*Max\_RSW-Min\_RSW*) \* * 0* (*P*) ⌋ + *Min\_RSW*.

For the RSW metric, *Max\_RSW* = 254 and *Min\_RSW* = 1, requiring only 8 bit values for ** (*P*). 255 is the maximum possible value of the metric, and is reserved to mean *infinity*.  To calculate the RSW metric over a multi-hop route, the link values are summed; anything added to *infinity* results in the same value, *infinity*.

* ***In Table 11, replace SQS with RSW***
* ***Insert “Received Signal Weakness RSW” in clause 3.2***
* ***Delete SQS from clause 3.2***