**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **Proposed comment resolution for i-92, i-106 from the sponsor ballot** |
| Date Submitted | 7 August 2016 |
| Source | \*[Verotiana Rabarijaona, Fumihide Kojima], †[Hiroshi Harada]\*[NICT], †[Kyoto University]\*[3-4, Hikarino-oka, Yokosuka, 239-0847 Japan], †[36-1 Yoshida-Honmachi, Sakyo-ku, Kyoto 606-8501 Japan] | Voice: [+81-46-847-5075]Fax: [+81-46-847-5089]E-mail: [rverotiana@nict.go.jp] |
| Re: | 802.15.10 Consolidated Sponsor Ballor Comments, CID i-92, i-106 |
| Abstract | Provides a proposed resolution to CID i-92, i-106 |
| Purpose | To be used by the technical editor to apply the necessary changes to the draft to resolve CID i-92, i-106 |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

**Comments**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Clause** | **Line** | **Comment** | **Proposed change** |
| i-92 | 118 | 7.2.1 | 9 | How does the multicast frame sending work. Musticast frames have short addresses as destination addresses, but here it says the address mode depends on the MeshAddressMode. | Specify how multicast frame sending works. |
| i-106 | 121 | 7.2.3 | 48 | How does the multicast frame receiving work. The FnlDestAddr is in short address format, even if the mesh uses long addresses, so the MeshAddressMode cannot be used to know the format of FnlDestAddr format. | Explain how multicast receiving works. |

**Resolution: Revise**

The L2R Routing IE contains a Mesh Address Mode field and a Destination Address Mode field. The latter was added after D05 to allow the use of multicast even in 64-bit address operated mesh.

Make the L2R-DATA.request primitive consistent with the L2R Routing IE.

* ***Modify the L2R-DATA.request primitive as follows (unchanged parameters omitted):***

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Type** | **Valid range**  | **Description** |
| MeshAddressMode | Enumeration | SHORT, EXTENDED | Indicates the addressing mode used in the L2R mesh. Does not apply to DestAddr if Multicast is TRUE. |
| MeshRootAddress | Address | Short or extended address as specified by MeshAddressMode | Address of the mesh root of the L2R mesh on which the data frame is being transmitted. |
| ... | ... | ... | ... |
| Multicast | Boolean | TRUE, FALSE | Indicates whether the data is intended for a multicast group. Ignored if MeshRootData is TRUE. |
| ... | ... | ... | ... |
| SrcPanId | Integer | 0x0000-0xffff | The PAN identifier of the original source of the data frame being transmitted. |
| DestPanId | Integer | 0x0000-0xffff | The PAN identifier of the final destination of the data frame being transmitted. Ignored if MeshRootData is TRUE. |
| DestAddr | Address | Short or extended address as specified by MeshAddressMode if Multicast is FALSE, or short address if Multicast is TRUE. | The address of the final destination of the data frame being transmitted. Ignored if MeshRootData is TRUE. |

* ***Modify the L2R-DATA.indication primitive as follows (unchanged parameters omitted):***

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Type** | **Valid range**  | **Description** |
| MeshAddressMode | Enumeration | SHORT, EXTENDED | Indicates the addressing mode used in the L2R mesh. Does not apply to DestAddr if Multicast is TRUE. |
| ... | ... | ... | ... |
| Multicast | Boolean | TRUE, FALSE | Indicates whether the received data is intended for a multicast group as indicated by a destination address within the range 0xff00 – 0xfffd. |
| SrcPanId | Integer | 0x0000-0xffff | The PAN identifier of the original source of the data frame received. |
| SrcAddr | Address | Short or extended address as specified by MeshAddressMode | The address of the original source of the data frame received. |
| DestPanId | Integer | 0x0000-0xffff | The PAN identifier of the final destination of the data frame received. |
| DestAddr | Address | Short or extended address as specified by MeshAddressMode if Multicast is FALSE, or short address if Multicast is TRUE. | The address of the final destination of the data frame received. |
| ... | ... | ... | ... |

* ***Create a new L2IB attribute as follows***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Attribute** | **Type** | **Range** | **Description** | **Default** |
| *l2rMulticastAddressList* | List of short addresses | 0xff00 – 0xfffd | List of addresses of the multicast groups of which the device is a member | \_\_ |

* ***Modify 5.2.6 as follows:***

An implementation may require the transmission of the same data to a group of devices based on criteria such as geographic location (district, block, floor…), device type (actuators, sensors…), etc. These devices are organized into static and administratively defined multicast groups. The set of short addresses ranging from 0xff00 to 0xfffd is reserved for multicast groups. Multicast groups may be dynamic. The management of the groups is out of the scope of this document. If a higher layer protocol uses extended multicast addresses, they should be mapped to the reserved multicast short addresses. This mapping is out of the scope of the document. Multicast routing is handled by the L2R sublayer if the L2R multicast parameter of the corresponding MT is TRUE. Otherwise, multicast frames are treated as broadcast frames by the L2R sublayer and are filtered by higher layers.

Multicast route establishment is achieved through the transmission of RA IEs. If a device belongs to a multicast group and if multicast routing is handled by the L2R sublayer, the next higher layer informs the L2R sublayer with an L2R-MULTICAST-SUBSCRIPTION.request primitive. Upon reception of the primitive, the L2R sublayer includes the multicast address(es) in its RA IEs. The L2R sublayer holds the multicast address(es) in *l2rMulticastAddressList*. If the device is the mesh root, the L2R sublayer records the multicast address(es) in *l2rMulticastAddressList* but does not transmit RA IEs.

A device belonging to one or more multicast groups sets the Multicast Subscription Present field to 1 and includes the corresponding multicast address(es) in the Multicast Subscription field in its RA IE during the DS route establishment procedure. The Multicast Subscription field of the RA IE is described in 6.2.1.7.

After the transmission of the RA IE with the multicast subscription information, the L2R sublayer notifies the next higher layer with an L2R-MULTICAST-SUBSCRIPTION.confirm primitive. This procedure is illustrated in Figure 19. The L2R-MULTICAST-SUBSCRIPTION.request and L2R-MULTICAST-SUBSCRIPTION.confirm primitives are described in 7.1.3.1 and 7.1.3.2 respectively. If a device has left a multicast group, the next higher layer informs the L2R sublayer with the L2R-MULTICAST-SUBSCRIPTION.request with the corresponding multicast address omitted. The change is reflected in the next scheduled RA IE and in *l2rMulticastAddressList*.

If a device receives an RA IE with the Multicast Subscription Present field set to 1, the multicast address(es) therein is treated as a unicast address and is recorded in the list of reachable multicast groups of the neighbor from which the RA IE was received.

* ***Modify the 5.4.2 as follows:***

Multicast routing is handled by the L2R sublayer in an L2R mesh if L2R Multicast in the corresponding MT is TRUE.

When multicast routing is handled at the L2R sublayer in a regular mesh (i.e. not in an SSPAN nor a TMCTP), if a frame is to be sent to a multicast group as indicated by a destination address within the range 0xff00 – 0xfffd, the next higher layer requests data routing with the L2R-DATA.request primitive where Multicast is set to TRUE and DestAddr is set to the multicast address. If the original source of the multicast frame is a device other than the mesh root, the frame is first routed to the mesh root through US routing with the multicast address as the DA in the L2R Routing IE. If the original source is the mesh root or when the mesh root receives a multicast frame, it forwards the frame DS with the broadcast address as the NHA. If the mesh root is also a member of the multicast group, its L2R sublayer delivers a copy of the frame to the next higher layer with the L2R-DATA.indication primitive where Multicast is set to TRUE and DestAddr is set to the multicast address.

From then on, a device receiving the frame forwards it only if it has a DS route to at least one member of the multicast group as indicated by the multicast address found in the list of reachable multicast groups of at least one neighbor, and the NHA is always set to the broadcast address. If a receiving device is a member of the multicast group, the frame is delivered to the next higher layer with the L2R-DATA.indication primitive where Multicast is set to TRUE, and DestAddr is set to the multicast address. If the member of the multicast group also has other members among its descendants, the frame is duplicated and forwarded.

When a device receives a multicast frame for the first time, it records the LSN and the SA. If it receives another frame with the same LSN and SA, the frame should be dropped. This record is deleted after *l2rSnSaRecordTimeout*. Figure 31 illustrates the processing of a multicast data frame by the original source; Figure 32 illustrates the processing of a multicast data frame by an intermediate hop.

* ***Modify Figure 32 as follows:***

