**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **Kookmin PHY 5 PPDU frame formats** |
| Date Submitted | [September, 2016] |
| Source | Trang Nguyen, and Yeong Min Jang (Kookmin University) |
| Re: |  |
| Abstract | Details of Resolutions regarding to the submitted Comments on D0 are suggested.  PHY 5 modes: PPDU frame formats are presented. |
| Purpose | D0 Comments Resolutions and Editorial Revision. |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

# PHY 5 PPDU formats

**9.6.7.2 M-FSK PPDU format**

|  |  |  |  |
| --- | --- | --- | --- |
| **Preamble**  (see 9.6.7.2.1) | **PHY header**  (see 9.6.7.2.2) | **HCS**  (see 9.6.7.2.3) | **PSDU**  (see 9.6.7.2.4) |
| SHR | PHR | | PHY payload |

The M-FSK PPDU frame structure consists of the preamble field, PHR sub-fields, and the PSDU PHY payload.

9.6.7.2.1 **M-FSK Preamble field**

The preamble field for M-FSK is two symbol times long. Each symbol time is for a specific preamble frequency as follows.

|  |  |  |
| --- | --- | --- |
| Duration | one symbol time | one symbol time |
| Preamble | fSF | f'SF |

* The first preamble : fSF = 200Hz is fixed frequency.
* The second preamble : f’SF = fSF + 33.∆f is variable as a function of ∆f.

9.6.7.2.2 **M-FSK PHY header**

The PHY header will support the related communication modes those are specified by MAC frame, at least low-overhead beacon mode, bidirectional communications mode, and D2D mode will be supported. The PHY header is TBD, will be clarified along with MAC frame when D1 comes out.

9.6.7.2.3 **M-FSK HSC**

TBD along with PHY header.

9.6.7.2.4 **M-FSK PSDU PHY payload**

The PSDU consists of multiple data frequency symbols, each symbol carries multiple bits data. The amount of bits carried by a frequency symbol depends on the number of frequencies used in modulation. By using 32 frequencies for modulation, 4 data bits along with an asynchronous bit (Ab) is transmitted by a frequency symbol each time. Likewise by using 64 frequencies for modulation, 5 data bits along with an asynchronous bit (Ab) is transmitted by a frequency symbol each time.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **PSDU payloads** | | | |
|  | frequency symbol 1 | frequency symbol 2 | **…** | frequency symbol N |
| Mode 1:  32-FSK | (1 Ab + 4 data bits) | (1 Ab + 4 data bits) |  | (1 Ab + 4 data bits) |
| Mode 2:  62-FSK | (1 Ab + 5 data bits) | (1 Ab + 5 data bits) |  | (1 Ab + 5 data bits) |
| Mode 3:  62-FSK/ 2-PSK | (1 Ab + 6 data bits) | (1 Ab + 6 data bits) |  | (1 Ab + 6 data bits) |

During transmission, the symbol rate of transmission must be less than the minimum frame rate of camera to guarantee that every symbol is sampled at least once.

**9.6.7.2 OOK PPDU format**

|  |  |  |  |
| --- | --- | --- | --- |
| **Preamble**  (see 9.6.7.2.1) | **PHY header**  (see 9.6.7.2.2) | **HCS**  (see 9.6.7.2.3) | **PSDU**  (see 9.6.7.2.4) |
| SHR | PHR | | PHY payload |

The OOK PPDU frame structure consists of the preamble field, PHR sub-fields, and the PSDU PHY payload.

9.6.7.2.1 **OOK Preamble field**

The preamble field for OOK is the same as the preamble used for M-FSK.

|  |  |  |
| --- | --- | --- |
| Duration | one symbol time | one symbol time |
| Preamble | fSF | f'SF |

* The first preamble : fSF = 200Hz is fixed frequency.
* The second preamble : f’SF = fSF + 33.∆f is variable as a function of ∆f.

9.6.7.2.2 **OOK PHY header**

The PHY header will support the related communication modes those are specified by MAC frame, at least low-overhead beacon mode, bidirectional communications mode, and D2D mode will be supported. The PHY header is TBD, will be clarified along with MAC frame when D1 comes out.

9.6.7.2.3 **OOK HSC**

TBD along with PHY header.

9.6.7.2.4 **OOK PSDU PHY payload**

The OOK PSDU consists of multiple data sub-packets (denoted as DS). Each sub-packet DS consists of its own preamble (DS preamble), Asynchronous bits (front Ab and rear Ab), and body payload.

**Table – PSDU frame format**

|  |  |  |  |
| --- | --- | --- | --- |
| **PSDU** | | | |
| Sub-packet 1 | Sub-packet 2 | **…** | Sub-packet N |

**Table – Sub-packet**

|  |  |  |  |
| --- | --- | --- | --- |
| **Sub-packet** | | | |
| SF | Ab | payload | Ab |

There are four different PSDU frames supporting four PHY modes as follows. Among them, mode 1 and mode 2 are operating at 2.2 kHz optical clock rate, whereas mode 3 and mode 4 are operating at 4.4 kHz optical clock rate.

**Table – Sub-Packet Structure Specifications**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Mode 1** | **Mode 2** | **Mode 3** | **Mode 4** |
| Preamble (SF) | 6B | 10B | 6B | 10B |
| Ab (front) | 2B | 2B | 4B | 4B |
| Payload (body) | 8 bits | 13 bits | 33 bits (24B) | 41 bits (62B) |
| Ab (rear) | 2B | 2B | 4B | 4B |