**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title | **PHY modes and TXs/RXs Revised based on Modulation Schemes** | |
| Date Submitted | September 2016 | |
| Source | Jaesang Cha,  Vinayagam Mariappan,  Soo-Young Chang  [SNUST, Korea, SYCA, USA] | Voice: [ ] Fax: [ ] E-mail: [chajs@seoultech.ac.kr] |
| Re: | [If this is a proposed revision, cite the original document.]  [If this is a response to a Call for Contributions, cite the name and date of the Call for Contributions to which this document responds, as well as the relevant item number in the Call for Contributions.]  [Note: Contributions that are not responsive to this section of the template, and contributions which do not address the topic under which they are submitted, may be refused or consigned to the “General Contributions” area.] | |
| Abstract | [Description of document contents.] | |
| Purpose | [Description of what the author wants P802.15 to do with the information in the document.] | |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |

# Annex X

(informative)

Table X1 shows that each PHY mode mainly supports what sorts of Tx.

Table X1 – PHY Modes / TXs

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | | Discrete (or single) source | Surface source | 2-Dimensional / Screen/M-Source | Painting |
| PHY I | | x | x |  |  |
| PHY II | | x | x |  |  |
| PHY III | | x | x |  |  |
| PHY IV | UFSOOK | x | x |  |  |
| Twinkle VPPM | x | x |  |  |
| S2-PSK | x |  |  |  |
| S2+DMS-PSK | x |  |  |  |
| Offset-VPWM | x | x |  |  |
| PHY V | RS-FSK |  | x |  |  |
| Compatible M-FSK |  | x |  |  |
| C-OOK |  | x |  |  |
| Packet PPM/PWM |  | x |  |  |
| PHY VI | 2D-sequential color code |  |  | x |  |
| VTASC | x | x | x | x |
| Sequential Scalable 2D Code |  |  | x | x |
| Invisible Data embedding |  |  | x | x |
| M-FSK |  |  | x | x |
| M-PSK |  |  | x | x |
| SS (Spread Spectrum) |  |  | x | x |
| Kookmin Invisible code |  |  | x |  |
| PHY VII | Fraunhofer High-bandwidth PHY | x | x |  |  |
| PureLiFi Low-bandwidth PHY | x | x |  |  |

Table X2 shows that each PHY mode mainly supports what sorts of Rx.

Table X2 – PHY Modes / RXs

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | | Photodiode | | Image sensor | | | Other characteristics |
| Monochrome | Color | Global shutter | Rolling shutter | High-speed / ROI |
| PHY I | | x | x |  |  |  |  |
| PHY II | | x | x |  |  |  |  |
| PHY III | |  | x |  |  |  |  |
| PHY IV | UFSOOK | x | x | x |  | x |  |
| Twinkle VPPM | x | x |  |  | x |  |
| S2-PSK |  |  | x |  | x |  |
| S2+DMS-PSK |  |  | x |  | x |  |
| Offset-VPWM | x | x |  |  |  |  |
| PHY V | RS-FSK | x | x |  | x | x |  |
| Compatible M-FSK | x | x |  | x | x | low-grade camera support |
| C-OOK | x | x |  | x | x |  |
| Packet PPM/PWM | x | x |  | x | x |  |
| PHY VI | 2D-sequential color code |  |  | x |  | x |  |
| Sequential Scalable 2D Code |  |  | x | x | x |  |
| VTASC | x | x | x | x | x |  |
| Invisible Data embedding |  |  | x | x | x |  |
| M-PSK | x | x | x | x | x |  |
| M-FSK | x | x | x | x | x |  |
| SS (Spread Spectrum) | x | x | x | x | x |  |
| Kookmin Invisible code |  |  | x | x | x |  |
| PHY VII | Fraunhofer High-bandwidth PHY | x | x |  |  |  |  |
| PureLiFi Low-bandwidth PHY | x | x |  |  |  |  |