**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **OCC Operating Modes – Table Revision** |
| Date Submitted | [August 2017] |
| Source | Jaesang Cha(SNUST), Kim Chan(SNUST), Soonho Jung(SNUST), Sooyoung Chang(CSUS), Seongjin Choi(SNUST) , , Vinayagam Mariappan(SNUST) |
| Re: |  |
| Abstract | Discussion on D3 comments’ resolution revision |
| Purpose | Resolution for D3 technical comments revision |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

# #1: PHY IV, V, and VI Operating Mode Tables

**Table 81 - PHY IV, V and VI Operating Modes**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Modulation**  **(phyOccMcsID)** | **RLL**  **(phyOccRLLCode)** | **Optical Clock Rate**  **(phyOccOpticalClockRate)** | **FEC**  **(phyOccFEC)** | **Bit Rate** |
| UFSOOK | NA | multiple of frame rate | MIMO path dependent | (1/2)\*(code rate)\*Frame Rate) |
| Twinkle VPPM | NA | 4x bit rate | RS(15, 11) | 4 kbps |
| S2-PSK | Differential code | 10 Hz | Temporal error correction | 5 bps |
| S8-PSK | Grey code | 10 Hz | Temporal error correction | 30 bps |
| HS-PSK | ½ code rate for S2-PSK; None for DS8-PSK | 10 kHz | Temporal error correction;  Outer FEC with GF(16) | 22 kbps |
| Offset-VPPM | None | 25Hz | RS(15,2) / RS(15,4) / None | 18bps  (FEC None) |

**Table 81 - PHY IV, V and VI Operating Modes (Continued)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Modulation**  **(phyOccMcsID)** | **RLL**  **(phyOccRLLCode)** | **Optical Clock Rate**  **(phyOccOpticalClockRate)** | **FEC**  **(phyOccFEC)** | **Bit Rate** |
| NS-FSK | None | 30 Hz | XOR FEC | 60/90 bps |
| C-OOK | Manchester/ 4B6B | 2.2 kHz/ 4.4 kHz | Temporal error correction  (DS rate=100/ DS rate=60) | 60/150/580/700 bps |
| CM-FSK | None | 10 Hz | Temporal error correction | 40/50/60  bps |
| Packet PWM/PPM | None | 100 kHz | Temporal error correction | 5.5/ 8 kbps |

**Table 81 - PHY IV, V and VI Operating Modes (Continued)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Modulation**  **(phyOccMcsID)** | **RLL**  **(phyOccRLLCode)** | **Optical Clock Rate**  **(phyOccOpticalClockRate)** | **FEC**  **(phyOccFEC)** | **Bit Rate** |
| A-QL | None | 10 Hz | Hamming (11,15)/ None | 5.28/ 7.56 kbps  (16x16 cells) |
| HA-QL | Differential code | 10 Hz | Hamming (11,15)/ None | 220/ 300 bps  (8x8 cells) |
| VTASC | None | 30 Hz | RS(64,32)/ RS(160,128)/ None | 512 Kbps  (FEC None) |
| SS2DC | None | 30 Hz | RS(64,32)/ RS(160,128)/ None | 368 Kbps  (FEC None) |
| IDE-MPFSK- BLEND | None | 30 Hz | RS(64,32)/ RS(160,128)/ None | 32 Kbps  (FEC None) |
| IDE-WM | None | 30 Hz | RS(64,32)/ RS(160,128)/ None | 128 Kbps  (FEC None) |