**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **Frequency Band Layout** |
| Date Submitted | [16 Jan, 2020] |
| Source | Frederick SmithChevron[address] | Voice: +1-661-332-8214Fax: E-mail: smithfh@chevron.com |
| Re: | Task Group 802.15.16t Requirements Discussion |
| Abstract | Frequency Band Layout for Sample Frequencies |
| Purpose | Facilitate discussion of System Level Requirements for 802.16t |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

|  |  |
| --- | --- |
| **Frequency Band** | **450 to 470MHz** |
| **Defined Channel widths** | **6.25, 12.5KHz,25KHz** |
| **Std. TX / RX Offset of Mobile Tx** |  **+5 MHz** |
| **Stacking sheme of duplex channel pairs** | **450.0125/455.0125--->454.9875/459.9875;460.0125/465.0125------>464.9875/469.9875** |
|   |   |
| **Frequency Band** | **150 to 174MHz** |
| **Defined Channel widths** | **6.25, 12.5KHz,25KHz** |
| **Std. TX / RX Offset of Mobile Tx** | **None** |
| **Stacking sheme of duplex channel pairs** | **None** |
|   |   |
| **Frequency Band** | **806 to 817, and 851-866MHz** |
| **Defined Channel widths** |  **6.25?,12.5KHz,25KHz** |
| **Std. TX / RX Offset of Mobile Tx** |  **-45MHz** |
| **Stacking sheme of duplex channel pairs** | **a standard 10 channel block 851.0125/806.0125;852.0125/807.0125, 853.0125/808.0125, etc.and then then next 10 channel block 851.0375/806.0375;852.0375/807.0375,853.0375/808.0375, etc** |
|   |   |
| **Frequency Band** | **896 to 901, and 935-940MHz** |
| **Defined Channel widths** |  **12.5KHz** |
| **Std. TX / RX Offset of Mobile Tx** |  **-39MHz** |
| **Stacking sheme of duplex channel pairs** | **a standard 10 channel block 935.00625/896.00625;935.01875/896.01875, 935.03125/896.03125 etc.and then then next 10 channel block 935.13125/896.13125, 935.14375/896.14375** |
|   |   |
| **Frequency Band** | **952-953, and 928-929MHz** |
| **Defined Channel widths** |  **12.5KHz** |
| **Std. TX / RX Offset of Remote Tx** |  **-24MHz** |
| **Stacking sheme of duplex channel pairs** | **952.00625/928.00625, 952.01875/928.01875, etc.** |