**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | Suggested Changes for Pulse Shaping Section 16.4.5  |
| Date Submitted | 26 February 2020 [presented at the CRG call on 2020/02/22] |
| Source | Jochen Hammerschmidt (Apple Inc.),  | J\_hammerschmidt@yahoo.com |
| Re: | Contribution to TG4z for IEEE 802.15.4z regarding pulse shape  |
| Abstract | Contribution to TG4z amendment of IEEE Std 802.15.4-2015 |
| Purpose | This submission proposes text to for the IEEE Std 802.15.4z draft amendment to IEEE Std 802.15.4.  |
| Notice | This document does not represent the agreed views of the IEEE 802.15 Working Group or IEEE 802.15.8 Task Group. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |
| Patent Policy | The contributor is familiar with the IEEE-SA Patent Policy and Procedures:<http://standards.ieee.org/guides/bylaws/sect6-7.html#6> and<http://standards.ieee.org/guides/opman/sect6.html#6.3>.Further information is located at <http://standards.ieee.org/board/pat/pat-material.html> and<http://standards.ieee.org/board/pat>. |

|  |
| --- |
| EXTRA NOTE(s): n/a |

**BACKGROUND / INTRODUCTION:**

This documents follows up on presentation 15-20-0084-00-004z, by providing first concrete suggestions to further update pulse shaping section 16.4.5.

Note that this material was presented and reviewed in the TG 4z CRG call on Monday Feb 22, 2020.

**16.4.5 Baseband impulse response**

*[further suggestion insertion after formerly approved insertion]*

For reference purposes, the operation of an ERDEV in particular should furthermore include a transmit mode in which each transmitted pulse *p(t)* closely follows the above mathematical formula of the root raised cosine reference pulse *r(t)* for a specific roll-off factor of beta=0.45 over at least +/- 4 chip intervals. The deviation of the baseband transmit pulse *p(t)* relative to the maximum peak amplitude of the reference pulse *r(t)* with beta=0.45 in this mode should be less than TBD % over the pulse duration,

*|p(t) – r(t, beta=0.45)| / max(|r(t)|) < TBD %, for all t = +/-4T*

Besides, an ERDEV shall be equipped to know and communicate to peer ERDEVs its own exact transmit pulse shape; correspondingly, an ERDEV shall be able to obtain a peer ERDEV’s transmit pulse shape and configure its receiver algorithms for time-of-flight extraction with this information. To that end, the pulse shape utilized by an ERDEV transmitter may be communicated between peer ERDEVs via an offline procedure, and/or during in-band and/or out-of-band connection setup steps, and/or via real-time messaging.

***[END]***