|  |  |
| --- | --- |
| Project | **IEEE 802.15 Wireless Specialty Networks Working Group <**<http://ieee802.org/15>**>** |
| Title | **IEEE 802.15.16t Draft Proposal - System Requirements Document**  |
| Date Submitted | **2021-01-19** |
| Source(s) | Menashe Shahar (Ondas Networks) | Voice: E-mail:  |
| Re: | 16t Task Group: Licensed Narrowband Amendment |
| Abstract | System Requirements Document – Draft Proposal |
| Purpose | To develop System Requirements for 802.16t  |
| Notice | *This document does not represent the agreed views of the IEEE 802.16 Working Group or any of its subgroups*. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion. It is not binding on the contributor(s), who reserve(s) the right to add, amend or withdraw material contained herein. |
| Copyright Policy | The contributor is familiar with the IEEE-SA Copyright Policy <http://standards.ieee.org/IPR/copyrightpolicy.html>. |
| Patent Policy | The contributor is familiar with the IEEE-SA Patent Policy and Procedures:<<http://standards.ieee.org/guides/bylaws/sect6-7.html#6>> and <rmation is located at <<http://standards.ieee.org/board/pat/pat-material.html>> and <<http://standards.ieee.org/board/pat>>. |

IEEE 802.16t System Requirements Document

R8

January 19, 2021

## Introduction

This document is to summarize the performance requirements for IEEE 802.16 operation in channel bandwidths greater than or equal to 5 kHz and less than 100 kHz. This SRD will act as a guide for the development of an amendment to IEEE Std 802.16-2017. This amendment builds on the 802.16s Amendment completed in 2017 and incorporated in the revision IEEE Std 802.16-2017

The following terminology is used in this document:

SHALL: This word, or the terms "REQUIRED" or "MUST", mean an absolute requirement of the specification.

SHALL NOT: This phrase means an absolute prohibition of the specification.

SHOULD: This word, or the adjective "RECOMMENDED", mean that there may exist valid reasons in particular circumstances to ignore a particular item, but the full implications must be understood and carefully weighed before choosing a different course.

SHOULD NOT: This phrase, or the phrase "NOT RECOMMENDED" mean that there may exist valid reasons in particular circumstances when the particular behavior is acceptable or even useful, but the full implications should be understood and the case carefully weighed before implementing any behavior described with this label.

MAY: This word, or the adjective "OPTIONAL", mean that an item is truly optional. One vendor may choose to include the item because a particular marketplace requires it or because the vendor feels that it enhances the product while another vendor may omit the same item. An implementation which does not include a particular option MUST be prepared to interoperate with another implementation which does include the option, though perhaps with reduced functionality. In the same vein an implementation which does include a particular option MUST be prepared to interoperate with another implementation which does not include the option (except, of course, for the feature the option provides.)

# Markets and Use Cases

The following markets and use cases were identified in [IEEE 802.15-20-0108r0](https://mentor.ieee.org/802.15/dcn/20/15-20-0111-00-016t-april-9-2020-teleconference-presentation.pptx)

|  |  |  |
| --- | --- | --- |
| **Market** | **Use Case/Application** | **Sub-Application** |
| Drone | UAS CNPC RADIO LINK |   |
| Oil/Gas | Pump Off Controller |   |
| Oil/Gas | PtP IP Backhaul | LoRa WAN Gateway |
| Electric | PtP Analog Data Circuit replacement | Transfer Trip/EMS SCADA |
| Electric | Advanced Metering Infrastructure (AMI) |   |
| Electric | Volt/VAR Control (Capacitor banks) |   |
| Electric | Distribution Feeder Automation |   |
| Electric | Circuit Sensors |   |
| Electric | Advanced Solar Inverters |   |
| Electric | Remote Fault Indicators |   |
| Water | SCADA |   |
| Electric | Substation Monitoring Devices |   |
| Electric | Field Devices | Reclosers, Fault Circuit Indicators (FCIs), Switches, Access Points |
| Electric | AMI Collector |   |
| Electric | Substation |   |
| Electric | Distribution Sub SCADA |   |
| Electric | Distribution Sub Metering |   |
| Electric | AMI |   |
| Electric | Distribution Substation SCADA |   |
| Electric | Downline Distribution Automation | Cap bank controller |
|   |   |   |
| Rail | I-ETMS Positive Train Control | Periodic wayside status |
| Rail | I-ETMS Positive Train Control | Back office to loco |
| Rail | Locomotive Distributed Power |   |
| Rail | End-of-Train Communication |   |
| Rail | Wayside Maintenance |   |
| Rail | Central Traffic Controller Communication |   |
| Rail | Fault detector communication |   |
| Rail | Grade Crossing Communication | Activation |
| Rail | Grade Crossing Communication | Monitoring |
| Rail | Hy-rail Limits Compliance |   |
| Rail | Employee-in-charge |   |
| Rail | Worksite protection |   |
| Rail | On-board Sensor Network |   |
| Rail | Remote Control Locomotive |   |
| Rail | Drone Communication |   |
| Rail | Differential GPS |   |
| Rail | Wayside signaling | Wayside to Office |
| Rail | Wayside signaling | Wayside to Wayside (main/remote) |
| Rail | PTC-enabled crossing |   |
| Rail | Remote monitoring and systems mgmt | w/o video |
| Rail | Remote monitoring and systems mgmt | w/video |
| Rail | ACSES Train control | Loco to Office and Wayside |
| Rail | End-of-train (EOT)/Head-of-Train (HOT) |   |
| Rail | Local DTMF crossing activation |   |
| Rail | Defect detectors | Voice and data |

The standard should support this set of use cases for field area networks, and similar critical infrastructure industry applications, that require high reliability and availability.

## 802.16t Amendment Requirements

Amendment Requirements that must be specified in the amendment in order to meet the operational requirements. These requirements identify the gaps in the existing standard that must be addressed by the amendment in order to attain those capabilities.

**Topology:**

Support of the following topologies is required:

Network topology: Multicell and multisector

Sector topology: Point to Multipoint Point to Point topology will be supported as a private case of Point to Multipoint

 Repeater for range extension:

S&F on the same carrier frequency/carrier frequency pair

Use of distinct carrier frequency/carrier frequency pair.

Base Station Controller (BSC) for:

Seamless handover

 Coordination of base station operation to minimize self-interference.

A Base Station to Base Station Controller communication protocol to support the above functions will be standardized.

Consider impact of PTT one-way LMR on topology.

**Frequency Range**

While ieee802.16t does not require or exclude support for any specific frequency, the ieee802.16t air interface protocol will be optimized for the sub 1 GHz frequency range.

Band Support Requirements

See [IEEE 802.15-20-0055-04-016t-frequency-band-layout.xls](https://mentor.ieee.org/802.15/dcn/20/15-20-0055-03-016t-frequency-band-layout.xlsx)

(Proposed in 802.15-20-0050r0)

* Support operation in paired and unpaired continuous licensed bands available for private networks is required (e.g., AMTS, IVDS, 454 A2G, 700 MHz A-Block, RR 900 MHz, 1.4 GHz).
* Support for partition of continuous licensed bands into multiple channels is required for frequency reuse and link budget/coverage considerations.
* Support operation in Private Land Mobile Radio (PLMR) bands (e.g., RR160 MHz) is required. This includes:
* Support of common PLMR channel bandwidth: 6.25, 12.5, 25 and 50 kHz
* Support special PLMR channel bandwidth: 5, 7.5 and 15 kHz
* Support aggregation of multiple adjacent and non-adjacent PLMR channels to enable higher throughput services.

**Channel BW Range**

From PAR: “The amendment defines operation for channel bandwidths greater than or equal to 5 kHz and less than 100 kHz.”

Operation above 100 kHz is already supported and will not be changed in this amendment.

Proposed Additional requirements:

* A remote will operate over one or more adjacent or non-adjacent subchannels. The bandwidth of one subchannel is between 5 KHz and 25 KHz.
* A base station will operate over any one or more sub-channel. The base station must support aggregation of multiple subchannels such that the total bandwidth in the sector is at least 100 KHz.

**TDD Frame Configuration**

The standard shall support configurable TDD frame configuration including:

* Configuration of the downlink subframe duration
* The Configuration of the uplink subframe duration
* The duration of the transmit to receive and the receive to transmit gaps duration.

The standard shall support a range of TDD frame durations consistent with throughput, latency, frequency utilization and overhead requirements defined in this document.

The standard shall support a range of downlink to uplink subframe duration ratios between 10:1 to 1:10, Subject to frequency utilization an overhead requirement defined in this document.

The gaps duration should support the maximum distance requirement defined document.

**Duplexing Requirements**

The standard will support both TDD and FDD

(Proposed in 802.15-20-0050r0)

TDD will be used in unpaired spectrum and in paired spectrum if allowed by the applicable regulation authority. A highly asymmetrical or reverse asymmetrical DL:UL ratio (e.g., 1:10 to 10:1) should be supported.

HD-FDD or FDD will be used in paired spectrum if TDD is not allowed. HD-FDD will use the same framing as in TDD.

Framing requirement for FDD mode: TBD

**Mobility Requirements**

The standard shall support a relative speed of remote to base station of up to 614 mph.

The standard shall support seamless handover between base stations.

**Data transport requirements:**

(Proposed in 802.15-20-0050r0)

The standard will support concurrent operation of low, medium and high throughput endpoint devices with the following characteristics:

* Low- throughput end point requirements:
* End user throughput < 1 kb/s. Given the periodicity characteristics, this seems to be a peak throughput, not average.
* End to end latency: in most cases, not time sensitive. One use case requires end to end latency < 100 msec. Other use cases require end to end latency below 1 second or higher.
* # of endpoints per base station: up to 150[[1]](#endnote-1)
* Most use cases in this category are fixed but some are mobile.
* Most use cases in this category are reverse asymmetrical but some are symmetrical, and some are asymmetrical. UL:DL ratio is in the range 90:10 to 10:90.
* Medium- throughput end point requirements:
* 1 kb/s < end user throughput < 10 kb/s
* End to end latency < 60 ms
* End to end jitter < 20 ms
* # of end points per sector < 60
* Fixed and mobile use cases. Some of the use cases, require high speed support.
* UL:DL ratio in the range 90:10 to 30:70
* High- throughput use cases characteristics.
* TBD

Specific use cases are summarized in …..

Additional general data transport requirements:

* Frequency utilization: up to 3 bits/sec/Hz (user data frequency utilization) subject to receiver sensitivity requirement.
* Air interface protocol overhead:
	+ PHY layer excluding FEC: < 10%
	+ MAC overhead: < 10%

**Predictable Performance:**

(Proposed in 802.15-20-0050r0)

Licensed band (mandated by the PAR)

Central scheduling

QOS

**Range (DL or UL) and Coverage Requirements:**

(Proposed in 802.15-20-0050r0)

Long range single hop coverage (e.g., up to 50+ miles cell radius):

Some railroad use cases currently experience signal coverage up to 100 miles .

Unmanned Aviation Use Case has a maximum cell radius of 200+ miles

Receiver sensitivity requirement

TDD frame structure requirements (related to efficiency and time for TDD guard interval?)

**Endpoints:**

(Proposed in 802.15-20-0050r0)

Support for 1000’s of endpoint devices per sector (known as “massive connectivity”) in a Point to Multi-Point architecture

An example of massive connectivity requirement includes rapid reconnection of all remotes in a sector after a base station failure has occurred. Reconnection time depends on use case.

**Advanced Antenna Systems:**

Unmanned Aviation use case intends to utilize Beam Steering antennas (would apply aviation spectrum and C-band - 5031-5090 ) Support for Beam Steering is a requirement for the standard.

 Practicality depends on operational band. There should be no impact if the feature is not used.

**Coexistence with PLMR channels operating with other standards**

Support of analog voice/data coexistence in low utilization voice channels. Voice will have priority over data. The voice may carried as analog, NXDN, P.25, etc.

**Cyber Security**

High Security is a requirement.

Example requirements coming from

* + IEC-62443, CR 1.2
	+ CIP 005-5, R-1.2
	+ DO-377 SER-08, SER-16, SER-17

Main feature required:

# FIPS required cryptographic functions

Encryption/decryption

|  |  |  |
| --- | --- | --- |
| Algorithm | Mode | Approved key lenght |
| AES (NIST.FIPS.197) | CBC (NIST.SP.800-38A) | 128, 192, 256 |
|  | CCM (NIST.SP.800-38C) | 128, 192, 256 |
|  | GCM (NIST.SP.800-38D) | 128, 192, 256 |
|  | XTS-AES (NIST.SP.800-38E) | 128, 192, 256 |
|  | CBC with key wrapping (NIST.SP.800-38F) | 128, 192, 256 |
| TDEA (3-DES)NIST.SP.800-67r2 | CBC (NIST.SP.800-38A) | Disallowed after 2023 |
|  | CBC with key wrapping (NIST.SP.800-38F) | Disallowed after 2023 |

Digital signature functions

|  |  |
| --- | --- |
| Algorithm | Mode / key length |
| SHA-2 family (NIST.FIPS.180-4) | SHA224, SHA-256, SHA-384, SHA-512, SHA-512/224 and SHA-512/256 |
| SHA-3 family (NIST.FIPS.202) | SHA3-224, SHA3-256, SHA3-384, and SHA3-512 |
| RSA | Key length: 2048 or higher |

Message authentication functions

|  |  |
| --- | --- |
| Algorithm | Mode / key length |
| HMAC | 112 bits or higher |
| CMAC – 3DES | Disallowed after 2023 |
| CMAC – AES |  |
| GMAC – AES |  |
| KMAK | 112 bits or higher |

1. The number of endpoints per base station depends on the base station coverage which may be increased to reduce infrastructure cost. [↑](#endnote-ref-1)