**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **D1-PHY VII specifications** |
| Date Submitted | March 2022 |
| Source | Huy Nguyen, Md. Shahjalal, and Yeong Min Jang(Kookmin University) | Voice: [ ]Fax: [ ]E-mail: [yjang@kookmin.ac.kr] |
| Re: | [If this is a proposed revision, cite the original document.][If this is a response to a Call for Contributions, cite the name and date of the Call for Contributions to which this document responds, as well as the relevant item number in the Call for Contributions.][Note: Contributions that are not responsive to this section of the template, and contributions which do not address the topic under which they are submitted, may be refused or consigned to the “General Contributions” area.] |
| Abstract | [Description of document contents.] |
| Purpose | [Description of what the author wants P802.15 to do with the information in the document.] |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

# 16. PHY VII specifications

## 16.1. RS-OFDM

The Rolling Shutter Orthogonal Frequency Division Multiplexing (RS-OFDM) Modulation for high-speed OCC system uses the PHY VII – Singular Point Source.

The PHY VII Operating Modes system specifications are given in Table xxx. The additional PHY Operating Modes by RS-OFDM for Smart Device is presented the Table xxx – PHY VII Operating Modes.

**Table xxx – PHY VII Operating Modes**

|  |  |
| --- | --- |
| **PHY Operating Modes** |  |
| **Modulation** | **RLL Code** | **Optical Clock Rate** | **FEC** | **OFDM symbol length** | **Data rate** |
| RS-OFDM | None | 20 kHz | Hamming (15,11) | 64 | 1.92 kbps |
| 40 kHz | RS (15,11) | 128 | * 1. bps
 |

### *16.1.1. Reference architecture*

A reference architecture to implement RS-OFDM is shown in Figure xxx



Figure xxx. Rolling Shutter OFDM block diagram

### *16.1.2. Encoder configuration*

A packet of data is modulated using OFDM modulation. The optical clock rate is at 20 kHz or 40 kHz. The optical clock rate at which RS-OFDM symbols are clocked out is configurable over PHY PIB attribute *phyOfdmOpticalClockRate*.



Figure xx. RS-OFDM data packet structure

The data packet structure is as shown in Figure xx. A packet consists of multiple similar data sub-packets to avoid missing data between adjacent images' gap time.

### *16.1.3. Hermitian Mapping*

Unlike the conventional OFDM in Radio Frequency, instead of feeding the data symbol directly into the IDFT block, each symbol must pass through the Hermitian block. The signal is then fed into the IFFT. The special purpose of the Hermitian block is that it ensures the output of the IDFT is entirely real. The modes of RS-OFDM shall be configured via the PHY PIB attribute *phyOfdmMode.* And the length of RS-OFDM symbol shall be configured via the PHY PIB attribute *phyOfdmFrame.*

### *16.1.4. Sequence Number inserting*

The data sub-packet payload shall consist of two subparts: SN data, payload. The SN Data consists of asynchronous information, which helps the receiver side decode data. SN shall be implemented over the PHY PIB attribute *phyOfdmSn*

### *16.1.5. Forward error correction (FEC)*

The data sub-packet payload may be coded by FEC to protect the payload from error. Hamming (8,4) or Reed Solomon (15,11) code may be used as an FEC. FEC shall be configured via the PHY PIB attribute *phyOfdmFEC*

Table xx shows PHY PIB attributes.

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute** | **Type** | **Range** | **Description** |
| *phyOfdmOpticalClockRate* | Integer | 0-7 | The optical clock rate (or symbol rate)applied for OFDM.0: 8 kHz1: 10 kHzOthers: Reserved |
| *phyOfdmMode* | Integer | 0-3 | This specifies the mode of OFDMmodulation.0: DCO-OFDM1: ACO-OFDMOther values: Reserved |
| *phyOfdmFec* | Integer | 0-7 | This attribute specifies FEC for OFDM modulation.0: None1: FEC: Hamming (8/4)2: FEC: Hamming (15/11)3: FEC: RS(15,11)Other values: Reserved |
| *phyOfdmFrame* | Integer | 0-3 | This attribute specifies the symbol length of OFDM frame.0: 321: 64Other values: Reserved |
| *phyOfdmSn* | Integer | 0-3 | This attribute specifies the length of Sequence Number per packet of OFDM0: 2 bits1: 3 bits Other values: reserved |

## 16.2. MIMO C-OOK

The Multiple Input Multiple Output Camera On-Off Keying (MIMO C-OOK) Modulation for high-speed OCC system uses the PHY VII – Multiple Point Source.

The PHY VII Operating Modes system specifications are given in Table 151. The additional PHY Operating Modes by MIMO C-OOK for Smart Device is presented the Table 151 – PHY VII Operating Modes.

**Table 151 – PHY VII Operating Modes**

|  |
| --- |
| **PHY Operating Modes** |
| **Modulation** | **RLL Code** | **Optical Clock Rate** | **FEC** | **Data Rate** **(two LEDs)** |
| MIMO C-OOK | Manchester  | 8 kHz | Hamming (15,11) | 4.8 kbps |
| 4B6B | 8 kHz | RS (15,11) | 7.2 kbps |
| Manchester | 10 kHz | Hamming (15,11) | 6.0 kbps |
| 4B6B | 10 kHz | RS (15,11) | 9.0 kbps |

### *16.2.1. Reference architecture*

The PHY VII with supported data rates and operating conditions is shown in Table 151 – PHY VII Operating Modes for Multiple Input Multiple Output Camera On-Off Keying (MIMO C-OOK) Modulation with high-speed OCC system uses the PHY VII - Multiple Point Source.

The proposed Multiple Input Multiple Output Camera On-Off Keying (MIMO C-OOK) was designed with the following characteristics:

* Modulation methods include line coding (Manchester code and 4B6B)
* The Optical clock rate is at 8 kHz or 10 kHz
* Sequence Number part was put in the head and tail of packets
* Multiple light sources were applied to increase the data rate

A reference architecture to implement MIMO C-OOK is shown in Figure 217



Figure 217. MIMO C-OOK block diagram

### *16.2.2 Encoder configuration*

A packet of data is modulated using OOK modulation. The optical clock rate is at 8 kHz or 10 kHz. The optical clock rate at which MIMO C-OOK symbols are clocked out is configurable over PHY PIB attribute *phyMimoCookOpticalClockRate.*



Figure 218. MIMO C-OOK data packet structure

The data packet structure is as shown in figure 218. A packet consists of multiple similar data sub-packets to avoid missing data between adjacent images' gap time. The number of repetitions depends on the communication mode specified later. The configuration of preamble shall be implemented over the PHY PIB attribute *phyMimoCookPreambleSymbol*.

Table 152—Data sub-packet format

|  |  |
| --- | --- |
| **Preamble** | **Data sub-packet payload** |
| **Start SN data****(Sequence Number)** | **Payload** | **End SN data****(Sequence Number)** |
| 011100  | Manchester coding |
| 0011111000  | 4B6B coding |

### 16.2.3 RLL coding

The data sub-packet payload shall consist of three subparts: the Start SN data, payload, and the End SN Data. The Start SN Data and the End SN Data shall carry the same information, which consists of the asynchronous information. SN shall be implemented over the PHY PIB attribute *phyMimoCookSn*

### 16.2.4 Forward error correction (FEC)

The data sub-packet payload may be coded by FEC to protect the payload from error. Hamming (8,4) or Reed Solomon (15,11) code may be used as an FEC. FEC shall be configured via the PHY PIB attribute *phyMimoCookFEC*

**Table xx shows PHY PIB attributes.**

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute** | **Type** | **Range** | **Description** |
| *phyMimoCookOpticalClockRate* | Integer | 0-7 | The optical clock rate (or symbol rate)applied for MIMO C-OOK.0: 8 kHz1: 10 kHzOthers: Reserved |
| *phyMimoCookRLLCode* | Integer | 0-7 | This specifies the RLL coding for MIMO C-OOKmodulation.0: Manchester1: 4B6B codingOther values: Reserved |
| *phyMimoCookFec* | Integer | 0-7 | This attribute specifies FEC for MIMO C-OOKmodulation.0: None1: Hamming (8/4)2: Hamming (15/11)3: Hamming (8/4),Other values: Reserved |
| *phyMimoCookPreambleSymbol* | Integer | 0-3 | This attribute specifies the preamblesymbol of PSDU of MIMO C-OOK.0: 6B symbol (preamble = 011100)1: 10B symbol (preamble = 0011111000)2–3: Reserved |
| *phyMimoCookSn* | Integer | 0-3 | This attribute specifies the length of Sequence Number per packet of MIMO C-OOK0: 2 bits1: 3 bits 2-3: reserved |

## 16.3. O-NOMA

The Optical Non-orthogonal multiple access (O-NOMA) Modulation for high-speed OCC system uses the PHY VII – Singular Point Source.

The PHY VII Operating Modes system specifications are given in Table xxx. The additional PHY Operating Modes by O-NOMA for Indoor applications is presented the Table xxx – PHY VII Operating Modes.

|  |
| --- |
| **PHY Operating Modes** |
| **Modulation** | **Number of power levels** | **Optical Clock Rate** | **FEC****(Reed Solomon)** | **Data Rate**  |
| MIMO-OOK | 2 | 2 kHz | RS (15,11) | 1.5 kbps |
| 3 | 4 kHz | RS (15,11) | 3 kbps |

### *16.3.1. Reference architecture*

A reference architecture to implement O-NOMA is shown in Figure xxx



Figure xxx. O-NOMA block diagram

### *16.3.2. Encoder configuration*

A packet of data is modulated using O-NOMA modulation. The optical clock rate is at 2 kHz or 3 kHz. The optical clock rate at which O-NOMA symbols are clocked out is configurable over PHY PIB attribute *phyNomaOpticalClockRate.*

The number of power levels of O-NOMA scheme will be configurable over PHY PIB attribute *phyNomaMode.*



Figure xxx. Data encoding scheme of 2-stage power allocation based NOMA-OCC system

### *16.3.3. Forward error correction (FEC)*

The data sub-packet payload may be coded by FEC to protect the payload from error. Hamming (8,4) or Reed Solomon (15,11) code may be used as an FEC. FEC shall be configured via the PHY PIB attribute *phyNomaFEC*

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute** | **Type** | **Range** | **Description** |
| *phyNomaOpticalClockRate* | Integer | 0-7 | The optical clock rate (or symbol rate)applied for O-NOMA.0: 2 kHz1: 3 kHzOthers: Reserved |
| *phyNomaMode* | Integer | 0-7 | This specifies the number of power levels for O-NOMAmodulation.0: 21: 3Other values: Reserved |
| *phyNomaFec* | Integer | 0-7 | This attribute specifies FEC for O-NOMAmodulation.0: None1: Hamming (8/4)2: Hamming (15/11)3: Hamming (8/4),4: Hamming (15/11)Other values: Reserved |

## 16.4. MIMO-OOK

The Multiple Input Multiple Output On-Off Keying (MIMO-OOK) Modulation based on RoI signaling for Optical IoT system uses the PHY VII – Multiple Point Source.

The PHY VII Operating Modes system specifications are given in Table 153. The additional PHY Operating Modes by MIMO-OOK for Smart Device is presented the Table 155– PHY VII Operating Modes.

**Table 155 – PHY VII Operating Modes**

|  |
| --- |
| **PHY Operating Modes** |
| **Modulation** | **RLL Code** | **Optical Clock Rate** | **FEC** | **Data Rate** **(two LEDs)** |
| MIMO-OOK | Manchester  | 20 Hz | RS (15,11) | 40 bps |
| 4B6B | 20 Hz | RS (15,11) | 53 bps |
| Manchester | 30 Hz | RS (15,11) | 60 bps |
| 4B6B | 30 Hz | RS (15,11) | 80 bps |

### *16.4.1. Reference architecture*

A reference architecture to implement MIMO-OOK is shown in Figure 217



Figure 217. MIMO-OOK block diagram

### *16.4.2. Encoder configuration*

A packet of data is modulated using OOK modulation. The optical clock rate is at 20 Hz or 30 Hz. The optical clock rate at which MIMO-OOK symbols are clocked out is configurable over PHY PIB attribute *phyMimoOokOpticalClockRate.*



Figure xx. MIMO-OOK data packet structure

The data packet structure is as shown in Figure xx. The clock rate of the MIMO-OOK scheme was set up lower than (at least two times) the camera frame rate to eliminate the variation effect of frame rate.

To access multiple light sources, we have added the node ID part to each frame. Each user will be defined by a unique ID, so that the receiver can categorize the signal from different users. Defining users by ID nodes helps the system accept dozens of users, up to hundreds of users.

Table 152—Data sub-packet format

|  |  |
| --- | --- |
| **Preamble** | **Data sub-packet payload** |
| **LED-ID** | **Payload** |
| 011100  | Manchester coding |
| 0011111000  | 4B6B coding |
| 00011111110000 | 8B10B coding |

### *16.4.3. RLL coding*

RLL coding shall be applied in the payload subfield to maintain an average brightness at 50%. Manchester code and 4B6B code are suggested for OOK mode. The configuration of RLL code shall be implemented over the PHY PIB attribute *phyMimoOokRLLCode*. Manchester code and 4B6B code are suggested for MIMO-OOK mode.

### *16.4.4. Forward error correction (FEC)*

The data sub-packet payload may be coded by the inner FEC to protect the payload from error. Hamming (8,4) or (15,11) code may be used as an inner FEC.

Additionally, outer FEC may also be used to protect the PHR and PSDU. When outer FEC is enabled, RS(15,11) shall be implemented.

FEC shall be configured via the PHY PIB attribute *phyMimoOokFEC*

Both inner FEC and outer FEC shall be configured via the PHY PIB attribute *phyMimoOokFEC*.

**Table xx shows PHY PIB attributes**

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute** | **Type** | **Range** | **Description** |
| *phyMimoOokOpticalClockRate* | Integer | 0-7 | The optical clock rate (or symbol rate)applied for MIMO-OOK.0: 20 Hz1: 30 HzOthers: Reserved |
| *phyMimoOokRLLCode* | Integer | 0-7 | This specifies the RLL coding for MIMO C-OOKmodulation.0: Manchester1: 4B6B coding2: 8B10B codingOther values: Reserved |
| *phyMimoOokFec* | Integer | 0-7 | This attribute specifies FEC for MIMO-OOKmodulation.0: None1: Hamming (8/4)2: Hamming (15/11)3: Hamming (8/4),4: Hamming (15/11)Other values: Reserved |
| *phyMimoOokPreambleSymbol* | Integer | 0-7 | This attribute specifies the preamblesymbol of PSDU of MIMO-OOK.0: 6B symbol (preamble = 011100)1: 10B symbol (preamble = 0011111000)2**: 14B symbol (preamble=****00011111110000)**Other values: Reserved |
| *phyMimoOokLedId* | Integer | 0-3 | This attribute specifies the length of LED-ID data for MIMO-OOK0: 2 bits1: 3 bitsOther values: Reserved |