**IEEE P802.15**

**Wireless Specialty Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Specialty Networks (WSNs) |
| Title | SSBD Technical Specification Framework Contribution |
| Date Submitted | 02 September 2021 |
| Source | Benjamin Rolfe (Blind Creek Associates), Dries Neirynck (Ultra-radio), Frederic Nabki (Spark), Frank Leong (NXP) | E-mail: [ben.rolfe @ ieee.org ]  |
|  |  |  |
| Re: | Developing technical content  |
| Abstract | This document provides proposed text for the TFD add the SSBD channel access method.  |
| Purpose | Support development of technical content for the draft |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

Spectrum Sensing Based Deferral

Technical Specification Framework Contribution

# Overview

## Purpose

This contribution provides proposed text to support addition of the Spectrum Sensing Based Deferral (SSBD) to the 802.15.4 channel access methods. It is intended to be an optional feature. This contribution has been developed to support latency constrained use of the UWB PHYs, but is also suitable for use with any PHY in which the non-exponential backoff and optional alternative channel access method is useful. The SSBD algorithm itself is not dependent upon the PHY type. It assumes the PHY supports CCA mode 1, energy above threshold, with the proposed modifications contained in this document.

SSBD operation and motivation is explained in reference [1].

This document provides (only) a starting point for developing draft text.

# References

1. Spectrum Sensing Based Deferral (SSBD) channel access, <https://mentor.ieee.org/802.15/dcn/22/15-22-0485-01-04ab-ssbd-channel-access.pptx>

# Definitions, acronyms, and abbreviations

## Definitions

None

## Acronyms and abbreviations

SSBD – Spectrum Sensing Based Deferral

# Format conventions

No proposed text

# General description

Add the following in Clause 5:

Spectrum sensing based deferral (SSBD) Overview of SSBD (goes into clause 5)

For applications that use the UWB PHY where channel access latency needs to be bounded, the Spectrum sensing based deferral channel access method is provided. SSBD is described in clause 6.2.5.x. The key elements of SSBD include:

* The energy detect threshold can be variable and adjusted based on channel conditions
* The duration of sensing the channel during CCA can be variable and adjusted based on channel conditions or local requirements.
* Deferral on CCA busy is provided, with random delay and linear back-off to bound channel access latency.
* To provide for bounding channel access latency, after a configurable number of CCA attempts the algorithm can revert to Aloha – proceed as if the channel is idle and continue with transmission of the frame (i.e. as if CCA Mode 4 was used).

# MAC Functional Description

*Insert new subclause in 6.2.5:*

6.2.5.x Spectrum sensing based deferral (SSBD)

Spectrum sensing based deferral (SSBD) can be used for channel access where bounding latency in the channel access is desired.  SSBD is optional in all device types.  SSBD may be used for unscheduled random access or with one of the scheduled access schemes.  SSBD employs channel sensing using CCA and bounded deferral using linearly growing random backoff at each deferral.

The timing and behaviour of SSBD is controlled by the attributes *macMinBf*, *macMaxBf*, *macMaxSSBDBackoffs* and *macSSBDBOEndAction* (see 8.4.3).

Figure 6-<ssbd1> illustrates the steps of the SSBD algorithm.  When the algorithm ends in “Success” the MAC shall commence transmission of the frame.  Otherwise the algorithm terminates and the MAC shall abandon the transmission and report channel access failure.

 

Figure 6-<ssbd1> SSBD algorithm

When performing the SSBD algorithm, the variables NB and BF are maintained.  NB is the number of times the SSBD algorithm was required to backoff due to channel busy condition. NB shall be initialized to zero for each new SSBD attempt. BF is the backoff factor. Prior to each CCA, the algorithm shall delay for a random delay value between 0 and 2\*BF, using the backoff period defined by *aSSBDUnitBackoffPeriod*. BF which shall be initialized to  *macMinBf* for each new SSBD attempt. When CCA returns busy, NB and BF shall be incremented and the backoff executed.

The algorithm shall terminate with Success when CCA returns idle.  The action when NB exceeds *macMaxSSBDBackoffs* depends on the value of *macSSBDBOEndAction*:  when set to TXonEnd, the algorithm shall end with Success.   When the value of *macSSBDBOEndAction* is FailOnEnd, the algorithm shall end with Failure.

When used for SSBD, and CCA Mode 1 or Mode 3 are used, the CCA threshold shall be set to phyCcaEDthreshold and the CCA detection time shall be set to *phyCcaDuration*.

8.4.2 MAC constants

Insert the following constants into table 8-93 in order:

|  |  |  |
| --- | --- | --- |
| Constant  | Description   | Value  |
|  |  |  |
|   |  |    |

Insert the following attributes into table 8-94 in order:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute  | Type  | Range  | Description  | Default  |
| *macMaxBf*  | Integer  | 1 - TBD  | The maximum value of the backoff factor (BF) in the SSBD algorithm as described in 6.2.5.x.  | 1  |
| *macMaxSSBDBackoffs*  | Integer  | 0 – TBD  | The maximum number of deferral iterations the SSBD algorithm will attempt before exiting.  | TBD  |
| *macMinBf*  | Integer  | 1 - *macMaxBf*  | The minimum value of the backoff factor (BF) in the SSBD algorithm as described in 6.2.5.x.  | TBD  |
| *macSSBDBOEndAction*  | Enumeration  | TxOnEnd, FailOnEnd  | Determines the termination result of the SSBD algorithm upon exceeding the maximum back-off count, as described in 6.2.5.x.   | TxOnEnd  |
| *macSSBDUnitBackoffPeriod*  | The unit time period use for deferral in the SSBD algorithm, in microseconds.  | TBD    |  |  |

10.2.8 Clear channel assessment (CCA)

Change the last paragraph of 10.2.8 as indicated:

The PHY PIB attribute phyCcaMode, as described in 11.3, shall indicate the appropriate operation mode. The CCA parameters are subject to the following criteria:

* Except for the SUN O-QPSK PHYs,  and when SSBD is being used, the ED threshold shall correspond to a received signal power of at most 10 dB greater than the specified receiver sensitivity for that PHY, or in accordance with local regulations. For the SUN O-QPSK PHY, the ED threshold shall comply with the specification in 21.5.13. When SSBD is being used, the ED threshold shall comply with the specification in 6.2.5.x.
* Except for the 920 MHz band PHYs and the RCC PHYs, and when SSBD is being used, the CCA detection time shall be equal to *aCcaTime*, as defined in as defined in Table 11-1. For the 920 MHz band, and the RCC PHYs, *phyCcaDuration* symbol periods shall be used. When SSBD is being used, the CCA detection time shall comply with the specification in 6.2.5.x.