**IEEE 802.15**

**Wireless Speciality Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Speciality Networks (WSNs) | |
| Title | Proposal for restructuring Chapter 4 of 802.153RevB | |
| Date Submitted | 13 November 2022 | |
| Source | Thomas Kürner  TU Braunschweig  Schleinitzstr. 22  38092 Braunschweig, Germany | Voice: +49 531 391 2416 Fax: +49 531 391 5192 E-mail: t.kuerner@tu-bs.de |
| Re: |  | |
| Abstract | Proposal for restructuring Chapter 4 of 802.153RevB | |
| Purpose | Resolving comments of LB191 | |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |

**Proposal for restructuring Chapter 4 of 802.153RevB**

**Starting Point:**

With amendment 15.3e the concept of parinet has been introduced in a addition to the already existing piconet. With the roll-up chapter 4 inherited a cnfsuing structure wrt parinet and piconet. There are aspects relevant for piconet only, relevant for pairnetsonly and relevant for both. In the following a restructuring is proposed using the following elements:

- Three types of section/subsection headlines are used:

- Sections/subsection relevant only for one of the two network have the term piconet or pairnet in the headline

- Sections/subsections relevant for both do not have the terms pairnet/piconet in the title

- A new section 4.1 is introduced mentioning the existence of two networks types

- The order of sections is partly rearranged

- Additional text is introduced, where necessary

Text in < > indicates, what has to b changed.

**Proposed new structure:**

4. General description

<Add new section> 4.1 Network Types

Devices can either be operated in a piconet or in a pairnet as defined in section 4.2 and 4.4.

4.2 What is a piconet?  
<keep text from former section 4.1>

<add current line 29 to the end of 4.1>

4.3 Components of a piconet

<keep text from former section 4.3>

4.4 What is a pairnet?  
<keep text from former section 4.2>

<add the following new sentence at the end of this section:>

The HRCP PHY and THz PHY are using a pairnet.

4.5 Components of a pairnet

<Reformulate the text of former section 4.4 as follows>:

An IEEE 802.15.3 pairnet consists of at most two DEVs as components. These two components are called PRC (pairnet coordinator) and PRDEV (pairnet device). A Beacon frame is transmitted from a PRC to allow a PRDEV to connect. Once a pairnet connection is established, the Beacon frame transmissions are turned off.

4.6 MAC Functionality

<keep text before section 4.5.1 of former section 4.5>

4.6.1 Coordination

<keep text of former section 4.5.1>

4.6.1.1 Starting a piconet

<keep text of former section 4.5.1.1 up to line 6 on page 42>

4.6.1.2 Starting a pairnet

<keep text of former section 4.5.1.1 starting from line 7 on page 42>

4.6.1.3 Handing over control of the piconet

keep text of former section 4.5.1.2 >

4.6.1.4 Creating a child piconet

keep text of former section 4.5.1.3 >

4.6.1.5 Creating a neigbor piconet

<keep text of former section 4.5.1.4 >

4.6.2 Ending a piconet

<keep text of former section 4.5.2 up to line 16 >

4.6.3 Ending a piconet with a dependent piconet involve

<keep text of former section 4.5.3 >

4.6.4 Ending a pairnet

<keep text of former section 4.5.2 starting form line 17 >

4.6.5 Association and disassociation in a piconet

<keep text of former section 4.5.4 starting up to line 11 >

4.6.5 Association and disassociation in a pairnet

<keep text of former section 4.5.4 line 12 >

4.6.6 Security Overview

<keep text of former section 4.5.5 >

4.6.7 The IEEE 802.15.3 superframe

<add new subsection:> 4.6.7.1 The IEEE 802.15.3 superframe for piconets

<keep text of former section 4.5.6 up to line 17 of page 45 >

<add new subsection:> 4.6.7.2 The IEEE 802.15.3 superframe for pairnets

<keep text of former section 4.5.6 from line 18 on >

4.6.8 Channel time management

<keep text of former section 4.5.7>

4.6.9 Data communications between DEVs <add “in the piconet”>

<keep text of former section 4.5.8>

4.6.10 Information discovery in the piconet

<keep text of former section 4.5.9>

4.6.11 Dynamic channel selection <add “in the piconet”>

<keep text of former section 4.5.10>

4.6.12 Power management

<keep text of former section 4.5.11>

4.6.13 Controlling transmit power in the piconet

<keep text of former section 4.5.12>

4.6.14 Superfame structure using quasi-omni mode <add “in mmW piconets”>

<keep text of former section 4.5.13>

4.6.15 Frame aggregation

<keep text of former section 4.5.14>

4.6.16 Beam forming <add “in the piconet”>

<keep text of former section 4.5.15>

4.6.17 Channel probing <add “in the piconet”>

<keep text of former section 4.5.16>

4.6.18 Unequal error protection (UEP) <add “in mmW piconets”>

<keep text of former section 4.5.17>

4.7 Characteristics of the 2.4 GHz PHY

<keep text of former section 4.6>

4.8 Characteristics of the mmWave PHY

<keep text of former section 4.7>

4.9 Characteristics of HRCP PHY

<keep text of former section 4.8>

4.10 Characteristics of THz PHY

<keep text of former section 4.9>

4.11 Conventions

<keep text of former section 4.10>

4.12 Concept of primitives

<keep text of former section 4.11>