Annex-x

Slot Configuration Profiles

# Introduction

This annex describes the 3 profiles of the slot configuration default, static, and mobile. Based on the a priori deployment scenarios one of them can be selected.

# Slot Profiles.

Bin is the basic building block of the slot, which is over a single subchannel, and the number of symbols varies based on the profile. All the profiles are given such that the slot contains the 48 data symbols maintaining the same data capacity, but the number of bins present in a slot varies.

## Default Profile.

Chart, box and whisker chart

Description automatically generated with medium confidence

Figure Default Profile Bin Structure

A picture containing diagram

Description automatically generated

Figure Default Profile Slot Structure

## Static Profile.

Graphical user interface

Description automatically generated with medium confidence

Figure Static Profile Bin Structure

A picture containing text, clock, screenshot

Description automatically generated

Figure Static Profile Slot Structure

## Mobile Profile.

Table

Description automatically generated with medium confidence

Figure Mobile Profile Bin Structure



Figure Mobile Profile Slot Structure