Table 6-334—Subchannel Group Relocation IE

|  |  |  |
| --- | --- | --- |
| Syntax | Size  (Bit) | Notes |
| SubchannelGroup Relocation IE () { | --- |  |
| New Subchannel group | 16 | Up to 512 subchannel groups |
| Unique Ranging Code | 8 | Code for ranging in new subchannel group |
| Ranging code | 8 | Initial ranging code to intimate which remote |
| } |  |  |