**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **Proposed Resolution for Comments #988** |
| Date Submitted | July 17, 2024 |
| Sources | Carlos Aldana (Meta)  |  |
| Re: |   |
| Abstract |  |
| Purpose | To propose resolution to comment with CID #988 for “P802.15.4ab™/Draft 1.0 Standard for Low-Rate Wireless Networks”  |
| Notice | This document does not represent the agreed views of the IEEE 802.15 Working Group or IEEE 802.15.4ab Task Group. It represents only the views of the participants listed in the “Sources” field above.It is offered as a basis for discussion and is not binding on the contributing individuals. The material in this document is subject to change in form and content after further study. The contributors reserve the right to add, amend or withdraw material contained herein. |

***Comment Index #988***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 988 | Technical | 71 | 10.38.7.3 | 13 | SSBD can be used to specify LBT behavior. Please add the following text: "Channel access using listen before talk shall be used for improved coexistence performance. When used for narrowband assist, SSBD shall use the following control attribute values:phyCcaDuration should be set as required by local regulations;macSsbdMinBf and macSsbdMaxBf shall be set to 0;macSsbdMaxBackoffs shall be set to 0;macSsbdTxOnEnd shall be set to FALSE;macSsbdPersistence shall be set to FALSE;phyCcaMode shall be set to 1 (energy above threshold)phyCcaEdThreshold shall be set to -67 dBm/MHz - Ptx for channels 0 to 49 and to -74 dBm/MHz - Ptx for channels 50 to 249, where Ptx is the equipment’s instantaneous transmit power in dBm." |  |

**Discussion**: There has been quite a bit of discussion on NB coexistence and various proposals have been made including LBT-based solution with a fixed EDT threshold and a duty-cycle limited no-LBT allowance.

This proposal allows for 2 options at the NB transmitter, where TXMAX\_power\_Regulatory is the max power allowed to be transmitted in the regulatory domain and Pcca\_dBm\_MHz is the CCA level is measured “per MHz”. The 2 options are as follows:

1. If Pcca\_dBm\_MHz <= EDT, then transmit up to TXMAX\_power\_Regulatory
2. If Pcca\_dBm\_MHz > EDT, then either
	1. do not transmit at TXMAX\_power\_Regulatory OR
	2. transmit up to Ptx using the formula below:

Ptx < = max(TXMAX\_power\_Regulatory, -67-Pcca\_dBm\_MHz) in channels 0 to 49 (UNII-3)

Ptx <= max(TXMAX\_power\_Regulatory, -74-Pcca\_dBm\_MHz) in channels 50 to 249 (UNII-5)

For example, if Pcca\_dBm\_MHz = -75 dBm, then the transmitter can transmit at 8 dBm in UNII-3 and 1 dBm in UNII-5.

Given that no consensus was reached on LBT-based solution with a fixed EDT threshold and a duty-cycle limited no-LBT allowance, this new transmit power control proposal is a way to achieve coexistence with non-802.15.4ab technologies.

**Proposed Resolution: Accepted**