**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title |  | |
| Date Submitted | September 2024 | |
| Source | Carl Murray (Qorvo), | carl.murray at qorvo.com |
| Re: | CIDs 1114, 1115, 1116, 1334, 1170 | |
| Abstract |  | |
| Purpose | To propose resolution for “P802.15.4ab™/D01 Draft Standard for Low-Rate Wireless Networks”. | |
| Notice | This document does not represent the agreed views of the IEEE 802.15 Working Group or IEEE 802.15.8 Task Group. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |
|  |  | |

## CID 1114

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Name** | **Index#** | **Pg** | **Sub-Clause** | **Ln** | **Comment** | **Proposed Change** | **Disposition** |
| Billy Verso | 1114 | 56 | 10.38.2 | 1 | I think some of the parameters talked about here are potentially in the realms of the next higher layer protocol and perhaps not configured directly into the MAC. Maybe for this introductory statement a rewording could help make this more generic. | Change "is configured for UWB MMS ranging by specifying" to "is reused for UWB MMS ranging including the specification of" | Accepted |

**Overview of changed text in context**

The ranging block structure ~~is configured for UWB MMS ranging by specifying~~ is reused for UWB MMS ranging including the specification of the ranging slot duration, the ranging round duration, and the ranging block duration in RSTU. For UWB MMS ranging, the ranging slot, ranging round, and ranging block durations shall be integer multiples of 300 RSTUs.

## CID 1115

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Name** | **Index#** | **Pg** | **Sub-Clause** | **Ln** | **Comment** | **Proposed Change** | **Disposition** |
| Billy Verso | 1115 | 56 | 10.38.2 | 5 | This phrase "carrier coherence" is not clear to me in meaning or how transmission offset might influence it.. I have no problem with the specifying that offset shall be zero, but I think we should note why. | Add a definition of this term and a NOTE giving some explanation of this requirement. | Revised |

**Change the text on page 56 beginning on line 4 as indicated**

The round hopping, specified in 10.32.3.3 may be optionally applied to UWB MMS ranging. ~~To ease carrier coherence between UWB MMS phases,~~ To simplify scheduling when round hopping is used~~,~~ the transmission offset shall be zero.

## CID 1116

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Name** | **Index#** | **Pg** | **Sub-Clause** | **Ln** | **Comment** | **Proposed Change** | **Disposition** |
| Billy Verso | 1116 | 56 | 10.38.2 | 15 | A ranging round is typically the time from the start of ranging exchange between two devices to the start of their next exchange. In figure 25, "Ranging Round" should be changed to "UWB MMS ranging exchange" to match the text, although later in the text this may be called a "ranging sub-round", but I think that term is never actually defined. This would be a good place to define it, if we want to use it to cover what is in Figure 25. | Define "MMS ranging sub-round" here, and add the definition to clause 3.1. Review all usages of sub-round to ensure that they are consistent (use "MMS ranging sub-round") everywhere. Change figure 25 "Ranging Round" to "MMS Ranging Sub-round". | Rejected |

**Reason for Rejection**

There is significant reluctance to changing Ranging Round to Ranging sub-round in this section. The ranging round defined here is for one-to-one ranging. The ranging sub-round is used in one-to-many ranging and CID 1405 (doc 458-03) defines it in the one-to-many section to distinguish it from the one-to-one ranging round specified here.

## CID 1334

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Name** | **Index#** | **Pg** | **Sub-Clause** | **Ln** | **Comment** | **Proposed Change** | **Disposition** |
| B. Rolfe | 1334 | 56 | 10.38.2 | 14 | Marginally incorrect use of "may" suggesting something outside of this standard (if only just). | alternatively, another OOB mechanism will be used. | Revised |

**Change the text on page 56 beginning on line 12 as indicated**

In UWB driven UWB MMS, the HRP UWB PHY is employed for the control phase, the ranging phase and the report phase. UWB driven MMS may use the O-QPSK PHY described in clause 13 for initialization and setup, or ~~it may use~~ an OOB mechanism can be used for this.

## CID 1170

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Name** | **Index#** | **Pg** | **Sub-Clause** | **Ln** | **Comment** | **Proposed Change** | **Disposition** |
| Billy Verso | 1170 | 68 | 10.38.5 | 23 | Lines 23 through to Line 6 of the next page, are trying to explain the PHY packet in words, this should be clear from clause 16 and should not be repeated here. | Delete as much as possible from this clause, since it is already specified in clause 16 (which is where this PHY level stuff it should be specified). Clause 16 should reference/use the PIB phyUwbMmsRsfNumberFrags and phyUwbMmsRifNumberFrags configurations, so they don’t need to be mentioned here again. All it that is needed to say is that, responder fragments are offset by 600 RSTU, as shown in the figure. | Revised |

**Change the text in 16.2.11 on page 192, starting on line 15 as indicated**

Where X and Y are *phyUwbMmsRsfNumberFrags* and *phyUwbMmsRifNumberFrags* respectively ~~the number of RSF and RIF fragments respectively in the MMS UWB packet~~, the following are the combinations that should be supported by the HRP-ARDEV in the case of NBA UWB MMS operations:

⎯ RSF only MMS packets, i.e., where Y=0 and X ∈ {1, 2, 4, 8, 16}.

⎯ RIF only MMS packets, i.e., where X=0 and Y ∈ {1, 2, 4, 8}.

⎯ Mixed RSF/RIF packets, i.e., where X ∈ {1, 2, 4, 8}, Y ∈ {1, 2, 4, 8}.

**Change the text in 10.38.5 on page 68, starting on line 22 as indicated -**

The UWB MMS ranging phase follows the control phase.

~~In the ranging phase, the initiator shall transmit~~ *~~phyUwbMmsRsfNumberFrags~~* ~~RSF fragments starting its first fragment at the start of the ranging phase, with each subsequent RSF fragment starting 1200 RSTU from the start of the previous one.~~

~~The initiator may start transmitting a first RIF fragment at the start of the ranging phase if no RSF fragments are present, or two milliseconds (2400 RSTU) after the start of its last RSF fragment transmission otherwise. The initiator may continue to send~~ *~~phyUwbMmsRifNumberFrags~~* ~~RIF fragments at regular intervals of 1200 RSTU.~~

~~The responder may start transmitting a first RSF fragment at 600 RSTU into the ranging phase. The responder may send~~ *~~phyUwbMmsRsfNumberFrags~~* ~~RSF fragments at regular intervals of 1200 RSTU.~~

~~The responder may start transmitting a first RIF fragment at 600 RSTU into the ranging phase if no RSF fragments were transmitted, or two milliseconds (2400 RSTU) after the start of its last RSF fragment transmission otherwise. The responder may continue to send~~ *~~phyUwbMmsRifNumberFrags~~* ~~RIF fragments at regular intervals of 1200 RSTU.~~

In the ranging phase, the initiator shall transmit the HRP UWB PHY MMS packet (described in 16.2.11), and the responder may start transmitting its HRP UWB PHY MMS packet offset by 600 RSTU from the start into the ranging phase.