**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title | **Proposed Comments Resolution for 15.4ab D1.0 NB Channel Map Comments: Part 1** | |
| Date Submitted | November 2024 | |
| Sources | Pooria Pakrooh (Qualcomm) |  |
| Re: |  | |
| Abstract | Resolution to comments: | |
| Purpose | To propose comments resolution for “P802.15.4ab™/D (pre-ballot) C Draft Standard for Low-Rate Wireless Networks” | |
| Notice | This document does not represent the agreed views of the IEEE 802.15 Working Group or IEEE 802.15.4ab Task Group. It represents only the views of the participants listed in the “Sources” field above.It is offered as a basis for discussion and is not binding on the contributing individuals. The material in this document is subject to change in form and content after further study. The contributors reserve the right to add, amend or withdraw material contained herein. | |

***Comment Indices #53 and 239 in 15-24-0371-13-04ab-consolidated-comments\_draft\_1.0***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Sub-Clause** | **Page** | **Line** | **Comment** | **Proposed Change** |
| 53 | Mickael Maman | 10.38.9.3.9 | 84 | 6 | the lower limit of y is 50 for NB higher channel map | change 50<=y<=249 |
| 239 | Mickael Maman | 10.38.9.3.9 | 83 | 25 | 0<=y<=249, should be 50<=y<=249 | as in comment |

**Resolution: Accepted**

***Comment Indices #53 and 239 in 15-24-0371-13-04ab-consolidated-comments\_draft\_1.0***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Sub-Clause** | **Page** | **Line** | **Comment** | **Proposed Change** |
| 118 | Rojan Chitrakar | 10.38.9.5 | 94 | 5 | Add the other versions of the NB channel Map field. | Only the 6 octet version the NB channel Map field (10.38.9.3.7) is referenced. |
| 1365 | Pooria Pakrooh | 10.38.9.5 | 94 | 5 | Change to "per 10.38.9.3.7, 10.38.9.3.8 and 10.38.9.3.9" | Change to "per 10.38.9.3.7, 10.38.9.3.8 and 10.38.9.3.9" |

**Resolution: Accepted**

Instruction to the editor: Change the text as below:

The NB Channel Map field if present shall be set as per 10.38.9.3.7, 10.38.9.3.8 and 10.38.9.3.9.