**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **LB225/D03 comment resolution -- CID 115** |
| Date Submitted | Oct 13, 2025 |
| Sources | Alex Krebs (Apple)  krebs @ apple.com |
| Re: |  |
| Abstract |  |
| Purpose | To propose resolution for MMS related comments for “P802.15.4ab™/D03 Draft Standard for Low-Rate Wireless Networks”. |
| Notice | This document does not represent the agreed views of the IEEE 802.15 Working Group or IEEE 802.15.4ab Task Group. It represents only the views of the participants listed in the “Sources” field above.It is offered as a basis for discussion and is not binding on the contributing individuals. The material in this document is subject to change in form and content after further study. The contributors reserve the right to add, amend or withdraw material contained herein. |

**Table of contents**

[CID 115 (Accepted) 3](#_Toc211253752)

# CID 115 (Accepted)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Index #** | **Page** | **Sub-clause** | **Line #** | **Comment** | **Proposed Change** |
| 115 | 65 | 10.39.2 | 20 | The path to follow to figure out that 1.95Mb/s modulation is required to be used for the control/report packets for the UWB driven MMS UWB ranging is a little convoluted, i.e., this is buried in the specification of the mmsControlPhaseMode and mmsReportPhaseMode parameters (and Control Phase Config and Report Phase Config field values) where in table 21 values 14 or 15 apply to UWB driven, and these point onwards to the Table UWB modulation sets #1 and #2 from Table 86. We should make this easier to see, and also clarify that the 4z PHR is to be used. | At the end of the first sentence on p65 line 28, add: ", and shall use the UWB modulation specified by set #1 or set #2 from Table 86 with the PHR described 16.2.7.3”. |

Discussion: OK.

Proposed resolution: Accepted.

Disposition detail: n/a