|  |  |
| --- | --- |
| Project | **IEEE 802.16 Broadband Wireless Access Working Group <**<http://ieee802.org/16>**>** |
| Title | **Proposed Modifications to DC Link Creation for BS-Controlled DC in IEEE 802.16.1a** |
| Date Submitted | **2012-09-13** |
| Source(s) | Wooram Shin, Eunkyung Kim, Anseok Lee, Jaesun Cha, Kwanjae LimETRI | Voice: +82-42-860-6687E-mail: w.shin@etri.re.kr |
| Re: | In response to Sponsor Ballot sb010a on P802.16.1a/D5 |
| Abstract | This contribution proposes modification to link creation in IEEE 802.16.1a. |
| Purpose | To discuss and adopt the proposed texts in the IEEE 802.16.1a Draft Standard. |
| Notice | *This document does not represent the agreed views of the IEEE 802.16 Working Group or any of its subgroups*. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion. It is not binding on the contributor(s), who reserve(s) the right to add, amend or withdraw material contained herein. |
| Copyright Policy | The contributor is familiar with the IEEE-SA Copyright Policy <http://standards.ieee.org/IPR/copyrightpolicy.html>. |
| Patent Policy | The contributor is familiar with the IEEE-SA Patent Policy and Procedures:<<http://standards.ieee.org/guides/bylaws/sect6-7.html#6>> and <<http://standards.ieee.org/guides/opman/sect6.html#6.3>>.Further information is located at <<http://standards.ieee.org/board/pat/pat-material.html>> and <<http://standards.ieee.org/board/pat>>. |

Proposed Modifications to DC Link Creation for BS-Controlled DC in IEEE 802.16.1a

Wooram Shin, Eunkyung Kim, Anseok Lee, Jaesun Cha, Kwangjae Lim

ETRI

# Introduction

In the current draft standard [1], when DC link is created, HR-BS sends AAI-DC-LC-REQ messages to both source and destination HR-MSs, which include two TWDC addresses for transmitting and receiving as identification of DC link. If an HR-BS needs to request creation of multiple DC links with different HR-MSs to an HR-MS, then there is no way how to distinguish each link. Therefore, we suggest how to distinguish DC link when its creation is requested. Also, an HR-BS needs to send multiple AAI-DC-LC-REQ messages even though it wants to create multiple DC links for an HR-MS with different HR-MSs. It is not efficient, so support of multiple DC link creations is suggested. Similarly, in case of messaging AAI-DC-LC-RSP, it needs to support sending multiple responses on multiple DC link creation requests in an AAI-DC-LC-RSP message.

# References

[1] IEEE P802.16.1a/D5, WirelessMAN-Advanced Air Interface for Broadband Wireless Access Systems - Draft Amendment: Higher Reliability Networks, Aug. 2012.

# Proposed Texts on the IEEE 802.16.1a Amendment Draft Standard

The proposed texts are written in three different types of fonts according to each change purpose as follows.

The same texts in the current draft: black

The texts to be deleted by this contribution: ~~red strikeout~~

The texts to be added by this contribution: blue underline

[-----------------------------------------------------Start of Text Proposal------------------------------------------------------]

*[Remedy #1: Modify the current texts in Section 6.2.3.65.14 on Page 73 in the IEEE P802.16.1a/D5 Draft Standard as follows.]*

**6.2.3.65.14 AAI-DC-LC-REQ**

When HR-BS creates direct communication link between two HR-MSs. It shall send link creation message to both source and destination HR-MSs. Direct communication link creation can only be initiated by the HR-BS.

**Table 106o – AAI-DC-LC-REQ message field description**

|  |  |  |  |
| --- | --- | --- | --- |
| **Field** | **Size****(bits)** | **Value/Description** | **Condition** |
| For (*i*=0; *i*<N-DC-Link; *i*++) { |  | N-DC-Link is the number of DC links [1..4] |  |
| FID | 4 | Indicates which DC link needs to be created, which is corresponding to the flow of this FID | mandatory |
| Uplink/Downlink Indicator | 1 | Indicates which DC link needs to be created, which is corresponding to the flow of this link direction | mandatory |
| TWDC address for transmitting | 12 | Address assigned to DC link | mandatory |
| TWDC address for receiving | 12 | Address assigned for DC link | mandatory |
| } |  |  |  |

**FID and Uplink/Downlink Indicator**

* A pair of FID and Uplink/Downlink Indicator is used to indicate which DC link creation is requested, which is corresponding to the flow of the FID and Uplink/Downlink Indicator.

**TWDC address for transmitting**

* The TWDC address is used by the HR-MS for transmitting. The peer HR-MS of the DC-link shall receive on the resource scheduled with this TWDC address.

**TWDC address for receiving**

* The HR-MS shall receive on the resource assigned to this TWDC address since it is assigned to the peer HR-MS on the DC-Link for transmission.

*[Remedy #2: Modify the current texts in Section 6.2.3.65.15 on Page 73 in the IEEE P802.16.1a/D5 Draft Standard as follows.]*

**6.2.3.65.15 AAI-DC-LC-RSP**

The HR-MSs shall send back a response once they receive the direct communication link creation request.

**Table 106p – AAI-DC-LC-RSP message field description**

|  |  |  |  |
| --- | --- | --- | --- |
| **Field** | **Size****(bits)** | **Value/Description** | **Condition** |
| For (*i*=0; *i* <N-DC-Link; *i*++) { |  | N-DC-Link is the number of DC links [1..4] |  |
| TWDC address for transmitting | 12 |  | mandatory |
| Confirmation Code | 1 | 0b0: accept0b1: reject | mandatory |
| } |  |  |  |

Once the HR-BS receives responses from both HR-MSs, it can continue on other steps of direct communication setup.

[------------------------------------------------------End of Text Proposal------------------------------------------------------]