IEEE P802.19  
Wireless Coexistence

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed resolution to comment to clause 5.2.2.2 WSO subscription update procedure | | | | |
| Date: 2012-09-18 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Stanislav Filin | NICT |  |  | sfilin@nict.go.jp |
| Hiroshi Harada | NICT |  |  |  |

Abstract

This document is a submission to IEEE 802.19 TG1 proposing resolution to comment to clause 5.2.2.2 WSO subscription update procedure.

**Notice:** This document has been prepared to assist IEEE 802.19. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein.

# Comment

WSO subscription update procedure is not described, only figure is provided.

# Proposed resolution

*It is proposed to substitute the text in the clause 5.2.2.2 WSO subscription update procedure by the text below.*

* + - 1. WSO subscription update procedure

A CE shall perform the WSO subscription update procedure when it has received new WSO subscription information. An illustrative example of this procedure is shown in Figure 1. SubscriptionRequest and SubscriptionResponse messages are defined in clause 5.3 Messages.



Figure 1 WSO subscription update procedure

After a CE has received new WSO subscription information, the CE shall generate a SubscriptionRequest message and shall send this SubscriptionRequest message to the CM that serves this CE. CE operation related to generating and sending a SubscriptionRequest message is specified in clause 6 CE Operation.

After the CM has received the SubscriptionRequest message from the CE, the CM shall perform WSO subscription, shall generate a SubscriptionResponse message and shall send this SubscriptionResponse message to the CE. CM operation related to WSO subscription, generating and sending a SubscriptionResponse message is specified in clause 7 CM Operation.

After the CE has received the SubscriptionResponse message from the CM, the CE shall process the SubscriptionResponse message. CE operation related to processing the SubscriptionResponse message is specified in clause 6 CE Operation.