IEEE P802.19  
Wireless Coexistence

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed resolution to comment to clause 5.2.11.1 Sending reconfiguration request from Cm to CE procedure | | | | |
| Date: 2012-09-18 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Stanislav Filin | NICT |  |  | sfilin@nict.go.jp |
| Hiroshi Harada | NICT |  |  |  |

Abstract

This document is a submission to IEEE 802.19 TG1 proposing resolution to comment to clause 5.2.11.1 Sending reconfiguration request from CM to CE procedure.

**Notice:** This document has been prepared to assist IEEE 802.19. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein.

# Comment

Sending reconfiguration request from CM to CE procedure is not described, only figure is provided.

# Proposed resolution

*It is proposed to substitute the text in the clause 5.2.11.1 Sending reconfiguration request from CM to CE procedure by the text below.*

* + - 1. Sending reconfiguration request from CM to CE procedure

A CM shall perform the sending reconfiguration request from CM to CE procedure when it has generated new coexistence decision that requires reconfiguration of one or several WSOs subscribed to management service and served by this CM. An illustrative example of this procedure is shown in Figure 1. ReconfigurationRequest and ReconfigurationResponse messages are defined in clause 5.3 Messages.



Figure 1 Sending reconfiguration request from CM to CE procedure

After a CM has generated new coexistence decision that requires reconfiguration of one or several WSOs subscribed to management service and served by this CM, the CM shall generate one or several ReconfigurationRequest messages. The number of the ReconfigurationRequest messages is equal to the number of the WSOs that require reconfiguration. After the CM has generated the ReconfigurationRequest messages, the CM shall send these ReconfigurationRequest messages to the CE serving WSOs that require reconfiguration. CM operation related to generating and sending a ReconfigurationRequest message is specified in clause 7 CM Operation.

After a CE has received the ReconfigurationRequest message from the CM, the CE shall perform requested reconfiguration of the WSO it serves, shall generate a ReconfigurationResponse message, and shall send this ReconfigurationResponse message to the CM. CE operation related to performing WSO reconfiguration, generating and sending ReconfigurationResponse message is specified in clause 6 CE Operation.

After the CM has received the ReconfigurationResponse message from the CE, the CM shall process the ReconfigurationResponse message. CM operation related to processing the ReconfigurationResponse message is specified in clause 7 CM Operation.