Comment for Letter Ballot #4a Re-Circulation:

Author: Antonio de la Oliva

## The primitive MIH\_Radio\_Get\_Radios does not have parameters.

Please consider next definition of the primitive

## MIH\_Radio\_Get\_Radios

* 1. **MIH\_Radio\_Get\_Radios.request**
		1. **Function**

This primitive is used by an MIH User to get information regarding the number of interfaces and their technology from the MIHF.

* + 1. **Semantics of service primitive**

MIH\_Radio\_Get\_Radios.request(

 DestinationIdentifier

)

Parameters:

|  |  |  |
| --- | --- | --- |
| **Name** | **Data type** | **Description** |
| **DestinationIdentifier** | MIHF\_ID | This identifies a remote MIHF that will be the destination of this request. |
|  |  |  |

* + 1. **When generated**

This primitive is invoked by an MIH user when it wants to request information about the available interfaces in a remote or local node.

* + 1. **Effect of receipt**

If the destination of the request is the local MIHF itself, the local MIHF gets the requested information on the available interfaces and responds with a MIH\_Radio\_Get\_Radios.confirm. If the destination of the request is a remote MIHF, the local MIHF generates and sends a MIH\_Radio\_Get\_Radios Request message to the remote MIHF.