IEEE P802.21
Media Independent Handover Services

|  |
| --- |
| Group manager, command center, and mobile nodes |
| Date: 2013-11-xx |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Lily Chen | NIST | 100 Bureau Dr. Gaithersburg, MD 20878 | +1 (301) 975-6974 | Lily.Chen at nist.gov |

Abstract

This contribution clarifies the relation between group manager, command center, and mobile nodes to resolve comment #97.

# This contribution is based on the following issues.

# Currently, the command center is defined as a MIH user. However, in many places, it is considered as a PoS.

# It is also not clear the relation between the group manager and the command center.

# Furthermore, a command center can be a multicast recipient. But in a lot of places, only MNs

The following figure illustrates a general understanding.



We need to make decision on

1. Whether CC is a PoS or an MIH user in a PoS;
2. Do we consider the “group manipulation command” from MG and CCs the same as from a CC to MNs?

We also need to correct wherever MNs are considered as the only multicast recipients.