|  |  |
| --- | --- |
| Project | **IEEE 802.21d****<**[**http://www.ieee802.org/21/**](http://www.ieee802.org/21/)**>** |
| Title | **Remedy for Cmt#63 in LB7b** |
| DCN | 21-14-0062-00-MuGM |
| Date Submitted | **March, 20, 2014** |
| Source(s) | Subir Das (ACS) |  |
| Re: | IEEE 802.21 Session #61 in Beijing |
| Abstract | Remedy for LB#7b comment  |
| Purpose |  |
| Notice | This document has been prepared to assist the IEEE 802.21 Working Group. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor grants a free, irrevocable license to the IEEE to incorporate material contained in this contribution, and any modifications thereof, in the creation of an IEEE Standards publication; to copyright in the IEEE’s name any IEEE Standards publication even though it may include portions of this contribution; and at the IEEE’s sole discretion to permit others to reproduce in whole or in part the resulting IEEE Standards publication. The contributor also acknowledges and accepts that IEEE 802.21 may make this contribution public. |
| Patent Policy | The contributor is familiar with IEEE patent policy, as stated in [Section 6 of the IEEE-SA Standards Board bylaws](http://standards.ieee.org/guides/opman/sect6.html#6.3) <[http://standards.ieee.org/guides/bylaws/sect6-7.html#6](http://127.0.0.1:4664/cache?event_id=757737&schema_id=1&s=5X0vID10lu_E6yrIkWkNd4Wz2H8&q=hancock)> and in *Understanding Patent Issues During IEEE Standards Development* <http://standards.ieee.org/board/pat/faq.pdf> |

Remedy for Cmt#63 in LB7b.

Change the original text to following new text.

Original text:

p. 51, 9.4.1.1:

The device key assignment mechanism specified in this standard is based on a binary key structure, called a key tree. A key tree is a binary tree in depth d, where d is a system constant. A command center, at its initialization period, shall generate a group management tree whose depth is less than 256. The root of the key tree is called a level 0 node. At level k, there are 2k nodes, 0≤ k≤d. Each level k node can be represented as a k-bit string. The string is called the index of the node. For example, when d > 1, the level 2 nodes are represented by the indices 00, 01, 11, 10. Each node is assigned to a key, called a node key and identified by the Node Index. For example, the node keys assigned to level 2 nodes are denoted as k<00>, k<01>, k<10>, k<11>.

Suggested Change:

The device key assignment mechanism specified in this standard is based on a binary key structure, called a key tree. A key tree is a binary tree in depth d, where d is a system constant. A command center, at its initialization period, shall generate a group management tree whose depth is less than 256. The root of the key tree is called a level 0 node. A node is a logical entity of a binary tree in which leaf node represents a device. At level k, there are 2k nodes, 0≤ k≤d. Each level k node can be represented as a k-bit string. The string is called the index of the node. For example, when d > 1, the level 2 nodes are represented by the indices 00, 01, 11, 10. Each node is assigned to a key, called a node key and identified by the Node Index. For example, the node keys assigned to level 2 nodes are denoted as k<00>, k<01>, k<10>, k<11>.