|  |  |
| --- | --- |
| Project | **IEEE 802.21 MIHS****<**[**http://www.ieee802.org/21/**](http://www.ieee802.org/21/)**>** |
| Title | **Proposed remedy for SB Comment i-37 and i-15** |
| DCN | **21-14-0152-00-MuGM** |
| Date Submitted | **September 30, 2014** |
| Source(s) | Yoshihiro Ohba (Toshiba) |  |
| Re: | IEEE 802.21d Sponsor Ballot comment resolution |
| Abstract | This document describes a proposed remedy for SB comment i-37 and i-15 about signature. |
| Purpose | For Sponsor Ballot Comment Resolution |
| Notice | This document has been prepared to assist the IEEE 802.21 Working Group. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor grants a free, irrevocable license to the IEEE to incorporate material contained in this contribution, and any modifications thereof, in the creation of an IEEE Standards publication; to copyright in the IEEE’s name any IEEE Standards publication even though it may include portions of this contribution; and at the IEEE’s sole discretion to permit others to reproduce in whole or in part the resulting IEEE Standards publication. The contributor also acknowledges and accepts that IEEE 802.21 may make this contribution public. |
| Patent Policy | The contributor is familiar with IEEE patent policy, as stated in [Section 6 of the IEEE-SA Standards Board bylaws](http://standards.ieee.org/guides/opman/sect6.html#6.3) <[http://standards.ieee.org/guides/bylaws/sect6-7.html#6](http://127.0.0.1:4664/cache?event_id=757737&schema_id=1&s=5X0vID10lu_E6yrIkWkNd4Wz2H8&q=hancock)> and in *Understanding Patent Issues During IEEE Standards Development* <http://standards.ieee.org/board/pat/faq.pdf> |

# Comments

# Comment i-37 (p81, Annex F)

SIGNATURE TLV should contain sequence number at least when AES-CCM protection via Security TLV is not used.

* Comment i-15

Signature TLV should be optional when S-bit is 1 and Security TLV is used. One case is when a message is sent to a two-member group which is equivalent to pairwise SA, then Message Authentication is sufficient and digital signature is not needed.

# Proposed resolution

* Comment i-37

[1] Change SIGNATURE data type as SEQUENCE(CERT\_SERIAL\_NUMBER, CHOICE(SEQUENCE\_NUMBER, NULL), SIGNATURE\_DATA).

[2] Add the following sentence to Description: "SEQUENCE\_NUMBER" shall be contained when MIH PDU protected by digital signature only.

[3] Revise 9.6.3.1 and 9.6.3.2 so that sequence number in signature is taken into account of signature generation and verification (see below)

* Comment i-15

[1] In the last row, change "Present" to "May not be present" for Signature TLV.

[2] Change 9.6.2 to make Signature TLV optional (see below).

*New text for 9.6.3.1 and 9.6.3.2 addressing comments i-35 and i-37:*

**9.6.3.1 Multicast Message Signatures**

Multicast Messages are signed with the message source using a private key of the message source. Integrity and proof of origin of a multicast message is verified by verifying the message signature with the public key of a message source.

In case the MIH PDU is protected through GKB-generated MIH SA with a signature as specified in ~~Clause~~ 8.4.2.3, the MIHF of PoS generates a Signature TLV consisting of a SIGNATURE\_DATA and a

CERT\_SERIAL\_NUMBER. The SIGNATURE\_DATA is created by signing an MIH\_Group\_Manipulate command or a group addressed command using a signing key corresponding with a verification key specified by CERT\_SERIAL\_NUMBER.

In case the MIH PDU is not protected through a GKB-generated MIH SA and protected with a signature only as specified in 8.4.2.4, the MIHF of PoS generates a Signature TLV consisting of a SIGNATURE\_DATA, a CERT\_SERIAL\_NUMBER and a SEQUENCE\_NUMBER.

On receipt of signed multicast message there is an optional response indicating the validity of signature.

Message source requests credentials for key updates. Message source provides updates of credentials to destination devices (with overlap period).

The message content is signed using elliptical curve cryptography.

**9.6.3.2 Signature Verification**

The signature is verified using the message source signature verification key. The message source will identify which key is to be used for the multicast message so that verification will utilize the correct key for signature verification.

In case the MIH PDU received contains a Signature TLV and is protected through a GKB-generated MIH SA, then the MIHF of recipient retrieves CERT\_SERIAL\_NUMBER and SIGNATURE\_DATA from the Signature TLV. Then, the MIHF verifies the SIGNATURE\_DATA using a verification key specified by the CERT\_SERIAL\_NUMBER.

In the case the MIH PDU contains a Signature TLV and is not protected through a GKB-generated MIH SA, then the MIHF of recipient retrieves CERT\_SERIAL\_NUMBER, SIGNATURE\_DATA and SEQUENCE\_NUMBER from the Signature TLV. Then, the MIHF verifies the SIGNATURE\_DATA using a verification key specified by the CERT\_SERIAL\_NUMBER, and the SEQUENCE\_NUMBER. The received SEQUENCE\_NUMBER is considered valid if and only if the SEQUENCE\_NUMBER is greater than the last valid incoming sequence number maintained for the sender.