IEEE P802.22
Wireless RANs

|  |
| --- |
| [802.22b Network and Defintions] |
| Date: 2013-03-19 |
| Author(s): |
| Name | Company | Address | Phone | email |
| Changwoo Pyo | NICT | 3-4, Hikarino-oka, Yokosuka, 239-0847, Japan |  | cwpyo@nict.go.jp |
| Zhang Xin | NICT | 20 Science Park Road, #01-09A/10 TeleTech Park, Singapore |  | amy.xinzhang@ieee.org |
| Chunyi Song | NICT | 3-4 Hikarion-Oka, Yokosuka, Japan |  | songe@ieee.org |
| Keiichi Mizutani  | NICT | 3-4 Hikarion-Oka, Yokosuka, Japan |  | mizk@nict.go.jp |
| Pin-Hsun Lin | NICT | 3-4 Hikarion-Oka, Yokosuka, Japan |  | pslin@nict.go.jp |
| Gabriel Porto Villardi | NICT | 3-4 Hikarion-Oka, Yokosuka, Japan |  | gpvillardi@nict.go.jp |
| Masayuki Oodo | NICT | 3-4 Hikarion-Oka, Yokosuka, Japan |  | moodo@nict.go.jp |
| Ryuhei Funada | NICT | 3-4 Hikarion-Oka, Yokosuka, Japan |  | funada@nict.go.jp |
| Hiroshi Harada | NICT | 3-4 Hikarion-Oka, Yokosuka, Japan |  | harada@ieee.org |

Abstract

This document is a revision of initialization and network association (7.14) for 802.22b systems and provies definitions related with the revision.

**Notice:** This document has been prepared to assist IEEE 802.22. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein.

**Release:** The contributor grants a free, irrevocable license to the IEEE to incorporate material contained in this contribution, and any modifications thereof, in the creation of an IEEE Standards publication; to copyright in the IEEE’s name any IEEE Standards publication even though it may include portions of this contribution; and at the IEEE’s sole discretion to permit others to reproduce in whole or in part the resulting IEEE Standards publication. The contributor also acknowledges and accepts that this contribution may be made public by IEEE 802.22.

**Patent Policy and Procedures:** The contributor is familiar with the IEEE 802 Patent Policy and Procedures

<[**http://standards.ieee.org/guides/bylaws/sb-bylaws.pdf**](http://standards.ieee.org/guides/bylaws/sb-bylaws.pdf)>, including the statement "IEEE standards may include the known use of patent(s), including patent applications, provided the IEEE receives assurance from the patent holder or applicant with respect to patents essential for compliance with both mandatory and optional portions of the standard." Early disclosure to the Working Group of patent information that might be relevant to the standard is essential to reduce the possibility for delays in the development process and increase the likelihood that the draft publication will be approved for publication. Please notify the Chair Apurva Mody <apurva.mody@ieee.org> as early as possible, in written or electronic form, if patented technology (or technology under patent application) might be incorporated into a draft standard being developed within the IEEE 802.22 Working Group. **If you have questions, contact the IEEE Patent Committee Administrator at <****patcom@ieee.org****>**.

**3. Definitions**

**3.4 base station (BS):** Generalized equipment set providing connectivity, management and control of the customer premise equipment (CPE). The functionalities attributed to the BS, in the context of this standard, may be implemented by a device or a collection of devices.

**3.4a multihop relay base station (MR-BS):** Generalized equipment set providing connectivity, management and control of the relay customer premise equipments (R-CPEs) and subscriber CPEs (S-CPEs). *See also*: base station (BS), relay customer premise equipment (R-CPE). The functionalities attributed to the MR-BS, in the context of this standard, may be implemented by a device or a collection of devices.

**3.16 customer premise or portable equipment (CPE):**  A generalized equipment set providing connectivity between a BS and a subscriber premise.

**3.16a relay customer premise or portable equipment (R-CPE):** A generalized equipment set, dependent on a multihop relay base station (MR-BS) providing connectivity, to subscriber customer premise equipments (S-CPEs). An R-CPE may also provide management and control of subordinate S-CPEs. The air interface between an R-CPE and an S-CPE is identical to the air interface between a BS and a CPE.

**3.16a.1 centralized scheduling**: A mode of operation applicable to multihop relay where a multihop relay BS (MR-BS) determines the bandwidth allocations and generates the corresponding MAPs [or dictates the information used by relay CPEs (R-CPEs) to generate their MAPs] for all access and relay links in the WRAN cell.

**3.16a.2 distributed scheduling:** A mode of operation applicable to multihop relay where each R-CPE in the WRAN cell (with or without information from the MR-BS) determines the bandwidth allocations and generate the corresponding MAPs for the access link to/from its S-CPEs

**3.16a subscribe customer premise or portable equipment (S-CPE):** A generalized equipment set providing connectivity between a subscriber premise and an MR-BS or an R-CPE.

**3.x relay link (R-link):** A radio link between an MR-BS and an R-CPE. This can be a relay uplink or downlink.





**Figure 1a – An 802.22b WRAN cell with a multihop relay base station, relay CPEs and subscribe CPEs for 2- hop connections**