IEEE P802.22  
Wireless RANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed Resolution for CID 202, 203, 204, and 205 | | | | |
| Date: 2014-03-19 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Shigenobu　 Sasaki | Niigata University | 8050 Ikarashi 2-no-cho, Niigata, 950-2181 Japan | 81-25-262-6737 | shinsasaki@ieee.org |
| Bingxuan Zhao | Niigata University | 8050 Ikarashi 2-no-cho, Niigata, 950-2181 Japan | 81-25-262-5284 | bxzhao@ieee.org |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This document contains the proposed resolution for CID 202, 203, 204 and 205 in the LB1 for the draft standard of the IEEE 802.22b

**Notice:** This document has been prepared to assist IEEE 802.22. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein.

**Release:** The contributor grants a free, irrevocable license to the IEEE to incorporate material contained in this contribution, and any modifications thereof, in the creation of an IEEE Standards publication; to copyright in the IEEE’s name any IEEE Standards publication even though it may include portions of this contribution; and at the IEEE’s sole discretion to permit others to reproduce in whole or in part the resulting IEEE Standards publication. The contributor also acknowledges and accepts that this contribution may be made public by IEEE 802.22.

**Patent Policy and Procedures:** The contributor is familiar with the IEEE 802 Patent Policy and Procedures

<[**http://standards.ieee.org/guides/bylaws/sb-bylaws.pdf**](http://standards.ieee.org/guides/bylaws/sb-bylaws.pdf)>, including the statement "IEEE standards may include the known use of patent(s), including patent applications, provided the IEEE receives assurance from the patent holder or applicant with respect to patents essential for compliance with both mandatory and optional portions of the standard." Early disclosure to the Working Group of patent information that might be relevant to the standard is essential to reduce the possibility for delays in the development process and increase the likelihood that the draft publication will be approved for publication. Please notify the Chair Apurva Mody <[apurva.mody@ieee.org](mailto:apurva.mody@ieee.org)> as early as possible, in written or electronic form, if patented technology (or technology under patent application) might be incorporated into a draft standard being developed within the IEEE 802.22 Working Group. **If you have questions, contact the IEEE Patent Committee Administrator at <**[**patcom@ieee.org**](mailto:patcom@ieee.org)**>**.

1. Introduction

This contribution provides the proposed resolution for the following comments in LB1 for the IEEE Draft Std. 802.22b D1.0. An additional proposed change is also provided.

|  |  |  |  |
| --- | --- | --- | --- |
| **ID** | **Commenter Name** | **Comment** | **Suggested Remedy** |
| 202 | Shigenobu Sasaki | Table 209: Add the parameters related to MD-TCM, if necessary. | Add the parameters related to MD-TCM, if necessary. |
| 203 | Shigenobu Sasaki | Table 211: Add the parameters related to MD-TCM, if necessary. | Add the parameters related to MD-TCM, if necessary. |
| 204 | Shigenobu Sasaki | Table 226: Add the parameters related to MD-TCM, if necessary. | Add the parameters related to MD-TCM, if necessary. |
| 205 | Shigenobu Sasaki | Table 227: Add the parameters related to MD-TCM, if necessary. | Add the parameters related to MD-TCM, if necessary. |

1. Proposed resolution

*[Start of proposed change]*

***Change Table 209 as indicated.***

Table 209 — Concatenation index for different modulations and coding

|  |  |
| --- | --- |
| **Modulation and Rate** | **j** |
| QPSK 1/2 | 12 |
| QPSK 2/3 | 9 |
| QPSK 3/4 | 8 |
| QPSK 5/6 | 7 |
| 16-QAM 1/2 | 6 |
| 16-QAM 2/3 | 4 |
| 16-QAM 3/4 | 4 |
| 16-QAM 5/6 | 3 |
| 64-QAM 1/2 | 4 |
| 64-QAM 2/3 | 3 |
| 64-QAM 3/4 | 2 |
| 64-QAM 5/6 | 2 |
| 256-QAM 1/2 | 3 |
| 256-QAM 2/3 | 2 |
| 256-QAM 3/4 | 2 |
| 256-QAM 5/6 | 1 |
| 256-QAM 7/8 | 1 |
| 4D-TCM 48QAM | 2 |
| 4D-TCM 192QAM | 1 |

*[End of proposed change]*

*[Start of proposed change]*

***Change Table 211 as indicated.***

Table 211 — Useful data payload in bytes for an FEC block

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **QPSK** | | | | **16-QAM** | | | | **64-QAM** | | | | **256-QAM** | | | | |
| **R=**  **1/2** | **R=**  **2/3** | **R=**  **3/4** | **R=**  **5/6** | **R=**  **1/2** | **R=**  **2/3** | **R=**  **3/4** | **R=**  **5/6** | **R=**  **1/2** | **R=**  **2/3** | **R=**  **3/4** | **R=**  **5/6** | **R=**  **1/2** | **R=**  **2/3** | **R=**  **3/4** | **R=**  **5/6** | **R=**  **7/8** |
| 3 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 4 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  | 5 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 6 |  |  |  | 6 |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 8 |  |  |  | 8 |  |  |  |  |  |  |  |  |  |  |  |
| 9 |  | 9 |  |  |  | 9 |  | 9 |  |  |  |  |  |  |  |  |
|  |  |  | 10 |  |  |  | 10 |  |  |  |  |  |  |  |  |  |
| 12 | 12 |  |  | 12 |  |  |  |  | 12 |  |  | 12 |  |  |  |  |
| 15 |  |  | 15 |  |  |  |  |  |  |  | 15 |  |  |  |  |  |
|  | 16 |  |  |  | 16 |  |  |  |  |  |  |  | 16 |  |  |  |
| 18 |  | 18 |  | 18 |  | 18 |  | 18 |  |  |  |  |  | 18 |  |  |
|  | 20 |  | 20 |  |  |  | 20 |  |  |  |  |  |  |  | 20 |  |
| 21 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 21 |
| 24 | 24 |  |  | 24 | 24 |  |  |  | 24 |  |  | 24 |  |  |  |  |
|  |  |  | 25 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 27 |  | 27 |  |  |  | 27 |  | 27 |  | 27 |  |  |  |  |  |  |
|  | 28 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  |  | 30 | 30 |  |  | 30 |  |  |  | 30 |  |  |  |  |  |
|  | 32 |  |  |  | 32 |  |  |  |  |  |  |  | 32 |  |  |  |
| 33 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  | 35 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 36 | 36 | 36 |  | 36 |  | 36 |  | 36 | 36 |  |  | 36 |  | 36 |  |  |

*[End of proposed change.]*

*[Start of proposed changes.]*

***Change Table 226 and Table 227 as indicated.***

Table 226 — Number of coded bit per carrier and normalization factor  
for different modulation constellations

|  |  |  |
| --- | --- | --- |
| **Modulation Type** | **NCBPC** | **KMOD** |
| QPSK | 2 |  |
| 16-QAM | 4 |  |
| 64-QAM | 6 |  |
| 256-QAM | 8 |  |
| 4D-TCM 48QAM | 5.5 | TBD |
| 4D-TCM 48QAM | 7.5 | TBD |

Table 227 — Number of coded bits per OFDM slot (NCBPS) and corresponding number of  
data bits for different modulation constellation and coding rate combinations

|  |  |  |  |
| --- | --- | --- | --- |
| **Constellation type** | **Coding rate** | **NCBPS** | **Corresponding number of data bits** |
| QPSK | 1/2 | 48 | 24 |
| QPSK | 2/3 | 48 | 32 |
| QPSK | 3/4 | 48 | 36 |
| QPSK | 5/6 | 48 | 40 |
| 16-QAM | 1/2 | 96 | 48 |
| 16-QAM | 2/3 | 96 | 64 |
| 16-QAM | 3/4 | 96 | 72 |
| 16-QAM | 5/6 | 96 | 80 |
| 64-QAM | ½ | 144 | 72 |
| 64-QAM | 2/3 | 144 | 96 |
| 64-QAM | 3/4 | 144 | 108 |
| 64-QAM | 5/6 | 144 | 120 |
| 256-QAM | 1/2 | 192 | 96 |
| 256-QAM | 2/3 | 192 | 128 |
| 256-QAM | 3/4 | 192 | 144 |
| 256-QAM | 5/6 | 192 | 160 |
| 256-QAM | 7/8 | 192 | 168 |
| 4D-TCM 48QAM | 10/11 for 4D-symbol | 132 | 120 |
| 4D-TCM 48QAM | 14/15 for 4D-symbol | 180 | 168 |

*[End of proposed changes]*

1. Additional Changes

In addition to the proposed resolutions and changes in the previous section, the following changes in Table 228 is also proposed.

*[Start of proposed changes]*

***Change Table 228 as indicated.***

Table 228 — Normalized CNR per modulation for BER= 2\*10-4

|  |  |  |
| --- | --- | --- |
| **Modulation - FEC rate** | **Normalized CNR (dB)** | |
| **AWGN**  **(default)** | **Multipath Channel**8F**[[1]](#footnote-1)** *(informative)* |
| CDMA code | 1.2 | 5 |
| QPSK, rate: 1/2 | 4.3 | 8.1 |
| QPSK, rate: 2/3 | 6.1 | 11.6 |
| QPSK, rate: 3/4 | 7.1 | 14.0 |
| QPSK, rate: 5/6 | 8.1 | 17.8 |
| 16-QAM, rate: 1/2 | 10.2 | 14.8 |
| 16-QAM, rate: 2/3 | 12.4 | 20.3 |
| 16-QAM, rate: 3/4 | 13.5 | 24.6 |
| 16-QAM, rate: 5/6 | 14.8 | 28.6 |
| 64-QAM, rate: 1/2 | 15.6 | 20.5 |
| 64-QAM, rate: 2/3 | 18.3 | 26.2 |
| 64-QAM, rate: 3/4 | 19.7 | 31.8 |
| 64-QAM, rate: 5/6 | 20.9 | 40.4 |
| 256-QAM, rate: 1/2 | 19.4 | TBD |
| 256-QAM, rate: 2/3 | 22.6 | TBD |
| 256-QAM, rate: 3/4 | 24.2 | TBD |
| 256-QAM, rate: 5/6 | 26.2 | TBD |
| 256-QAM, rate: 7/8 | 27.5 | TBD |
| 4D-TCM 48QAM | 15.5 | TBD |
| 4D-TCM 192 QAM | 22.5 | TBD |

*[End of proposed change]*

1. References

1. The multipath channel used for the calculations is defined on 6 paths as follows: excess delay: -3, 0, 2, 4, 7 and 11 μsec; relative amplitude: -6, 0, -7, -22, -16 and -20 dB; the phase for each path is random. The delay, amplitude and phase are assumed to be constant over the period of one symbol. [↑](#footnote-ref-1)