IEEE P802.22  
Wireless RANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A-WRAN Descriptions | | | | |
| Date: 2014-07-17 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| cwpyo | NICT |  |  | [cwpyo@nict.go.jp](mailto:cwpyo@nict.go.jp) |
|  |  |  |  |  |

Abstract

Add descriptions for the advanced-WRAN on the Section 1.3 on the draft

**Notice:** This document has been prepared to assist IEEE 802.22. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein.

**Release:** The contributor grants a free, irrevocable license to the IEEE to incorporate material contained in this contribution, and any modifications thereof, in the creation of an IEEE Standards publication; to copyright in the IEEE’s name any IEEE Standards publication even though it may include portions of this contribution; and at the IEEE’s sole discretion to permit others to reproduce in whole or in part the resulting IEEE Standards publication. The contributor also acknowledges and accepts that this contribution may be made public by IEEE 802.22.

**Patent Policy and Procedures:** The contributor is familiar with the IEEE 802 Patent Policy and Procedures

<[**http://standards.ieee.org/guides/bylaws/sb-bylaws.pdf**](http://standards.ieee.org/guides/bylaws/sb-bylaws.pdf)>, including the statement "IEEE standards may include the known use of patent(s), including patent applications, provided the IEEE receives assurance from the patent holder or applicant with respect to patents essential for compliance with both mandatory and optional portions of the standard." Early disclosure to the Working Group of patent information that might be relevant to the standard is essential to reduce the possibility for delays in the development process and increase the likelihood that the draft publication will be approved for publication. Please notify the Chair Apurva Mody <[apurva.mody@ieee.org](mailto:apurva.mody@ieee.org)> as early as possible, in written or electronic form, if patented technology (or technology under patent application) might be incorporated into a draft standard being developed within the IEEE 802.22 Working Group. **If you have questions, contact the IEEE Patent Committee Administrator at <**[**patcom@ieee.org**](mailto:patcom@ieee.org)**>**.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 20 | 3 |  | T | Additional definitions on Advanced BS (A-BS) and Advenced CPE (A-CPE) are necessary. It is also necessary to clarify the diffrence of these A-BS and A-CPE from conventional BS and CPE defiend in the IEEE 802.22-2011 main standard. | Add additional definitions on Advanced BS (A-BS) and Advenced CPE (A-CPE) . Clarification of the diffrence of these A-BS and A-CPE from conventional BS and CPE defiend in the IEEE 802.22-2011 main standard should be described. Creating additional table to show the comparison of A-BS, A-CPE and conventional BS and CPE looks desirable. |

* 1. Reference Application

The Wireless Regional Area Networks (WRANs) for which this standard has been developed are expected to operate primarily in low population density areas in order to provide broadband access to data networks. The WRAN systems will use vacant channels in the VHF and UHF bands allocated to the Television Broadcasting Service in the frequency range between 54 MHz and 862 MHz while avoiding interference to the broadcast incumbents in these bands. A typical application can be the coverage of the rural area around a village, as illustrated in Figure 1, within a radius of 10 km to 30 km from the base station depending on its EIRP and antenna height. The MAC can also accommodate user terminals located as far as 100 km with proper scheduling of the traffic in the frame when exceptional RF signal propagation conditions are present. With the PHY implemented in this standard, WRAN systems can cover up to a radius of 30 km without special scheduling.



A base station (BS) complying with this standard shall be able to provide high-speed Internet service for up to 512 fixed or portable customer premise equipment (CPE) devices or groups of devices within its coverage area assuming different quality of service (QoS) requirements for various CPEs, while meeting the regulatory requirements for protection of the incumbents.

The standard includes cognitive radio techniques to mitigate interference to incumbents, including geolocation capability, provision to access a database of incumbent services, and spectrum-sensing technology to detect the presence of incumbent services, other WRAN systems, and IEEE 802.22.1 wireless beacons.

The Advanced Wireless Regional Area Networks (A-WRANs) for which this standard has been developed are expected to support enhanced broadband services and monitoring applications such as real-time and/or near real-time monitoring, emergency broadband services, remote medical services, etc. The A-WRAN provides all essential functionalities of PHY, MAC, security, and cognitive radio technologies defined in the IEEE 802.22 WRAN and supports an additional PHY mode and additional functionalities of multihop relay operations, multiple channel operations, multiple input multiple output (MIMO) operations, and advanced security to extend regional area broadband services to the regional monitoring applications and the enhanced broadband services.

Figure A illustrates an A-WRAN. An advanced base station (A-BS) complying with this standard shall be able to provide broadband services for the customer premise equipments (CPEs) such as an advanced CPE (A-CPE) and a subscriber CPE (S-CPE) through direct or multihop relay connectivity. An advanced customer premise equipment (A-CPE) enables to provide multihop relay connectivity for the S-CPEs, which enables to enhance connection reliability between the A-BS and S-CPEs, reduce the network management overhead of the A-BS as well as could extend the service coverage of A-WRAN.

Figure A – An A-WRAN with an A-BS, A-CPEs and S-CPEs